
-------
Username: alfatome
Password: C85ccQm+Tk
--
-------------

 IN (\d{3})\
Default keybindings:
Action
Key combination
History
Ctrl + Alt + h
Actions
Ctrl + Alt + a
Menu
Ctrl + Alt + p
Search
Ctrl + Alt + f
Offline mode
Ctrl + Alt + o
20191204             10:14:08 GitHub - CristianHenzel/ClipIt: ClipIt clipboard manager for GTK+ https://github.com/CristianHenzel/ClipIt
Default keybindings:
Action 	Key combination
History 	Ctrl + Alt + h
Actions 	Ctrl + Alt + a
Menu 	Ctrl + Alt + p
Search 	Ctrl + Alt + f
Offline mode 	Ctrl + Alt + o
clipit
ClipIt
       -?, --help
             Show help options.
-d, --daemon
             Run as daemon. Use this mode if you just want ClipIt to  keep  your  clipboard  and
             primary contents safe.
20191204             10:23:42 Ubuntu Manpage: ClipIt - Lightweight GTK+ Clipboard Manager http://manpages.ubuntu.com/manpages/bionic/man1/clipit.1.html
       -d, --daemon
             Run as daemon. Use this mode if you just want ClipIt to  keep  your  clipboard  and
             primary contents safe.
       -c, --clipboard
             Print clipboard contents.
-p, --primary
             Print primary contents.
20191204             10:24:05 Ubuntu Manpage: ClipIt - Lightweight GTK+ Clipboard Manager http://manpages.ubuntu.com/manpages/bionic/man1/clipit.1.html
       -p, --primary
             Print primary contents.
ACTIONS
       ClipIt's  actions  perform  commands  using  the  contents  of your clipboard. "%s" in the
       command is replaced with the clipboard contents.
20191204             10:24:30 Ubuntu Manpage: ClipIt - Lightweight GTK+ Clipboard Manager http://manpages.ubuntu.com/manpages/bionic/man1/clipit.1.html
   ACTIONS
       ClipIt's  actions  perform  commands  using  the  contents  of your clipboard. "%s" in the
       command is replaced with the clipboard contents.
   CLI EXAMPLES
       Put text in the clipboard
             echo "copied to clipboard" | clipit
             clipit "copied to clipboard"
       Put text in the clipboard and print the clipboard contents
             echo "copied to clipboard" | clipit -c
THE—FEW default keybindings are:

    History Ctrl+Alt+h
    Actions Ctrl+Alt+a
    Menu Ctrl+Alt+p
    Search Ctrl+Alt+f
    Offline mode Ctrl+Alt+o

http://transit.iut2.upmf-grenoble.fr/cgi-bin/man/man2html
You can enter a program name, possibly preceded by the section, the directories to search (with -M) or a full name. For example:

    find
    1 find
    -M /usr/share/man:/opt/man:/usr/local/share/man find
    /usr/share/man/man1/gperf.1 
The Manual Page text search interface was created for Linux
http://transit.iut2.upmf-grenoble.fr/cgi-bin/man/mansearch
http://transit.iut2.upmf-grenoble.fr/cgi-bin/man/man2html?query=search%2B%2B+1
cgi-bin/man/manwhatis?1
http://transit.iut2.upmf-grenoble.fr/
Apache2 Debian Default Page
20191204             10:55:32 Apache2 Debian Default Page: It works http://transit.iut2.upmf-grenoble.fr/
Ubuntu Manpage: Directory Listing
20191204             11:03:14 ClipIt manpage - Ecosia https://www.ecosia.org/search?tt=mzl&q=ClipIt+manpage
trusty
14.04 LTS	xenial
16.04 LTS	bionic
18.04 LTS	disco
19.04	eoan
19.10	Section Description
print(1)	print(1)	print(1)	print(1)	print(1)	(1) - Executable programs or shell commands
.	.	.	.	.	(2) - System calls (functions provided by the kernel)
print(3)	print(3)	print(3)	print(3)	print(3)	(3) - Library calls (functions within program libraries)

http://manpages.ubuntu.com/cgi-bin/search.py?q=print&cx=003883529982892832976%3A5zl6o8w6f0s&cof=FORID%3A9&ie=UTF-8
trusty14.04 LTSxenial16.04 LTSbionic18.04 LTSdisco19.04eoan19.10Section Descriptionprint(1)print(1)print(1)print(1)print(1)(1) - Executable programs or shell commands.....(2) - System calls (functions provided by the kernel)print(3)print(3)print(3)print(3)print(3)(3) - Library calls (functions within program libraries)
20191204             11:05:19 Ubuntu Manpage: Searching http://manpages.ubuntu.com/cgi-bin/search.py?q=print&cx=003883529982892832976%3A5zl6o8w6f0s&cof=FORID%3A9&ie=UTF-8
http://manpages.ubuntu.com/manpages/trusty/en/man1/print.1.html
print(3)
20191204             11:07:23 Ubuntu Manpage: Searching http://manpages.ubuntu.com/cgi-bin/search.py?q=print&cx=003883529982892832976%3A5zl6o8w6f0s&cof=FORID%3A9&ie=UTF-8
http://manpages.ubuntu.com/manpages/trusty/en/man3/print.3ncurses.html

------------------
mtp://%5Busb%3A002,010%5D/Internal%20shared%20storage/Download/SetupFreeDataCapture.exe
How to Install Shlwapi.dll? How to Fix Shlwapi.dll Errors?
20191129004307       Download Shlwapi.dll for Windows 10, 8.1, 8, 7, Vista and XP - 32 Bit and 64 Bit http://www.dlldownloader.com/shlwapi-dll/
http://www.dlldownloader.com/shlwapi-dll
http://www.dlldownloader.com/shlwapi-dl
shlwapi.dll
0.43 MB Download for 64 Bit (x64)  
20191129004124       Download Shlwapi.dll for Windows 10, 8.1, 8, 7, Vista and XP - 32 Bit and 64 Bit http://www.dlldownloader.com/shlwapi-dll/
Download Shlwapi.dll for Windows 10, 8.1, 8, 7, Vista and ...
20191129004116       download shlwapi.dll for wine - Ecosia https://www.ecosia.org/search?q=download+shlwapi.dll+for+wine
how to install 
how to instal
Wine cannot load dlls that already exist - WineHQ Forums
20191129003850       how to install shlwapi.dll for wine - Ecosia https://www.ecosia.org/search?q=how+to+install+shlwapi.dll+for+wine
Wine API: shlwapi.dll
20191129003702       shlwapi.dll for wine - Ecosia https://www.ecosia.org/search?tt=mzl&q=shlwapi.dll+for+wine
Ich
notepad++6.2.4.exe
notepad++
/home/me/.wine/drive_c/Program Files/Notepad++new/notepad++.exe
home/me/Downloads
npp.7.6.2.Installer.x64.exe
npp.7.6.2.Installer.x64
Installer
20191129001521       Notepad++ 7.6.2 Gilet Jaune Edition | Notepad++ https://notepad-plus-plus.org/downloads/v7.6.2/
Installer
20191129001337       Notepad++ 7.6.2 Gilet Jaune Edition | Notepad++ https://notepad-plus-plus.org/downloads/v7.6.2/
Notepad++ 7.6.2 Gilet Jaune Edition
20191129001307       Downloads | Notepad++ https://notepad-plus-plus.org/downloads/
wine --version
20191129001133       How To Install Wine On Ubuntu 18.04 LTS | Itsubuntu.com https://itsubuntu.com/how-to-install-wine-on-ubuntu-18-04-lts/
sudo apt install wine64
lscpu
https://notepad-plus-plus.org/downloads/v7.7/
Installer
20191129000458       Notepad++ 7.7 release | Notepad++ https://notepad-plus-plus.org/downloads/v7.7/
Notepad++ 7.7 release
20191129000313       Downloads | Notepad++ https://notepad-plus-plus.org/downloads/
Download
Notepad++ 7.6.6 release
20191129000003       Downloads | Notepad++ https://notepad-plus-plus.org/downloads/
npp.7.6.6.Installer.exe
npp.7.6.6.Installer
Download
20191128234926       Download Notepad++ (32-bit) 7.6.6 for Windows - Filehippo.com https://filehippo.com/download_notepad_32/7.6.6.0.0/
Greenshot-INSTALLER-1.2.10.6-RELEASE
npp.7.6.4.Installer
Download
20191128234741       Download Notepad++ (32-bit) 7.6.6 for Windows - Filehippo.com https://filehippo.com/download_notepad_32/7.6.6.0.0/
Download
20191128234707       Download Notepad++ (32-bit) 7.6.4 for Windows - Filehippo.com https://filehippo.com/download_notepad_32/7.6.4.0.0/
npp.7.6.4.Installer.exe
Download
20191128234029       Download Notepad++ (32-bit) 7.6.4 for Windows - Filehippo.com https://filehippo.com/download_notepad_32/7.6.4.0.0/
https://askubuntu.com/questions/1087032/notepad-plus-plus-snap-does-not-start-on-ubuntu
sudo snap connect notepad-plus-plus:process-control
notepad-plus-plus snap does not start on Ubuntu
20191128233337       18.04 - Unable to use or open Notepad++ after installation - Ask Ubuntu https://askubuntu.com/questions/1094439/unable-to-use-or-open-notepad-after-installation/1094771
snap install wine-platform-3-stable
snap run notepad-plus-plus
snap install wine-platform-runtime
snap connect notepad-plus-plus:wine-runtime wine-platform-runtime

snap run notepad-plus-plus
20191128232528       18.04 - Unable to use or open Notepad++ after installation - Ask Ubuntu https://askubuntu.com/questions/1094439/unable-to-use-or-open-notepad-after-installation/1094771
sudo snap install notepad-plus-plus
snap install wine-platform
snap disconnect notepad-plus-plus:wine-platform-plug
sudo snap install notepad-plus-plus 
18.04 - Unable to use or open Notepad++ after installation ...
20191128232246       notepad ++ won't start after updating wine - Ecosia https://www.ecosia.org/search?q=notepad+%2B%2B+won%27t+start+after+updating+wine
Notepad++
chmod a+x $HOME/bin/run_linux_program
20191128230040       FAQ - WineHQ Wiki https://wiki.winehq.org/FAQ
Frequently Asked Questions
20191128225837       WineHQ Wiki https://wiki.winehq.org/Main_Page
Main page
20191128225832       Ubuntu - WineHQ Wiki https://wiki.winehq.org/Ubuntu
winecfg
/opt/wine-stable/bin/winecfg
hoptome/me
home/me
sudo apt install --install-recommends winehq-stable
> 20191128224636       Ubuntu - WineHQ Wiki https://wiki.winehq.org/Ubuntu

sudo apt-add-repository 'deb https://dl.winehq.org/wine-builds/ubuntu/
20191128224636       Ubuntu - WineHQ Wiki https://wiki.winehq.org/Ubuntu
sudo apt-add-repository 'deb https://dl.winehq.org/wine-builds/ubuntu/
20191128224527       Ubuntu - WineHQ Wiki https://wiki.winehq.org/Ubuntu
sudo
20191128224519       Ubuntu - WineHQ Wiki https://wiki.winehq.org/Ubuntu
sudo apt-key add winehq.key
20191128224420       Ubuntu - WineHQ Wiki https://wiki.winehq.org/Ubuntu
wget -nc https://dl.winehq.org/wine-builds/winehq.key
sudo dpkg --add-architecture i386 
sudo apt-key add winehq.k
20191128224313       Ubuntu - WineHQ Wiki https://wiki.winehq.org/Ubuntu
sudo dpkg --add-architecture i386
20191128224246       Ubuntu - WineHQ Wiki https://wiki.winehq.org/Ubuntu
sudo apt-add-repository 'deb https://dl.winehq.org/wine-builds/ubuntu/
20191128223630       Ubuntu - WineHQ Wiki https://wiki.winehq.org/Ubuntu
Ubuntu
20191128223615       Download - WineHQ Wiki https://wiki.winehq.org/Download
https://wiki.winehq.org/Git_Wine_Tutorial#Downloading_and_installing_Git
Wine 4.0.3
20191128223414       WineHQ - Run Windows applications on Linux, BSD, Solaris and macOS https://www.winehq.org/
English
20191128223401       WineHQ - WineHQ - Wählen Sie Ihre Sprache https://www.winehq.org/lang
Sprache ändern
20191128223358       WineHQ - Windows-Anwendungen unter Linux, BSD, Solaris und macOS ausführen https://www.winehq.org/
apt show wine
wine --version
WINE
---
affix morphemes
-----------------
20191114             https://www.ecosia.org/search?tt=mzl&q=ubuntu+kernel+modules

20191114             usb+video+grabber

20191114             https://www.ecosia.org/search?tt=mzl&q=ubuntu+kernel+modules+usb%2Bvideo%2Bgrabber
20191114             https://help.ubuntu.com/community/Loadable_Modules
20191114             modules

20191114             cx231xx,cx25840

20191114             SilverCrest USB 2.0 Video Grabber SVG 2.0 A2 - LinuxTVWiki
20191114             https://www.linuxtv.org/wiki/index.php/SilverCrest_USB_2.0_Video_Grabber_SVG_2.0_A2
20191114             Overview/Features. Features of the SilverCrest USB-Video-Grabber SVG 2.0 A2: Digitalization of analogue video signals as VHS, Video8, Hi8 etc. Connects devices e.g. Camcorder, Video-Recorder and other analogue Video sources with Notebook or Personal Computer.

20191114             https://www.linuxtv.org/wiki/index.php/SilverCrest_USB_2.0_Video_Grabber_SVG_2.0_A2

20191114             lsusb -v  -d 1d19:6109

20191114             drivers/media/video/cx231xx/cx231xx-cards.c

20191114             drivers/media/usb/cx231xx/cx231xx-cards.c

20191114             drivers/media/video/

20191114             usb_device_id

20191114             https://www.linuxtv.org/wiki/index.php/SilverCrest_USB_2.0_Video_Grabber_SVG_2.0_A2

20191114             drivers/media

20191114             media/usb

20191114             drivers/media/usb

20191114             drivers/media/video

20191114             _id_table

20191114             > dmesg

20191114             ID 1d19:6109
https://www.ecosia.org/search?tt=mzl&q=cx231xx%2Ccx25840
20191114             Dexatek Technology Ltd.
Bus 002 Device 011: ID 1d19:6109 Dexatek Technology Ltd. 
Couldn't open device, some information will be missing
Device Descriptor:
  bLength             18
  bDescriptorType         1
  bcdUSB             2.00
  bDeviceClass          239 Miscellaneous Device
  bDeviceSubClass         2 ?
  bDeviceProtocol         1 Interface Association
  bMaxPacketSize0        64
  idVendor           0x1d19 Dexatek Technology Ltd.
  idProduct          0x6109 
  bcdDevice           40.02
  iManufacturer           1 
  iProduct             2 
  iSerial             3 
  bNumConfigurations      1
  Configuration Descriptor:
    bLength             9
    bDescriptorType         2
    wTotalLength          248
    bNumInterfaces          6
    bConfigurationValue     1
    iConfiguration          4 
    bmAttributes         0x80
      (Bus Powered)
    MaxPower             500mA
    Interface Descriptor:
      bLength             9
      bDescriptorType         4
      bInterfaceNumber        0
      bAlternateSetting       0
      bNumEndpoints           2
      bInterfaceClass       255 Vendor Specific Class
      bInterfaceSubClass    255 Vendor Specific Subclass
      bInterfaceProtocol    255 Vendor Specific Protocol
      iInterface             32 
      Endpoint Descriptor:
        bLength             7
        bDescriptorType         5
        bEndpointAddress     0x8e  EP 14 IN
        bmAttributes            3
          Transfer Type            Interrupt
          Synch Type             None
          Usage Type             Data
        wMaxPacketSize     0x0020  1x 32 bytes
        bInterval             4
      Endpoint Descriptor:
        bLength             7
        bDescriptorType         5
        bEndpointAddress     0x0e  EP 14 OUT
        bmAttributes            3
          Transfer Type            Interrupt
          Synch Type             None
          Usage Type             Data
        wMaxPacketSize     0x0020  1x 32 bytes
        bInterval             4
    Interface Association:
      bLength             8
      bDescriptorType        11
      bFirstInterface         1
      bInterfaceCount         5
      bFunctionClass        255 Vendor Specific Class
      bFunctionSubClass     255 Vendor Specific Subclass
      bFunctionProtocol     255 Vendor Specific Protocol
      iFunction             0 
    Interface Descriptor:
      bLength             9
      bDescriptorType         4
      bInterfaceNumber        1
      bAlternateSetting       0
      bNumEndpoints           1
      bInterfaceClass       255 Vendor Specific Class
      bInterfaceSubClass    255 Vendor Specific Subclass
      bInterfaceProtocol    255 Vendor Specific Protocol
      iInterface             7 
      Endpoint Descriptor:
        bLength             7
        bDescriptorType         5
        bEndpointAddress     0x8f  EP 15 IN
        bmAttributes            3
          Transfer Type            Interrupt
          Synch Type             None
          Usage Type             Data
        wMaxPacketSize     0x0008  1x 8 bytes
        bInterval             7
    Interface Descriptor:
      bLength             9
      bDescriptorType         4
      bInterfaceNumber        2
      bAlternateSetting       0
      bNumEndpoints           1
      bInterfaceClass       255 Vendor Specific Class
      bInterfaceSubClass    255 Vendor Specific Subclass
      bInterfaceProtocol    255 Vendor Specific Protocol
      iInterface             20 
      Endpoint Descriptor:
        bLength             7
        bDescriptorType         5
        bEndpointAddress     0x83  EP 3 IN
        bmAttributes            2
          Transfer Type            Bulk
          Synch Type             None
          Usage Type             Data
        wMaxPacketSize     0x0200  1x 512 bytes
        bInterval             0
    Interface Descriptor:
      bLength             9
      bDescriptorType         4
      bInterfaceNumber        2
      bAlternateSetting       1
      bNumEndpoints           1
      bInterfaceClass       255 Vendor Specific Class
      bInterfaceSubClass    255 Vendor Specific Subclass
      bInterfaceProtocol    255 Vendor Specific Protocol
      iInterface             21 
      Endpoint Descriptor:
        bLength             7
        bDescriptorType         5
        bEndpointAddress     0x83  EP 3 IN
        bmAttributes            5
          Transfer Type            Isochronous
          Synch Type             Asynchronous
          Usage Type             Data
        wMaxPacketSize     0x001c  1x 28 bytes
        bInterval             1
    Interface Descriptor:
      bLength             9
      bDescriptorType         4
      bInterfaceNumber        2
      bAlternateSetting       2
      bNumEndpoints           1
      bInterfaceClass       255 Vendor Specific Class
      bInterfaceSubClass    255 Vendor Specific Subclass
      bInterfaceProtocol    255 Vendor Specific Protocol
      iInterface             22 
      Endpoint Descriptor:
        bLength             7
        bDescriptorType         5
        bEndpointAddress     0x83  EP 3 IN
        bmAttributes            5
          Transfer Type            Isochronous
          Synch Type             Asynchronous
          Usage Type             Data
        wMaxPacketSize     0x0034  1x 52 bytes
        bInterval             1
    Interface Descriptor:
      bLength             9
      bDescriptorType         4
      bInterfaceNumber        3
      bAlternateSetting       0
      bNumEndpoints           1
      bInterfaceClass       255 Vendor Specific Class
      bInterfaceSubClass    255 Vendor Specific Subclass
      bInterfaceProtocol    255 Vendor Specific Protocol
      iInterface             23 
      Endpoint Descriptor:
        bLength             7
        bDescriptorType         5
        bEndpointAddress     0x84  EP 4 IN
        bmAttributes            2
          Transfer Type            Bulk
          Synch Type             None
          Usage Type             Data
        wMaxPacketSize     0x0200  1x 512 bytes
        bInterval             0
    Interface Descriptor:
      bLength             9
      bDescriptorType         4
      bInterfaceNumber        3
      bAlternateSetting       1
      bNumEndpoints           1
      bInterfaceClass       255 Vendor Specific Class
      bInterfaceSubClass    255 Vendor Specific Subclass
      bInterfaceProtocol    255 Vendor Specific Protocol
      iInterface             24 
      Endpoint Descriptor:
        bLength             7
        bDescriptorType         5
        bEndpointAddress     0x84  EP 4 IN
        bmAttributes            5
          Transfer Type            Isochronous
          Synch Type             Asynchronous
          Usage Type             Data
        wMaxPacketSize     0x00b8  1x 184 bytes
        bInterval             1
    Interface Descriptor:
      bLength             9
      bDescriptorType         4
      bInterfaceNumber        3
      bAlternateSetting       2
      bNumEndpoints           1
      bInterfaceClass       255 Vendor Specific Class
      bInterfaceSubClass    255 Vendor Specific Subclass
      bInterfaceProtocol    255 Vendor Specific Protocol
      iInterface             25 
      Endpoint Descriptor:
        bLength             7
        bDescriptorType         5
        bEndpointAddress     0x84  EP 4 IN
        bmAttributes            5
          Transfer Type            Isochronous
          Synch Type             Asynchronous
          Usage Type             Data
        wMaxPacketSize     0x02d8  1x 728 bytes
        bInterval             1
    Interface Descriptor:
      bLength             9
      bDescriptorType         4
      bInterfaceNumber        3
      bAlternateSetting       3
      bNumEndpoints           1
      bInterfaceClass       255 Vendor Specific Class
      bInterfaceSubClass    255 Vendor Specific Subclass
      bInterfaceProtocol    255 Vendor Specific Protocol
      iInterface             26 
      Endpoint Descriptor:
        bLength             7
        bDescriptorType         5
        bEndpointAddress     0x84  EP 4 IN
        bmAttributes            5
          Transfer Type            Isochronous
          Synch Type             Asynchronous
          Usage Type             Data
        wMaxPacketSize     0x13c4  3x 964 bytes
        bInterval             1
    Interface Descriptor:
      bLength             9
      bDescriptorType         4
      bInterfaceNumber        3
      bAlternateSetting       4
      bNumEndpoints           1
      bInterfaceClass       255 Vendor Specific Class
      bInterfaceSubClass    255 Vendor Specific Subclass
      bInterfaceProtocol    255 Vendor Specific Protocol
      iInterface             27 
      Endpoint Descriptor:
        bLength             7
        bDescriptorType         5
        bEndpointAddress     0x84  EP 4 IN
        bmAttributes            5
          Transfer Type            Isochronous
          Synch Type             Asynchronous
          Usage Type             Data
        wMaxPacketSize     0x0b84  2x 900 bytes
        bInterval             1
    Interface Descriptor:
      bLength             9
      bDescriptorType         4
      bInterfaceNumber        4
      bAlternateSetting       0
      bNumEndpoints           1
      bInterfaceClass       255 Vendor Specific Class
      bInterfaceSubClass    255 Vendor Specific Subclass
      bInterfaceProtocol    255 Vendor Specific Protocol
      iInterface             28 
      Endpoint Descriptor:
        bLength             7
        bDescriptorType         5
        bEndpointAddress     0x85  EP 5 IN
        bmAttributes            2
          Transfer Type            Bulk
          Synch Type             None
          Usage Type             Data
        wMaxPacketSize     0x0200  1x 512 bytes
        bInterval             0
    Interface Descriptor:
      bLength             9
      bDescriptorType         4
      bInterfaceNumber        4
      bAlternateSetting       1
      bNumEndpoints           1
      bInterfaceClass       255 Vendor Specific Class
      bInterfaceSubClass    255 Vendor Specific Subclass
      bInterfaceProtocol    255 Vendor Specific Protocol
      iInterface             31 
      Endpoint Descriptor:
        bLength             7
        bDescriptorType         5
        bEndpointAddress     0x05  EP 5 OUT
        bmAttributes            2
          Transfer Type            Bulk
          Synch Type             None
          Usage Type             Data
        wMaxPacketSize     0x0200  1x 512 bytes
        bInterval             1
    Interface Descriptor:
      bLength             9
      bDescriptorType         4
      bInterfaceNumber        5
      bAlternateSetting       0
      bNumEndpoints           1
      bInterfaceClass       255 Vendor Specific Class
      bInterfaceSubClass    255 Vendor Specific Subclass
      bInterfaceProtocol    255 Vendor Specific Protocol
      iInterface             29 
      Endpoint Descriptor:
        bLength             7
        bDescriptorType         5
        bEndpointAddress     0x86  EP 6 IN
        bmAttributes            2
          Transfer Type            Bulk
          Synch Type             None
          Usage Type             Data
        wMaxPacketSize     0x0200  1x 512 bytes
        bInterval             0
    Interface Descriptor:
      bLength             9
      bDescriptorType         4
      bInterfaceNumber        5
      bAlternateSetting       1
      bNumEndpoints           1
      bInterfaceClass       255 Vendor Specific Class
      bInterfaceSubClass    255 Vendor Specific Subclass
      bInterfaceProtocol    255 Vendor Specific Protocol
      iInterface             30 
      Endpoint Descriptor:
        bLength             7
        bDescriptorType         5
        bEndpointAddress     0x86  EP 6 IN
        bmAttributes            5
          Transfer Type            Isochronous
          Synch Type             Asynchronous
          Usage Type             Data
        wMaxPacketSize     0x0240  1x 576 bytes
        bInterval             1
me@Me-Me:~$ 

----------------

20191024             http://192.168.8.1/html/home.html

20191020             https://www.ecosia.org/search?tt=mzl&q=usb+video+grabber+silvercrest+treiber

20191020             EM2863

hunspell has limitations on what affix morphemes you can attach to word roots with the consequence that not all languages with

rich inflectional morphologies can be conveniently implemented in hunspell.

to use a generic framework of finite-state automata for these tasks.

With finite-state automata it is possible to implement the spell-checking functionality as a one-tape weighted automaton containing

the language model and a two-tape weighted automaton containing the error model.

In addition, we extend the hunspell spell-checking system by using simple corpus-based unigram probability training

With this probability trained lexicon it is possible to fine-tune and improve the suggestions for spelling errors.

We also provide a path for integrating our finite-state spell-checking and hyphenation into applications through the open-source spell-checking library voikko 4 , which

has been integrated with typical open-source software, such as Mozilla Firefox, Open-Office.org and the Gnome desktop via enchant.

A spell-checking dictionary is essentially A spelling correction model or an error model T E is

For practical applications, the input alphabet needs to be extended by a special any symbol with the semantics of a character not belonging

to the alphabet of the language model in order to account for input text containing typos outside the target natural language alphabet.

A hunspell spell-checking dictionary consists of two files: a dictionary file and an affix file.

The dictionary file contains only root forms of words with information about morphological affix classes to combine with the roots.

The affix file contains lists of affixes along with their context restrictions and effects, but
the character set encoding

The ordered confusion set of possible spelling error pairs is given on lines 19–27, where

each line is a pair of a ‘mistyped’ and a ‘corrected’ word separated by whitespace.

POSIX regular expressions

. the context description

‘0’

As our toolkit we use the free open-source HFST toolkit 8 , which is a general purpose API for finite-state automata, and a set of

tools for using legacy data, such as Xerox finite-state morphologies.

the morphotactics

The twolc rule formalism is used for defining context-based rules with two-level automata

em2863

SilverCrest USB 2.0 Video Grabber VG 2000

shell> lsusb

lsusb

EM2863_BOARD_SILVERCREST_VG2000
SilverCrest USB-Video-Grabber VG 2000
0xeb1a:0x2863

Define 	Name 	Vendor/Product ID

sudo lshw

Beschreibung: Allgemeines USB-Gerät
Produkt: Video Grabber
Hersteller: DK
Physische ID: 2
Bus-Informationen: usb@2:2
Version: 40.02
Seriennummer: 0000000000
Fähigkeiten: usb-2.00
Konfiguration: driver=cx231xx maxpower=500mA speed=480Mbit/s

sudo apt-get install lshw

sudo lshw -short

/0/100/14/0/7             generic        EMV Smartcard Reader

Video Grabber

0xeb1a:0x2863

Vendor/Product ID

lsusb

(lsusb -v)

udev-util.c

Take note: a new batch being sold by Lidl late 2012 called SilverCrest USB 2.0 Video Grabber SVG 2.0 A2 and looks exactly similar and has the same packaging, but uses a different chipset (Conexant CX23103-11Z), identified as ID 1d19:6109 by Dexatek Technology Ltd. The batch sold in 2010 called VG2010 ID 1d19:6105 has a chipset AF9035. The chipset support for AF9035 ID 1d19:6105 has to be enabled in the kernel modules. The kernel driver has to be amended to support the ID 1d19:6105.

lsusb

ID 1d19:6109 Dexatek Technology Ltd.

https://www.linuxtv.org/wiki/index.php/SilverCrest_USB_2.0_Video_Grabber_VG_2000

SilverCrest USB 2.0 Video Grabber VG 2000

1d19:6109

Couldn't open device, some information will be missing

dmesg | egrep '(video|acpi)'

lsmod | grep videodev

gst-launch v4l2src device=/dev/video0 ! 'video/x-raw-yuv,width=640,height=480,framerate=30/1' ! xvimagesink

/sbin/lspci

modprobe lm78

 modprobe lm78

lsusb -v  -d eb1a:2863

20191019             Enchant

20191019             glib

20191019             Watermelon

20191019             Robot esfregona

20191019             O robot esfregona Braava jet® m6 com ligação Wi-Fi® ajuda a limpar a gordura da cozinha, manchas pegajosas e a sujidade entranhada* em toda a casa.

20191019             699,99 €

20191019             https://www.irobot.pt/braava/serie-m

20191019             InnovaGoods Robot Esfregona White - V0100806

20191019             https://www.worten.pt/pequenos-eletrodomesticos/limpeza-de-superficies/aspiradores-robo/aspirador-robo-irobot-mopa-braava-jet-240-autonomia-ate-25-m2-6086148

20191019             Aspirador Robô IROBOT Mopa Braava Jet 240 (Autonomia: Até 25 m2)

20191019             €229,99
------
20191013             https://community.notepad-plus-plus.org/topic/17912/utc-8-problem
------------------------------------------
|20191005             me@Me-Me:~$ sudo df --version
|20191005             [sudo] Passwort für me:
|20191005             df (GNU coreutils) 8.28
|20191005             Copyright © 2017 Free Software Foundation, Inc.
|20191005             Lizenz GPLv3+: GNU GPL Version 3 oder höher <http://gnu.org/licenses/gpl.html>
|20191005             Dies ist freie Software: Sie können sie ändern und weitergeben.
|20191005             Es gibt keinerlei Garantien, soweit wie es das Gesetz erlaubt.
|20191005             Geschrieben von Torbjorn Granlund, David MacKenzie und Paul Eggert.
|20191005             me@Me-Me:~$ ~]# df
|20191005             ~]#: Befehl nicht gefunden.
|20191005             me@Me-Me:~$ sudo df
|20191005             Dateisystem    1K-Blöcke   Benutzt Verfügbar Verw% Eingehängt auf
|20191005             udev             4017460         0   4017460    0% /dev
|20191005             tmpfs             807928      1944    805984    1% /run
|20191005             /dev/sda2      959863856 758391192 152644456   84% /
|20191005             tmpfs            4039628    240388   3799240    6% /dev/shm
|20191005             tmpfs             5120         8      5112    1% /run/lock
|20191005             tmpfs            4039628         0   4039628    0% /sys/fs/cgroup
|20191005             /dev/loop0         21248     21248         0  100% /snap/uefi-fw-tools/15
|20191005             /dev/loop1          4224      4224         0  100% /snap/gnome-calculator/406
|20191005             /dev/loop2          4864      4864         0  100% /snap/network-manager/355
|20191005             /dev/loop3           512       512         0  100% /snap/dav1d/21
|20191005             /dev/loop4         91264     91264         0  100% /snap/core/7713
|20191005             /dev/loop5         55808     55808         0  100% /snap/core18/1144
|20191005             /dev/loop6         15104     15104         0  100% /snap/gnome-characters/317
|20191005             /dev/loop7         75776     75776         0  100% /snap/wine-platform-3-stable/6
|20191005             /dev/loop8        153600    153600         0  100% /snap/gnome-3-28-1804/71
|20191005             /dev/loop9          4864      4864         0  100% /snap/network-manager/314
|20191005             /dev/loop10       222464    222464         0  100% /snap/wine-platform-runtime/37
|20191005             /dev/loop11         1024      1024         0  100% /snap/gnome-logs/73
|20191005             /dev/loop12       144128    144128         0  100% /snap/gnome-3-26-1604/92
|20191005             /dev/loop14       144128    144128         0  100% /snap/gnome-3-26-1604/90
|20191005             /dev/loop13         3840      3840         0  100% /snap/gnome-system-monitor/100
|20191005             /dev/loop15         3968      3968         0  100% /snap/notepad-plus-plus/212
|20191005             /dev/loop16       207232    207232         0  100% /snap/vlc/770
|20191005             /dev/loop17        43904     43904         0  100% /snap/gtk-common-themes/1313
|20191005             /dev/loop18        90880     90880         0  100% /snap/core/7396
|20191005             /dev/loop19         3840      3840         0  100% /snap/gnome-system-monitor/95
|20191005             /dev/loop20       268544    268544         0  100% /snap/gnss-sdr-next/317
|20191005             /dev/loop21       153600    153600         0  100% /snap/gnome-3-28-1804/67
|20191005             /dev/loop22        21248     21248         0  100% /snap/uefi-fw-tools/14
|20191005             /dev/loop23        88832     88832         0  100% /snap/simplescreenrecorder/1
|20191005             /dev/sda1         523248      6232    517016    2% /boot/efi
|20191005             /dev/loop24        77568     77568         0  100% /snap/cubicsdr-casept/4
|20191005             /dev/loop25         4352      4352         0  100% /snap/gnome-calculator/501
|20191005             /dev/loop26        36224     36224         0  100% /snap/gtk-common-themes/1198
|20191005             /dev/loop27        55808     55808         0  100% /snap/core18/1192
|20191005             /dev/loop29        15104     15104         0  100% /snap/gnome-characters/296
|20191005             /dev/loop28       268544    268544         0  100% /snap/gnss-sdr-next/312
|20191005             /dev/loop30       207744    207744         0  100% /snap/vlc/1049
|20191005             /dev/loop31         4864      4864         0  100% /snap/network-manager/379
|20191005             /dev/loop32         1024      1024         0  100% /snap/gnome-logs/81
|20191005             tmpfs             807924        44    807880    1% /run/user/1000
|20191005             /dev/mmcblk0p1   1899356   1899356         0  100% /media/me/skywavelinux-latest
|20191005             me@Me-Me:~$ sudo df
|20191005             [sudo] Passwort für me:
|20191005             Dateisystem    1K-Blöcke   Benutzt Verfügbar Verw% Eingehängt auf
|20191005             udev             4017460         0   4017460    0% /dev
|20191005             tmpfs             807928      1944    805984    1% /run
|20191005             /dev/sda2      959863856 758482724 152552924   84% /
|20191005             tmpfs            4039628    240432   3799196    6% /dev/shm
|20191005             tmpfs             5120         8      5112    1% /run/lock
|20191005             tmpfs            4039628         0   4039628    0% /sys/fs/cgroup
|20191005             /dev/loop0         21248     21248         0  100% /snap/uefi-fw-tools/15
|20191005             /dev/loop1          4224      4224         0  100% /snap/gnome-calculator/406
|20191005             /dev/loop2          4864      4864         0  100% /snap/network-manager/355
|20191005             /dev/loop3           512       512         0  100% /snap/dav1d/21
|20191005             /dev/loop4         91264     91264         0  100% /snap/core/7713
|20191005             /dev/loop5         55808     55808         0  100% /snap/core18/1144
|20191005             /dev/loop6         15104     15104         0  100% /snap/gnome-characters/317
|20191005             /dev/loop7         75776     75776         0  100% /snap/wine-platform-3-stable/6
|20191005             /dev/loop8        153600    153600         0  100% /snap/gnome-3-28-1804/71
|20191005             /dev/loop9          4864      4864         0  100% /snap/network-manager/314
|20191005             /dev/loop10       222464    222464         0  100% /snap/wine-platform-runtime/37
|20191005             /dev/loop11         1024      1024         0  100% /snap/gnome-logs/73
|20191005             /dev/loop12       144128    144128         0  100% /snap/gnome-3-26-1604/92
|20191005             /dev/loop14       144128    144128         0  100% /snap/gnome-3-26-1604/90
|20191005             /dev/loop13         3840      3840         0  100% /snap/gnome-system-monitor/100
|20191005             /dev/loop15         3968      3968         0  100% /snap/notepad-plus-plus/212
|20191005             /dev/loop16       207232    207232         0  100% /snap/vlc/770
|20191005             /dev/loop17        43904     43904         0  100% /snap/gtk-common-themes/1313
|20191005             /dev/loop18        90880     90880         0  100% /snap/core/7396
|20191005             /dev/loop19         3840      3840         0  100% /snap/gnome-system-monitor/95
|20191005             /dev/loop20       268544    268544         0  100% /snap/gnss-sdr-next/317
|20191005             /dev/loop21       153600    153600         0  100% /snap/gnome-3-28-1804/67
|20191005             /dev/loop22        21248     21248         0  100% /snap/uefi-fw-tools/14
|20191005             /dev/loop23        88832     88832         0  100% /snap/simplescreenrecorder/1
|20191005             /dev/sda1         523248      6232    517016    2% /boot/efi
|20191005             /dev/loop24        77568     77568         0  100% /snap/cubicsdr-casept/4
|20191005             /dev/loop25         4352      4352         0  100% /snap/gnome-calculator/501
|20191005             /dev/loop26        36224     36224         0  100% /snap/gtk-common-themes/1198
|20191005             /dev/loop27        55808     55808         0  100% /snap/core18/1192
|20191005             /dev/loop29        15104     15104         0  100% /snap/gnome-characters/296
|20191005             /dev/loop28       268544    268544         0  100% /snap/gnss-sdr-next/312
|20191005             /dev/loop30       207744    207744         0  100% /snap/vlc/1049
|20191005             /dev/loop31         4864      4864         0  100% /snap/network-manager/379
|20191005             /dev/loop32         1024      1024         0  100% /snap/gnome-logs/81
|20191005             tmpfs             807924        44    807880    1% /run/user/1000
|20191005             /dev/mmcblk0p1   1899356   1899356         0  100% /media/me/skywavelinux-latest
|20191005             me@Me-Me:~$ sudo df -a
|20191005             Dateisystem    1K-Blöcke   Benutzt Verfügbar Verw% Eingehängt auf
|20191005             sysfs             0         0         0     — /sys
|20191005             proc             0         0         0     — /proc
|20191005             udev             4017460         0   4017460    0% /dev
|20191005             devpts             0         0         0     — /dev/pts
|20191005             tmpfs             807928      1944    805984    1% /run
|20191005             /dev/sda2      959863856 758492240 152543408   84% /
|20191005             securityfs             0         0         0     — /sys/kernel/security
|20191005             tmpfs            4039628    240388   3799240    6% /dev/shm
|20191005             tmpfs             5120         8      5112    1% /run/lock
|20191005             tmpfs            4039628         0   4039628    0% /sys/fs/cgroup
|20191005             cgroup             0         0         0     — /sys/fs/cgroup/unified
|20191005             cgroup             0         0         0     — /sys/fs/cgroup/systemd
|20191005             pstore             0         0         0     — /sys/fs/pstore
|20191005             efivarfs             0         0         0     — /sys/firmware/efi/efivars
|20191005             cgroup             0         0         0     — /sys/fs/cgroup/cpu,cpuacct
|20191005             cgroup             0         0         0     — /sys/fs/cgroup/devices
|20191005             cgroup             0         0         0     — /sys/fs/cgroup/cpuset
|20191005             cgroup             0         0         0     — /sys/fs/cgroup/net_cls,net_prio
|20191005             cgroup             0         0         0     — /sys/fs/cgroup/pids
|20191005             cgroup             0         0         0     — /sys/fs/cgroup/freezer
|20191005             cgroup             0         0         0     — /sys/fs/cgroup/hugetlb
|20191005             cgroup             0         0         0     — /sys/fs/cgroup/blkio
|20191005             cgroup             0         0         0     — /sys/fs/cgroup/memory
|20191005             cgroup             0         0         0     — /sys/fs/cgroup/rdma
|20191005             cgroup             0         0         0     — /sys/fs/cgroup/perf_event
|20191005             systemd-1             —         —         —     — /proc/sys/fs/binfmt_misc
|20191005             debugfs             0         0         0     — /sys/kernel/debug
|20191005             hugetlbfs             0         0         0     — /dev/hugepages
|20191005             mqueue             0         0         0     — /dev/mqueue
|20191005             fusectl             0         0         0     — /sys/fs/fuse/connections
|20191005             configfs             0         0         0     — /sys/kernel/config
|20191005             /dev/loop0         21248     21248         0  100% /snap/uefi-fw-tools/15
|20191005             /dev/loop1          4224      4224         0  100% /snap/gnome-calculator/406
|20191005             /dev/loop2          4864      4864         0  100% /snap/network-manager/355
|20191005             /dev/loop3           512       512         0  100% /snap/dav1d/21
|20191005             /dev/loop4         91264     91264         0  100% /snap/core/7713
|20191005             /dev/loop5         55808     55808         0  100% /snap/core18/1144
|20191005             /dev/loop6         15104     15104         0  100% /snap/gnome-characters/317
|20191005             /dev/loop7         75776     75776         0  100% /snap/wine-platform-3-stable/6
|20191005             /dev/loop8        153600    153600         0  100% /snap/gnome-3-28-1804/71
|20191005             /dev/loop9          4864      4864         0  100% /snap/network-manager/314
|20191005             /dev/loop10       222464    222464         0  100% /snap/wine-platform-runtime/37
|20191005             /dev/loop11         1024      1024         0  100% /snap/gnome-logs/73
|20191005             /dev/loop12       144128    144128         0  100% /snap/gnome-3-26-1604/92
|20191005             /dev/loop14       144128    144128         0  100% /snap/gnome-3-26-1604/90
|20191005             /dev/loop13         3840      3840         0  100% /snap/gnome-system-monitor/100
|20191005             /dev/loop15         3968      3968         0  100% /snap/notepad-plus-plus/212
|20191005             /dev/loop16       207232    207232         0  100% /snap/vlc/770
|20191005             /dev/loop17        43904     43904         0  100% /snap/gtk-common-themes/1313
|20191005             /dev/loop18        90880     90880         0  100% /snap/core/7396
|20191005             /dev/loop19         3840      3840         0  100% /snap/gnome-system-monitor/95
|20191005             /dev/loop20       268544    268544         0  100% /snap/gnss-sdr-next/317
|20191005             /dev/loop21       153600    153600         0  100% /snap/gnome-3-28-1804/67
|20191005             /dev/loop22        21248     21248         0  100% /snap/uefi-fw-tools/14
|20191005             /dev/loop23        88832     88832         0  100% /snap/simplescreenrecorder/1
|20191005             /dev/sda1         523248      6232    517016    2% /boot/efi
|20191005             /dev/loop24        77568     77568         0  100% /snap/cubicsdr-casept/4
|20191005             binfmt_misc            0         0         0     — /proc/sys/fs/binfmt_misc
|20191005             /dev/loop25         4352      4352         0  100% /snap/gnome-calculator/501
|20191005             /dev/loop26        36224     36224         0  100% /snap/gtk-common-themes/1198
|20191005             /dev/loop27        55808     55808         0  100% /snap/core18/1192
|20191005             /dev/loop29        15104     15104         0  100% /snap/gnome-characters/296
|20191005             /dev/loop28       268544    268544         0  100% /snap/gnss-sdr-next/312
|20191005             /dev/loop30       207744    207744         0  100% /snap/vlc/1049
|20191005             /dev/loop31         4864      4864         0  100% /snap/network-manager/379
|20191005             /dev/loop32         1024      1024         0  100% /snap/gnome-logs/81
|20191005             tmpfs             807924        44    807880    1% /run/user/1000
|20191005             tmpfs             807928      1944    805984    1% /run/snapd/ns
|20191005             nsfs             0         0         0     — /run/snapd/ns/network-manager.mnt
|20191005             nsfs             0         0         0     — /run/snapd/ns/uefi-fw-tools.mnt
|20191005             gvfsd-fuse             0         0         0     — /run/user/1000/gvfs
|20191005             /dev/mmcblk0p1   1899356   1899356         0  100% /media/me/skywavelinux-latest
|20191005             /dev/fuse             0         0         0     — /run/user/1000/doc
|20191005             nsfs             0         0         0     — /run/snapd/ns/notepad-plus-plus.mnt
|20191005             me@Me-Me:~$ sudo df h
|20191005             df: h: Datei oder Verzeichnis nicht gefunden
|20191005             me@Me-Me:~$ sudo df -h
|20191005             Dateisystem    Größe Benutzt Verf. Verw% Eingehängt auf
|20191005             udev            3,9G       0  3,9G    0% /dev
|20191005             tmpfs           789M    1,9M  788M    1% /run
|20191005             /dev/sda2       916G    724G  146G   84% /
|20191005             tmpfs           3,9G    236M  3,7G    6% /dev/shm
|20191005             tmpfs           5,0M    8,0K  5,0M    1% /run/lock
|20191005             tmpfs           3,9G       0  3,9G    0% /sys/fs/cgroup
|20191005             /dev/loop0       21M     21M     0  100% /snap/uefi-fw-tools/15
|20191005             /dev/loop1      4,2M    4,2M     0  100% /snap/gnome-calculator/406
|20191005             /dev/loop2      4,8M    4,8M     0  100% /snap/network-manager/355
|20191005             /dev/loop3      512K    512K     0  100% /snap/dav1d/21
|20191005             /dev/loop4       90M     90M     0  100% /snap/core/7713
|20191005             /dev/loop5       55M     55M     0  100% /snap/core18/1144
|20191005             /dev/loop6       15M     15M     0  100% /snap/gnome-characters/317
|20191005             /dev/loop7       74M     74M     0  100% /snap/wine-platform-3-stable/6
|20191005             /dev/loop8      150M    150M     0  100% /snap/gnome-3-28-1804/71
|20191005             /dev/loop9      4,8M    4,8M     0  100% /snap/network-manager/314
|20191005             /dev/loop10     218M    218M     0  100% /snap/wine-platform-runtime/37
|20191005             /dev/loop11     1,0M    1,0M     0  100% /snap/gnome-logs/73
|20191005             /dev/loop12     141M    141M     0  100% /snap/gnome-3-26-1604/92
|20191005             /dev/loop14     141M    141M     0  100% /snap/gnome-3-26-1604/90
|20191005             /dev/loop13     3,8M    3,8M     0  100% /snap/gnome-system-monitor/100
|20191005             /dev/loop15     3,9M    3,9M     0  100% /snap/notepad-plus-plus/212
|20191005             /dev/loop16     203M    203M     0  100% /snap/vlc/770
|20191005             /dev/loop17      43M     43M     0  100% /snap/gtk-common-themes/1313
|20191005             /dev/loop18      89M     89M     0  100% /snap/core/7396
|20191005             /dev/loop19     3,8M    3,8M     0  100% /snap/gnome-system-monitor/95
|20191005             /dev/loop20     263M    263M     0  100% /snap/gnss-sdr-next/317
|20191005             /dev/loop21     150M    150M     0  100% /snap/gnome-3-28-1804/67
|20191005             /dev/loop22      21M     21M     0  100% /snap/uefi-fw-tools/14
|20191005             /dev/loop23      87M     87M     0  100% /snap/simplescreenrecorder/1
|20191005             /dev/sda1       511M    6,1M  505M    2% /boot/efi
|20191005             /dev/loop24      76M     76M     0  100% /snap/cubicsdr-casept/4
|20191005             /dev/loop25     4,3M    4,3M     0  100% /snap/gnome-calculator/501
|20191005             /dev/loop26      36M     36M     0  100% /snap/gtk-common-themes/1198
|20191005             /dev/loop27      55M     55M     0  100% /snap/core18/1192
|20191005             /dev/loop29      15M     15M     0  100% /snap/gnome-characters/296
|20191005             /dev/loop28     263M    263M     0  100% /snap/gnss-sdr-next/312
|20191005             /dev/loop30     203M    203M     0  100% /snap/vlc/1049
|20191005             /dev/loop31     4,8M    4,8M     0  100% /snap/network-manager/379
|20191005             /dev/loop32     1,0M    1,0M     0  100% /snap/gnome-logs/81
|20191005             tmpfs           789M     44K  789M    1% /run/user/1000
|20191005             /dev/mmcblk0p1  1,9G    1,9G     0  100% /media/me/skywavelinux-latest
|20191005             me@Me-Me:~$

|20191005             me@Me-Me:~$ sudo df --version
|20191005             [sudo] Passwort für me:
|20191005             df (GNU coreutils) 8.28
|20191005             Copyright © 2017 Free Software Foundation, Inc.
|20191005             Lizenz GPLv3+: GNU GPL Version 3 oder höher <http://gnu.org/licenses/gpl.html>
|20191005             Dies ist freie Software: Sie können sie ändern und weitergeben.
|20191005             Es gibt keinerlei Garantien, soweit wie es das Gesetz erlaubt.
|20191005             Geschrieben von Torbjorn Granlund, David MacKenzie und Paul Eggert.
|20191005             me@Me-Me:~$ ~]# df
|20191005             ~]#: Befehl nicht gefunden.
|20191005             me@Me-Me:~$ sudo df
|20191005             Dateisystem    1K-Blöcke   Benutzt Verfügbar Verw% Eingehängt auf
|20191005             udev             4017460         0   4017460    0% /dev
|20191005             tmpfs             807928      1944    805984    1% /run
|20191005             /dev/sda2      959863856 758391192 152644456   84% /
|20191005             tmpfs            4039628    240388   3799240    6% /dev/shm
|20191005             tmpfs             5120         8      5112    1% /run/lock
|20191005             tmpfs            4039628         0   4039628    0% /sys/fs/cgroup
|20191005             /dev/loop0         21248     21248         0  100% /snap/uefi-fw-tools/15
|20191005             /dev/loop1          4224      4224         0  100% /snap/gnome-calculator/406
|20191005             /dev/loop2          4864      4864         0  100% /snap/network-manager/355
|20191005             /dev/loop3           512       512         0  100% /snap/dav1d/21
|20191005             /dev/loop4         91264     91264         0  100% /snap/core/7713
|20191005             /dev/loop5         55808     55808         0  100% /snap/core18/1144
|20191005             /dev/loop6         15104     15104         0  100% /snap/gnome-characters/317
|20191005             /dev/loop7         75776     75776         0  100% /snap/wine-platform-3-stable/6
|20191005             /dev/loop8        153600    153600         0  100% /snap/gnome-3-28-1804/71
|20191005             /dev/loop9          4864      4864         0  100% /snap/network-manager/314
|20191005             /dev/loop10       222464    222464         0  100% /snap/wine-platform-runtime/37
|20191005             /dev/loop11         1024      1024         0  100% /snap/gnome-logs/73
|20191005             /dev/loop12       144128    144128         0  100% /snap/gnome-3-26-1604/92
|20191005             /dev/loop14       144128    144128         0  100% /snap/gnome-3-26-1604/90
|20191005             /dev/loop13         3840      3840         0  100% /snap/gnome-system-monitor/100
|20191005             /dev/loop15         3968      3968         0  100% /snap/notepad-plus-plus/212
|20191005             /dev/loop16       207232    207232         0  100% /snap/vlc/770
|20191005             /dev/loop17        43904     43904         0  100% /snap/gtk-common-themes/1313
|20191005             /dev/loop18        90880     90880         0  100% /snap/core/7396
|20191005             /dev/loop19         3840      3840         0  100% /snap/gnome-system-monitor/95
|20191005             /dev/loop20       268544    268544         0  100% /snap/gnss-sdr-next/317
|20191005             /dev/loop21       153600    153600         0  100% /snap/gnome-3-28-1804/67
|20191005             /dev/loop22        21248     21248         0  100% /snap/uefi-fw-tools/14
|20191005             /dev/loop23        88832     88832         0  100% /snap/simplescreenrecorder/1
|20191005             /dev/sda1         523248      6232    517016    2% /boot/efi
|20191005             /dev/loop24        77568     77568         0  100% /snap/cubicsdr-casept/4
|20191005             /dev/loop25         4352      4352         0  100% /snap/gnome-calculator/501
|20191005             /dev/loop26        36224     36224         0  100% /snap/gtk-common-themes/1198
|20191005             /dev/loop27        55808     55808         0  100% /snap/core18/1192
|20191005             /dev/loop29        15104     15104         0  100% /snap/gnome-characters/296
|20191005             /dev/loop28       268544    268544         0  100% /snap/gnss-sdr-next/312
|20191005             /dev/loop30       207744    207744         0  100% /snap/vlc/1049
|20191005             /dev/loop31         4864      4864         0  100% /snap/network-manager/379
|20191005             /dev/loop32         1024      1024         0  100% /snap/gnome-logs/81
|20191005             tmpfs             807924        44    807880    1% /run/user/1000
|20191005             /dev/mmcblk0p1   1899356   1899356         0  100% /media/me/skywavelinux-latest
|20191005             me@Me-Me:~$ sudo df
|20191005             [sudo] Passwort für me:
|20191005             Dateisystem    1K-Blöcke   Benutzt Verfügbar Verw% Eingehängt auf
|20191005             udev             4017460         0   4017460    0% /dev
|20191005             tmpfs             807928      1944    805984    1% /run
|20191005             /dev/sda2      959863856 758482724 152552924   84% /
|20191005             tmpfs            4039628    240432   3799196    6% /dev/shm
|20191005             tmpfs             5120         8      5112    1% /run/lock
|20191005             tmpfs            4039628         0   4039628    0% /sys/fs/cgroup
|20191005             /dev/loop0         21248     21248         0  100% /snap/uefi-fw-tools/15
|20191005             /dev/loop1          4224      4224         0  100% /snap/gnome-calculator/406
|20191005             /dev/loop2          4864      4864         0  100% /snap/network-manager/355
|20191005             /dev/loop3           512       512         0  100% /snap/dav1d/21
|20191005             /dev/loop4         91264     91264         0  100% /snap/core/7713
|20191005             /dev/loop5         55808     55808         0  100% /snap/core18/1144
|20191005             /dev/loop6         15104     15104         0  100% /snap/gnome-characters/317
|20191005             /dev/loop7         75776     75776         0  100% /snap/wine-platform-3-stable/6
|20191005             /dev/loop8        153600    153600         0  100% /snap/gnome-3-28-1804/71
|20191005             /dev/loop9          4864      4864         0  100% /snap/network-manager/314
|20191005             /dev/loop10       222464    222464         0  100% /snap/wine-platform-runtime/37
|20191005             /dev/loop11         1024      1024         0  100% /snap/gnome-logs/73
|20191005             /dev/loop12       144128    144128         0  100% /snap/gnome-3-26-1604/92
|20191005             /dev/loop14       144128    144128         0  100% /snap/gnome-3-26-1604/90
|20191005             /dev/loop13         3840      3840         0  100% /snap/gnome-system-monitor/100
|20191005             /dev/loop15         3968      3968         0  100% /snap/notepad-plus-plus/212
|20191005             /dev/loop16       207232    207232         0  100% /snap/vlc/770
|20191005             /dev/loop17        43904     43904         0  100% /snap/gtk-common-themes/1313
|20191005             /dev/loop18        90880     90880         0  100% /snap/core/7396
|20191005             /dev/loop19         3840      3840         0  100% /snap/gnome-system-monitor/95
|20191005             /dev/loop20       268544    268544         0  100% /snap/gnss-sdr-next/317
|20191005             /dev/loop21       153600    153600         0  100% /snap/gnome-3-28-1804/67
|20191005             /dev/loop22        21248     21248         0  100% /snap/uefi-fw-tools/14
|20191005             /dev/loop23        88832     88832         0  100% /snap/simplescreenrecorder/1
|20191005             /dev/sda1         523248      6232    517016    2% /boot/efi
|20191005             /dev/loop24        77568     77568         0  100% /snap/cubicsdr-casept/4
|20191005             /dev/loop25         4352      4352         0  100% /snap/gnome-calculator/501
|20191005             /dev/loop26        36224     36224         0  100% /snap/gtk-common-themes/1198
|20191005             /dev/loop27        55808     55808         0  100% /snap/core18/1192
|20191005             /dev/loop29        15104     15104         0  100% /snap/gnome-characters/296
|20191005             /dev/loop28       268544    268544         0  100% /snap/gnss-sdr-next/312
|20191005             /dev/loop30       207744    207744         0  100% /snap/vlc/1049
|20191005             /dev/loop31         4864      4864         0  100% /snap/network-manager/379
|20191005             /dev/loop32         1024      1024         0  100% /snap/gnome-logs/81
|20191005             tmpfs             807924        44    807880    1% /run/user/1000
|20191005             /dev/mmcblk0p1   1899356   1899356         0  100% /media/me/skywavelinux-latest
|20191005             me@Me-Me:~$ sudo df -a
|20191005             Dateisystem    1K-Blöcke   Benutzt Verfügbar Verw% Eingehängt auf
|20191005             sysfs             0         0         0     — /sys
|20191005             proc             0         0         0     — /proc
|20191005             udev             4017460         0   4017460    0% /dev
|20191005             devpts             0         0         0     — /dev/pts
|20191005             tmpfs             807928      1944    805984    1% /run
|20191005             /dev/sda2      959863856 758492240 152543408   84% /
|20191005             securityfs             0         0         0     — /sys/kernel/security
|20191005             tmpfs            4039628    240388   3799240    6% /dev/shm
|20191005             tmpfs             5120         8      5112    1% /run/lock
|20191005             tmpfs            4039628         0   4039628    0% /sys/fs/cgroup
|20191005             cgroup             0         0         0     — /sys/fs/cgroup/unified
|20191005             cgroup             0         0         0     — /sys/fs/cgroup/systemd
|20191005             pstore             0         0         0     — /sys/fs/pstore
|20191005             efivarfs             0         0         0     — /sys/firmware/efi/efivars
|20191005             cgroup             0         0         0     — /sys/fs/cgroup/cpu,cpuacct
|20191005             cgroup             0         0         0     — /sys/fs/cgroup/devices
|20191005             cgroup             0         0         0     — /sys/fs/cgroup/cpuset
|20191005             cgroup             0         0         0     — /sys/fs/cgroup/net_cls,net_prio
|20191005             cgroup             0         0         0     — /sys/fs/cgroup/pids
|20191005             cgroup             0         0         0     — /sys/fs/cgroup/freezer
|20191005             cgroup             0         0         0     — /sys/fs/cgroup/hugetlb
|20191005             cgroup             0         0         0     — /sys/fs/cgroup/blkio
|20191005             cgroup             0         0         0     — /sys/fs/cgroup/memory
|20191005             cgroup             0         0         0     — /sys/fs/cgroup/rdma
|20191005             cgroup             0         0         0     — /sys/fs/cgroup/perf_event
|20191005             systemd-1             —         —         —     — /proc/sys/fs/binfmt_misc
|20191005             debugfs             0         0         0     — /sys/kernel/debug
|20191005             hugetlbfs             0         0         0     — /dev/hugepages
|20191005             mqueue             0         0         0     — /dev/mqueue
|20191005             fusectl             0         0         0     — /sys/fs/fuse/connections
|20191005             configfs             0         0         0     — /sys/kernel/config
|20191005             /dev/loop0         21248     21248         0  100% /snap/uefi-fw-tools/15
|20191005             /dev/loop1          4224      4224         0  100% /snap/gnome-calculator/406
|20191005             /dev/loop2          4864      4864         0  100% /snap/network-manager/355
|20191005             /dev/loop3           512       512         0  100% /snap/dav1d/21
|20191005             /dev/loop4         91264     91264         0  100% /snap/core/7713
|20191005             /dev/loop5         55808     55808         0  100% /snap/core18/1144
|20191005             /dev/loop6         15104     15104         0  100% /snap/gnome-characters/317
|20191005             /dev/loop7         75776     75776         0  100% /snap/wine-platform-3-stable/6
|20191005             /dev/loop8        153600    153600         0  100% /snap/gnome-3-28-1804/71
|20191005             /dev/loop9          4864      4864         0  100% /snap/network-manager/314
|20191005             /dev/loop10       222464    222464         0  100% /snap/wine-platform-runtime/37
|20191005             /dev/loop11         1024      1024         0  100% /snap/gnome-logs/73
|20191005             /dev/loop12       144128    144128         0  100% /snap/gnome-3-26-1604/92
|20191005             /dev/loop14       144128    144128         0  100% /snap/gnome-3-26-1604/90
|20191005             /dev/loop13         3840      3840         0  100% /snap/gnome-system-monitor/100
|20191005             /dev/loop15         3968      3968         0  100% /snap/notepad-plus-plus/212
|20191005             /dev/loop16       207232    207232         0  100% /snap/vlc/770
|20191005             /dev/loop17        43904     43904         0  100% /snap/gtk-common-themes/1313
|20191005             /dev/loop18        90880     90880         0  100% /snap/core/7396
|20191005             /dev/loop19         3840      3840         0  100% /snap/gnome-system-monitor/95
|20191005             /dev/loop20       268544    268544         0  100% /snap/gnss-sdr-next/317
|20191005             /dev/loop21       153600    153600         0  100% /snap/gnome-3-28-1804/67
|20191005             /dev/loop22        21248     21248         0  100% /snap/uefi-fw-tools/14
|20191005             /dev/loop23        88832     88832         0  100% /snap/simplescreenrecorder/1
|20191005             /dev/sda1         523248      6232    517016    2% /boot/efi
|20191005             /dev/loop24        77568     77568         0  100% /snap/cubicsdr-casept/4
|20191005             binfmt_misc            0         0         0     — /proc/sys/fs/binfmt_misc
|20191005             /dev/loop25         4352      4352         0  100% /snap/gnome-calculator/501
|20191005             /dev/loop26        36224     36224         0  100% /snap/gtk-common-themes/1198
|20191005             /dev/loop27        55808     55808         0  100% /snap/core18/1192
|20191005             /dev/loop29        15104     15104         0  100% /snap/gnome-characters/296
|20191005             /dev/loop28       268544    268544         0  100% /snap/gnss-sdr-next/312
|20191005             /dev/loop30       207744    207744         0  100% /snap/vlc/1049
|20191005             /dev/loop31         4864      4864         0  100% /snap/network-manager/379
|20191005             /dev/loop32         1024      1024         0  100% /snap/gnome-logs/81
|20191005             tmpfs             807924        44    807880    1% /run/user/1000
|20191005             tmpfs             807928      1944    805984    1% /run/snapd/ns
|20191005             nsfs             0         0         0     — /run/snapd/ns/network-manager.mnt
|20191005             nsfs             0         0         0     — /run/snapd/ns/uefi-fw-tools.mnt
|20191005             gvfsd-fuse             0         0         0     — /run/user/1000/gvfs
|20191005             /dev/mmcblk0p1   1899356   1899356         0  100% /media/me/skywavelinux-latest
|20191005             /dev/fuse             0         0         0     — /run/user/1000/doc
|20191005             nsfs             0         0         0     — /run/snapd/ns/notepad-plus-plus.mnt
|20191005             me@Me-Me:~$ sudo df h
|20191005             df: h: Datei oder Verzeichnis nicht gefunden
|20191005             me@Me-Me:~$ sudo df -h
|20191005             Dateisystem    Größe Benutzt Verf. Verw% Eingehängt auf
|20191005             udev            3,9G       0  3,9G    0% /dev
|20191005             tmpfs           789M    1,9M  788M    1% /run
|20191005             /dev/sda2       916G    724G  146G   84% /
|20191005             tmpfs           3,9G    236M  3,7G    6% /dev/shm
|20191005             tmpfs           5,0M    8,0K  5,0M    1% /run/lock
|20191005             tmpfs           3,9G       0  3,9G    0% /sys/fs/cgroup
|20191005             /dev/loop0       21M     21M     0  100% /snap/uefi-fw-tools/15
|20191005             /dev/loop1      4,2M    4,2M     0  100% /snap/gnome-calculator/406
|20191005             /dev/loop2      4,8M    4,8M     0  100% /snap/network-manager/355
|20191005             /dev/loop3      512K    512K     0  100% /snap/dav1d/21
|20191005             /dev/loop4       90M     90M     0  100% /snap/core/7713
|20191005             /dev/loop5       55M     55M     0  100% /snap/core18/1144
|20191005             /dev/loop6       15M     15M     0  100% /snap/gnome-characters/317
|20191005             /dev/loop7       74M     74M     0  100% /snap/wine-platform-3-stable/6
|20191005             /dev/loop8      150M    150M     0  100% /snap/gnome-3-28-1804/71
|20191005             /dev/loop9      4,8M    4,8M     0  100% /snap/network-manager/314
|20191005             /dev/loop10     218M    218M     0  100% /snap/wine-platform-runtime/37
|20191005             /dev/loop11     1,0M    1,0M     0  100% /snap/gnome-logs/73
|20191005             /dev/loop12     141M    141M     0  100% /snap/gnome-3-26-1604/92
|20191005             /dev/loop14     141M    141M     0  100% /snap/gnome-3-26-1604/90
|20191005             /dev/loop13     3,8M    3,8M     0  100% /snap/gnome-system-monitor/100
|20191005             /dev/loop15     3,9M    3,9M     0  100% /snap/notepad-plus-plus/212
|20191005             /dev/loop16     203M    203M     0  100% /snap/vlc/770
|20191005             /dev/loop17      43M     43M     0  100% /snap/gtk-common-themes/1313
|20191005             /dev/loop18      89M     89M     0  100% /snap/core/7396
|20191005             /dev/loop19     3,8M    3,8M     0  100% /snap/gnome-system-monitor/95
|20191005             /dev/loop20     263M    263M     0  100% /snap/gnss-sdr-next/317
|20191005             /dev/loop21     150M    150M     0  100% /snap/gnome-3-28-1804/67
|20191005             /dev/loop22      21M     21M     0  100% /snap/uefi-fw-tools/14
|20191005             /dev/loop23      87M     87M     0  100% /snap/simplescreenrecorder/1
|20191005             /dev/sda1       511M    6,1M  505M    2% /boot/efi
|20191005             /dev/loop24      76M     76M     0  100% /snap/cubicsdr-casept/4
|20191005             /dev/loop25     4,3M    4,3M     0  100% /snap/gnome-calculator/501
|20191005             /dev/loop26      36M     36M     0  100% /snap/gtk-common-themes/1198
|20191005             /dev/loop27      55M     55M     0  100% /snap/core18/1192
|20191005             /dev/loop29      15M     15M     0  100% /snap/gnome-characters/296
|20191005             /dev/loop28     263M    263M     0  100% /snap/gnss-sdr-next/312
|20191005             /dev/loop30     203M    203M     0  100% /snap/vlc/1049
|20191005             /dev/loop31     4,8M    4,8M     0  100% /snap/network-manager/379
|20191005             /dev/loop32     1,0M    1,0M     0  100% /snap/gnome-logs/81
|20191005             tmpfs           789M     44K  789M    1% /run/user/1000
|20191005             /dev/mmcblk0p1  1,9G    1,9G     0  100% /media/me/skywavelinux-latest
|20191005             me@Me-Me:~$

---
20191005             https://www.itsmarttricks.com/how-to-install-jedit-text-editor-application-in-ubuntu-18-04/

----

20191003             ISO 8859-1 ist neben US-ASCII und UTF-8 (einer Unicode-Kodierung) die wohl wichtigste und am häufigsten gebrauchte Kodierung für lateinische Schriften.
20191003             Für mindestens folgende Sprachen reicht ISO 8859-1 aus:

---------
"─"
20190925             der beste Stift "Microsoft Surface Pen"

20190925             zugehörigen bzw. kompatiblen Apps wie Whiteboard, Penbook, etc.

20190925             Sprache zu Text umwandeln, indem man diktiert, kann das iPad oder iPhone hervorragend!

20190925             Ich habe u.a. Live Scribe und Bamboo Folio im Einsatz gehabt, aber war nie wirklich zufrieden. J

20190925             Auf jeden Fall erwähnenswert wären hier also die Surface-Geräte oder die x360 von HP oder was es in der Windowswelt sonst noch so mit Stift gibt.

------------------
20190919             sudo apt-get install dictionaries-common

20190919             dictionaries-common

20190919             The extension's files have the file extension 'OXT'.

20190919             https://de.wikipedia.org/wiki/Workflow-Management-System

20190919             https://de.wikipedia.org/wiki/Computer_Supported_Cooperative_Work
----

20190918             Aspell-0-50-3-3-

20190918             sudo apt-get install aspell

20190918             sudo apt-get update

20190918             aspell-dictionary

20190918             aspell-fr_0.50-3-7_all.deb

---------------

C:\Program Files (x86)\Aspell\bin\aspell-15.dll

C:\users\me\Application Data\Notepad++\plugins\Config\Hunspell

20190918             file:///home/me/.wine/drive_c/Program%20Files%20(x86)/Notepad++/plugins/DSpellCheck/Aspell/doc/html/manual.html

20190918             c:\Program Files (x86)\Notepad++\plugins\DSpellCheck\Aspell\bin\aspell-15.dll
-------------------
Mehrbenutzereditoren

https://de.wikipedia.org/wiki/Computer_Supported_Cooperative_Work

https://subethaedit.net/

SubEthaEdit

http://msevior.livejournal.com/27859.html

etherpad

AbiWord

etherpad-lite

curl -sL https://deb.nodesource.com/setup_9.x | sudo -E bash -

sudo apt-get install -y nodejs

git clone --branch master https://github.com/ether/etherpad-lite.git && cd etherpad-lite && bin/run.sh

Started Etherpad...
[2019-09-19 12:45:24.489] [DEBUG] console - Running on Node v9.11.2 (minimum required Node version: 6.9.0)
[2019-09-19 12:45:24.521] [INFO] console - All relative paths will be interpreted relative to the identified Etherpad base dir: /home/me/etherpad-lite
[2019-09-19 12:45:24.522] [DEBUG] AbsolutePaths - Relative path "settings.json" can be rewritten to "/home/me/etherpad-lite/settings.json"
[2019-09-19 12:45:24.522] [DEBUG] AbsolutePaths - Relative path "credentials.json" can be rewritten to "/home/me/etherpad-lite/credentials.json"
[2019-09-19 12:45:24.523] [INFO] console - Settings loaded from: /home/me/etherpad-lite/settings.json
[2019-09-19 12:45:24.523] [INFO] console - No credentials file found in /home/me/etherpad-lite/credentials.json. Ignoring.
[2019-09-19 12:45:24.527] [INFO] console - Using skin "no-skin" in dir: /home/me/etherpad-lite/src/static/skins/no-skin
[2019-09-19 12:45:24.527] [INFO] console - Session key file "/home/me/etherpad-lite/SESSIONKEY.txt" not found. Creating with random contents.
[2019-09-19 12:45:24.528] [WARN] console - DirtyDB is used. This is fine for testing but not recommended for PRODUCTION. File location: /home/me/etherpad-lite/var/dirty.db
[2019-09-19 12:45:25.306] [INFO] APIHandler - Api key file "/home/me/etherpad-lite/APIKEY.txt" not found. Creating with random contents.
[2019-09-19 12:45:25.599] [INFO] console - Installed plugins:
[2019-09-19 12:45:25.602] [INFO] console - Report bugs at https://github.com/ether/etherpad-lite/issues
[2019-09-19 12:45:25.603] [INFO] console - Your Etherpad version is 1.7.5 (6a3e4c6)
[2019-09-19 12:45:25.710] [INFO] console - You can access your Etherpad instance at http://0.0.0.0:9001/
[2019-09-19 12:45:25.710] [WARN] console - Admin username and password not set in settings.json.  To access admin please uncomment and edit 'users' in settings.json
[2019-09-19 12:45:25.710] [WARN] console - Etherpad is running in Development mode.  This mode is slower for users and less secure than PRODUCTION mode.  You should set the NODE_ENV environment variable to PRODUCTION by using: export NODE_ENV=PRODUCTION

------
More information about apt-get install

Advanced Package Tool, or APT, is a free software user interface that works with core libraries to handle the installation and removal of software on Debian, 
Ubuntu and other Linux distributions. 
APT simplifies the process of managing software on Unix-like computer systems by automating the retrieval, configuration and installation of software packages,
either from precompiled files or by compiling source code.

apt-get is the command-line tool for handling packages, and 
may be considered the user's "back-end" to other tools using the APT library.

apt-get install is followed by one or more packages desired for installation or upgrading. 
Each package is a package name, not a fully qualified filename. 
All packages required by the package(s) specified for installation will also be retrieved and installed. 
The /etc/apt/sources.list file is used to locate the desired packages. 
If a hyphen is appended to the package name (with no intervening space), the identified package will be removed if it is installed. 
Similarly a plus sign can be used to designate a package to install. 
These latter features may be used to override decisions made by apt-get's conflict resolution system. 
-----------
20190918             Aspell
20190918             sudo apt-get update
20190918             sudo apt-get install aspell
------------------------------
20190914             Aktualisierung für 2 Pakete verfügbar. Führen Sie »apt list --upgradable« aus, um sie anzuzeigen.
me@Me-Me:~$ 
me@Me-Me:~$ apt list --upgradable
Auflistung... Fertig
libsnmp-base/bionic-updates,bionic-updates 5.7.3+dfsg-1.8ubuntu3.3 all [aktualisierbar von: 5.7.3+dfsg-1.8ubuntu3.1]
libsnmp30/bionic-updates 5.7.3+dfsg-1.8ubuntu3.3 amd64 [aktualisierbar von: 5.7.3+dfsg-1.8ubuntu3.1]
???????????????
20190914             https://github.com/tesseract-ocr/tesseract/wiki/NeuralNetsInTesseract4.00
20190914             https://github.com/Shreeshrii/tess4training
20190914             https://github.com/tesseract-ocr/tesseract/wiki/4.0-with-LSTM
20190914             sudo apt update
20190914             sudo apt install ttf-mscorefonts-installer
20190914             sudo apt install fonts-dejavu
20190914             fc-cache -vf
----
https://www.researchgate.net/profile.ProfileStatsReportProfileViews.html?date=2019-08-18
researchgate
hinzkunzclix
£r^btf(f>of(ini^rlbcrt
--------------
<?xml version="1.0" encoding="UTF-8"?>
<playlist xmlns="http://xspf.org/ns/0/" xmlns:vlc="http://www.videolan.org/vlc/playlist/ns/0/" version="1">
<title>DVB Playlist</title>
<creator>w_scan—20170107</creator>
<info>http://wirbel.htpc-forum.de</info>
<trackList>
<track>
<title>0001. RTP 1</title>
<location>dvb-t://frequency=754000000</location>
<extension application="http://www.videolan.org/vlc/playlist/0">
<vlc:option>dvb-bandwidth=8</vlc:option>
<vlc:option>dvb-ts-id=1101</vlc:option>
<vlc:option>dvb-code-rate-hp=2/3</vlc:option>
<vlc:option>dvb-modulation=64QAM</vlc:option>
<vlc:option>dvb-transmission=8</vlc:option>
<vlc:option>dvb-guard=1/4</vlc:option>
<vlc:id>2</vlc:id>
<vlc:option>program=1101</vlc:option>
</extension>
</track>
<track>
<title>0002. RTP 2</title>
<location>dvb-t://frequency=754000000</location>
<extension application="http://www.videolan.org/vlc/playlist/0">
<vlc:option>dvb-bandwidth=8</vlc:option>
<vlc:option>dvb-ts-id=1101</vlc:option>
<vlc:option>dvb-code-rate-hp=2/3</vlc:option>
<vlc:option>dvb-modulation=64QAM</vlc:option>
<vlc:option>dvb-transmission=8</vlc:option>
<vlc:option>dvb-guard=1/4</vlc:option>
<vlc:id>3</vlc:id>
<vlc:option>program=1102</vlc:option>
</extension>
</track>
<track>
<title>0003. SIC</title>
<location>dvb-t://frequency=754000000</location>
<extension application="http://www.videolan.org/vlc/playlist/0">
<vlc:option>dvb-bandwidth=8</vlc:option>
<vlc:option>dvb-ts-id=1101</vlc:option>
<vlc:option>dvb-code-rate-hp=2/3</vlc:option>
<vlc:option>dvb-modulation=64QAM</vlc:option>
<vlc:option>dvb-transmission=8</vlc:option>
<vlc:option>dvb-guard=1/4</vlc:option>
<vlc:id>4</vlc:id>
<vlc:option>program=1103</vlc:option>
</extension>
</track>
<track>
<title>0004. TVI</title>
<location>dvb-t://frequency=754000000</location>
<extension application="http://www.videolan.org/vlc/playlist/0">
<vlc:option>dvb-bandwidth=8</vlc:option>
<vlc:option>dvb-ts-id=1101</vlc:option>
<vlc:option>dvb-code-rate-hp=2/3</vlc:option>
<vlc:option>dvb-modulation=64QAM</vlc:option>
<vlc:option>dvb-transmission=8</vlc:option>
<vlc:option>dvb-guard=1/4</vlc:option>
<vlc:id>5</vlc:id>
<vlc:option>program=1104</vlc:option>
</extension>
</track>
<track>
<title>0005. ARTV</title>
<location>dvb-t://frequency=754000000</location>
<extension application="http://www.videolan.org/vlc/playlist/0">
<vlc:option>dvb-bandwidth=8</vlc:option>
<vlc:option>dvb-ts-id=1101</vlc:option>
<vlc:option>dvb-code-rate-hp=2/3</vlc:option>
<vlc:option>dvb-modulation=64QAM</vlc:option>
<vlc:option>dvb-transmission=8</vlc:option>
<vlc:option>dvb-guard=1/4</vlc:option>
<vlc:id>6</vlc:id>
<vlc:option>program=1107</vlc:option>
</extension>
</track>
<track>
<title>0006. RTP 3</title>
<location>dvb-t://frequency=754000000</location>
<extension application="http://www.videolan.org/vlc/playlist/0">
<vlc:option>dvb-bandwidth=8</vlc:option>
<vlc:option>dvb-ts-id=1101</vlc:option>
<vlc:option>dvb-code-rate-hp=2/3</vlc:option>
<vlc:option>dvb-modulation=64QAM</vlc:option>
<vlc:option>dvb-transmission=8</vlc:option>
<vlc:option>dvb-guard=1/4</vlc:option>
<vlc:id>7</vlc:id>
<vlc:option>program=1108</vlc:option>
</extension>
</track>
<track>
<title>0007. RTP Memoria</title>
<location>dvb-t://frequency=754000000</location>
<extension application="http://www.videolan.org/vlc/playlist/0">
<vlc:option>dvb-bandwidth=8</vlc:option>
<vlc:option>dvb-ts-id=1101</vlc:option>
<vlc:option>dvb-code-rate-hp=2/3</vlc:option>
<vlc:option>dvb-modulation=64QAM</vlc:option>
<vlc:option>dvb-transmission=8</vlc:option>
<vlc:option>dvb-guard=1/4</vlc:option>
<vlc:id>8</vlc:id>
<vlc:option>program=1109</vlc:option>
</extension>
</track>
</trackList>
</playlist>
----------
20190626             Check that your GPS is live and you can get data from it
20190626             Start by making sure you can get data from your GPS, otherwise the later steps will be very frustrating. 
In this command
20190626             stty -F /dev/ttyXXX ispeed 4800 && cat </dev/ttyXXX
20190626             replace ttyXXX with the filename of the port. 
This will probably be either /dev/ttyUSB0 or /dev/ttyS0. 
stty -F /dev/ttyS0 ispeed 4800 && cat </dev/ttyS0

If you are on a *BSD Unix or MacOS X, replace -F with -f.

20190626             stty -F /dev/ttyXXX ispeed 4800 && cat </dev/ttyXXX

20190626             /dev/ttyUSB0

20190626             stty -F /dev/ttyUSB0 ispeed 4800 && cat </dev/ttyUSB0

20190626             lspci

20190626             me@Me-Me:~$ lspci
20190626             00:00.0 Host bridge: Intel Corporation Broadwell-U Host Bridge -OPI (rev 09)
20190626             00:02.0 VGA compatible controller: Intel Corporation HD Graphics 5500 (rev 09)
20190626             00:03.0 Audio device: Intel Corporation Broadwell-U Audio Controller (rev 09)
20190626             00:14.0 USB controller: Intel Corporation Wildcat Point-LP USB xHCI Controller (rev 03)
20190626             00:16.0 Communication controller: Intel Corporation Wildcat Point-LP MEI Controller #1 (rev 03)
20190626             00:19.0 Ethernet controller: Intel Corporation Ethernet Connection (3) I218-LM (rev 03)
20190626             00:1b.0 Audio device: Intel Corporation Wildcat Point-LP High Definition Audio Controller (rev 03)
20190626             00:1c.0 PCI bridge: Intel Corporation 82801 Mobile PCI Bridge (rev e3)
20190626             00:1c.1 PCI bridge: Intel Corporation Wildcat Point-LP PCI Express Root Port #2 (rev e3)
20190626             00:1c.2 PCI bridge: Intel Corporation Wildcat Point-LP PCI Express Root Port #3 (rev e3)
20190626             00:1d.0 USB controller: Intel Corporation Wildcat Point-LP USB EHCI Controller (rev 03)
20190626             00:1f.0 ISA bridge: Intel Corporation Wildcat Point-LP LPC Controller (rev 03)
20190626             00:1f.2 SATA controller: Intel Corporation Wildcat Point-LP SATA Controller [AHCI Mode] (rev 03)
20190626             00:1f.3 SMBus: Intel Corporation Wildcat Point-LP SMBus Controller (rev 03)
20190626             02:00.0 Network controller: Intel Corporation Wireless 7265 (rev 59)
20190626             03:00.0 Unassigned class [ff00]: Realtek Semiconductor Co., Ltd. RTS5227 PCI Express Card Reader (rev 01)
20190626             me@Me-Me:~$

20190626             lsusb

20190626             me@Me-Me:~$ lsusb
20190626             Bus 001 Device 002: ID 8087:8001 Intel Corp.
20190626             Bus 001 Device 001: ID 1d6b:0002 Linux Foundation 2.0 root hub
20190626             Bus 003 Device 001: ID 1d6b:0003 Linux Foundation 3.0 root hub
20190626             Bus 002 Device 009: ID 058f:9540 Alcor Micro Corp. AU9540 Smartcard Reader
20190626             Bus 002 Device 005: ID 8087:0a2a Intel Corp.
20190626             Bus 002 Device 008: ID 062a:4101 MosArt Semiconductor Corp. Wireless Keyboard/Mouse
20190626             Bus 002 Device 010: ID 12d1:1001 Huawei Technologies Co., Ltd. E161/E169/E620/E800 HSDPA Modem
20190626             Bus 002 Device 006: ID 064e:9924 Suyin Corp.
20190626             Bus 002 Device 003: ID 0424:2514 Standard Microsystems Corp. USB 2.0 Hub
20190626             Bus 002 Device 004: ID 1d19:1101 Dexatek Technology Ltd. DK DVB-T Dongle
20190626             Bus 002 Device 002: ID 1a40:0101 Terminus Technology Inc. Hub
20190626             Bus 002 Device 001: ID 1d6b:0002 Linux Foundation 2.0 root hub

20190626             pcsc_scan

20190626             sudo apt install pcsc-tools

20190626             uname -sr

20190626             groups

20190626             pcsc_scan

20190626             me@Me-Me:~$ uname -sr
20190626             Linux 4.15.0-52-generic
20190626             me@Me-Me:~$ groups
20190626             me adm cdrom sudo dip plugdev lpadmin sambashare
20190626             me@Me-Me:~$ pcsc_scan
20190626             PC/SC device scanner
20190626             V 1.5.2 (c) 2001—2017, Ludovic Rousseau <ludovic.rousseau@free.fr>
20190626             SCardEstablishContext: Service not available.

--------------------------
Check that your GPS is live and you can get data from it

Start by making sure you can get data from your GPS, otherwise the later steps will be very frustrating.
In this command

stty -F /dev/ttyXXX ispeed 4800 && cat </dev/ttyXXX

replace ttyXXX with the filename of the port. 
This will probably be either /dev/ttyUSB0 
or 
/dev/ttyS0. 
If you are on a *BSD Unix or MacOS X, replace -F with -f.

stty -F /dev/ttyUSB0 ispeed 4800 && cat </dev/ttyUSB0

-----------------------------
20190615             sudo apt-get install modem-manager-gui

20190615             sudo apt autoremove

20190615             linux-headers-4.15.0-48 linux-headers-4.15.0-48-generic

20190615             sudo apt-get install modem-manager-gui

20190615             modem-manager-gui ist schon die neueste Version (0.0.19.1-1)

-------------------------
20190615             http://blog.alfatomega

20190615             %O@ON8F2Qu6y

20190615             magico

---------------
https://en.wikipedia.org/wiki/The_Fisherman_and_His_Wife
kaffeine
Re: reinstall packages with command prompt?

    well there's
sudo apt-get install modem-manager-gui
    Code:

    sudo apt-get install --reinstall package

    or if you want tO—REInstall config files as well you could do

    Code:

    sudo apt-get purge package
    sudo apt-get install package

20190521             https://bugs.launchpad.net/ubuntu/+source/modem-manager-gui/0.0.19.1-1

20190520             https://askubuntu.com/questions/1144503/modem-manager-gui-does-not-work

20190409             Balkenmäher   Mähwerk

20190409             Regulärer Preis: 1.648,00 €

20190409             Sonderpreis: 1.498,00 €

20190409             Details
20190409             Kreiselmäher: Die ideale Futterbasis
20190409             Das macht Appetit: Der Kreiselmäher AS 565 KM macht einen sauberen Schnitt und die Ablage des Wiesengrases im Schwad erleichtert das Abtragen für die Futternutzung erheblich.Kreiselmäher sind die wirtschaftliche und wartungsarme Alternative zum Balkenmäher und sind eine ganz besondere Erfindung für alle, die das Gras unzerkleinert als Futter verwenden wollen. Kein Zusammenrechen mehr, nur reihenweise aufladen und fertig. Das Ganze durch die wendige Konstruktion auch in engem Gelände mit beweglich gelagerten, beidseitig verwendbaren Messern auf 56 cm Schnittbreite und manuell sperrbarem Differenzial einsetzbar.
20190409             TECHNISCHE DATEN
20190409             GerätetypAS 565 KM
20190409             Geräte FamilieKreiselmäher
20190409             GrasauswurfSeitliche Grasablage
20190409             Schnitthöhe (mm)40
20190409             Aufwuchshöhe (cm)ca. 60
20190409             Motor-TypB + S, 4-Takt - 850 E Series I/C
20190409             Nennleistung (kW (PS))3,1 (4,3)
20190409             StartvorrichtungSeilstart
20190409             Gewicht (kg)64
20190409             Fahrgeschwindigkeit vorwärts (km/h)2,0
20190409             Transportmaße (cm L/B/H)120/63/71
20190409             Füllmenge Kraftstofftank (Liter)1.2
20190409             Schnittbreite (Arbeitsbreite) (cm)58
20190409             Flächenleistung max. (m²/h)1100
20190409             Motor-BauartEinzylinder-Viertakt-Motor
20190409             Hubraum (cm³)190
20190409             Motordrehzahl (min-¹)3000
20190409             FahrantriebHinterradantrieb
20190409             Betriebsmaße (cm L/B/H)171/75/101
20190409             Schneideinrichtung, ArtKreiselmähscheibe mit 4 beweglich gelagerten Klingen

http://www.maeher-shop.de/angebot/gartengeraete-rasenmaeher/as-motor-565-km-kreiselmaher.html

20190409             Die LUMAG-Kreiselmäher werden mit einem Benzinmotor angetrieben und ersetzen den veralteten Balkenmäher. Die Funktionsweise bei dieser Art des Hochgrasmähers ist ein drehender Teller auf dem 3 Klingen angebracht sind. Diese schneiden das Mähgut direkt und legen es seitlich im Schwad ab. Weiterhin gibt es bei dieser Funktionsweise einen sehr sauberen Schnitt durch die Fliehkraft der Klingen und durch die rotierende Bewegung des Kreiselmähers wenige Vibrationen. Ein Rupfen wie man es von einem Balkenmäher gewohnt ist, gibt es bei einem Kreiselmäher nicht, da man keine zwei übereinander laufenden Messer einstellen muss.
20190409             Generell sollte ein Kreiselmäher dann benutzt werden, wenn das Mähgut verfüttert werden soll oder die Fläche komplett von Resten geräumt werden muss.

20190409             NAVIGATION
20190409             Brennholzbearbeitung
20190409             Baumaschinen
20190409             Garten- & Landschaftsbau
20190409             Zubehör & Ersatzteile
20190409             Baumstumpffräse
20190409             Erdbohrer
20190409             Gartenrollsiebe
20190409             Generatoren & Stromerzeuger
20190409             Häcksler & Schredder
20190409             Heckenscheren
20190409             Mäher & Mulcher
20190409             Hochgrasmäher
20190409             Hochgrasmulcher
20190409             Rasenmäher
20190409             Rasentrimmer & Sensen
20190409             Unkrautbürste
20190409             Zubehör / Ersatzteile
20190409             Dumper & Transporter
20190409             Tischlerei & Hobbybastler
20190409             Herbst- & Winterhelfer
20190409             Transport & Lager
20190409             Kompressoren
20190409             % Aktion %
20190409             5.00 / 5.00
20190409             Sehr gut
20190409             Kurze knackige, Kommunikation schneller Versand. Su...
20190409             Gesamt: 17
20190409             pool
20190409             Hochgrasschneider / Kreiselmäher HGS50058
20190409             Hersteller:	LUMAG
20190409             Art.Nr.:	HGS-50058
20190409             EAN:	4047424005835
20190409             999,01 EUR
20190409             inkl. 19 % MwSt. / Versandkostenfrei
20190409             Menge

https://www.youtube.com/embed/sVv1vWV9wQM

------------------
20190405             Externe Anwendungen/Befehle, die zur Indizierung Ihrer Dateitypen gebraucht werden und nicht gefunden wurden - vom letzten Indizierungslauf hinterlegt unter /home/me/.recoll/missing:
20190405             Perl::Image::ExifTool (image/gif image/png)
20190405             antiword (application/msword)
20190405             djvutxt (image/vnd.djvu)
20190405             python:chm (application/x-chm)
20190405             python:libxml2/python:libxslt1 (application/vnd.openxmlformats-officedocument.presentationml.presentation application/vnd.openxmlformats-officedocument.wordprocessingml.document application/vnd.sun.xml.draw application/vnd.sun.xml.writer image/svg+xml)
20190405             python:midi (audio/x-karaoke)
20190405             python:pylzma (application/x-7z-compressed)
20190405             python:rarfile (application/x-rar)
20190405             untex (application/x-tex)
----------------------------------------
201903401             GRASS=  (Geographic Resources Analysis Support SYSTEM)
https://www.youtube.com/redirect?redir_token=Ilpsn_GkeVnbuSZxRJ9BEMdYQHd8MTU1NDIwNTcxOUAxNTU0MTE5MzE5&event=comments&q=https%3A%2F%2Fgrass.osgeo.org%2Fdownload%2Fsample-data%2F&stzid=UgxL2BvIEYdaQGTgly94AaABAg.8Gbj6c12x9s8WbzkPmh1W3

201903401             Multistats
201903401             —VOR, 2—JAHREn (bearbeitet)
201903401             This needs to be updated.  I downloaded GRASS GIS 7 (whereas this tutorial is based on 6).  
There are some differences that have me very confused.  
For example, I believe the grassdata is set-up automatically.  
At least, I was never directed to create a grassdata file.  
Also, the home screen seen at about 7:20 looks different than what I have.  
Viewers take note that this is 3—YEARS—OLD and deals with the previous version of GRASS GIS.  
If there are any GRASS GIS experts out there, there is a need for a current tutorial, and let me know when you have done it.  
I will subscribe.  
According to the YT search, there is not much available.  
There is a lot of moving parts with GIS, and many tutorials I have seen elsewhere assume some prior knowledge.  
For example, I saw one where it says to get an add-in without saying where to get it.  
It was not listed on the home sites list of add-ins, and to make things even more confusing, 
the site just described what the add-ins did without providing a way to download the add-in!  
I'm still not sure how to get an add-in.?

https://www.youtube.com/watch?v=YvEPOfSzhO0

20190401             DGM

20190401             xyz Datei

https://www.youtube.com/watch?v=ehUf7bbC4O4

https://www.youtube.com/watch?v=56xkXMd9XBM&list=PLycBDiXWmuxnfLUjs1wkm6WvYsazeLZ0K

20190303             Ubuntu Total Recoll - HDD Volltextsuche

20190303             Die grundlegenden Einheiten /watch?v=f01fZY8r38w

https://www.youtube.comeines regulären Ausdrucks sind solche, die ein einzelnes Zeichen beschreiben. 
Die meisten Zeichen (darunter alle Buchstaben und Ziffern) passen auf sich selbst, zum Beispiel passt "4" auf alle Vieren. 
Alle Zeichen mit 1 besonderen Bedeutung (wie zum Beispiel der Punkt ".") lassen sich durch das Voranstellen eines Rückstrichs "\" ihrer besonderen Bedeutung berauben. 
Um also 1 Punkt "." zu finden muss man in dem regulären Ausdruck ein "\." verwenden. 
Um den Rückstrich selbst zu finden, benötigt man ein "\\".

20190303             verarbeiten auch viele Texteditoren reguläre Ausdrücke in der Funktion „Suchen und Ersetzen“.

20190303             1 einfacher Anwendungsfall von regulären Ausdrücken sind Wildcards.

20190303             Wildcard (vom englischen Wildcard, 1 Spielkarte im Poker), Joker (nach Joker, 1 Spielkarte) oder Platzhalter bezeichnet im Computer-Bereich 1 Platzhalter für andere Zeichen. 
Dieses Konzept wird des Öfteren auch als Globbing oder Trunkierung (Abschneiden) bezeichnet.

https://de.wikipedia.org/wiki/Regul%C3%A4rer_Ausdruck#Regul%C3%A4re_Ausdr%C3%BCcke_in_der_Praxis

https://de.wikipedia.org/wiki/Wildcard_(Informatik)

https://de.wikipedia.org/wiki/Regul%C3%A4rer_Ausdruck#Regul.C3.A4re_Ausdr.C3.BCcke_in_der_Praxis

https://wiki.ubuntuusers.de/grep/

20190214             PowerLite 1700-Series.

20190214             The two high-end models also offer wireless screen mirroring from a smartphone or streaming device(1) with Miracast for optimized connectivity options.

20190214             ll new PowerLite 1700-Series projectors support Chromecast™, Roku® and MHL-enabled devices.

20190214             WXGA resolution, and the flagship PowerLite 1795F features 1080p resolution for Full HD-quality content.

20190214             "Thin as a laptop and just 4 pounds, the PowerLite 1700-Series are lightweight and wireless projectors, ideal for road warriors that require bright images, optimized connectivity and HD quality presentations,"

20190214             Wireless Connectivity: Project from laptop, tablet, or smartphone without plugging into the projector for flexibility and mobility(1)

20190214             Quick and easy setup: Wireless setup from mobile devices by scanning QR code using phone or tablet device(1)

20190214             Availability and Support
20190214             The PowerLite 1781W ($799 MSRP) projector will be sold through authorized retailers, and the PowerLite 1780W ($749 MSRP), 1785W ($1,099 MSRP) and 1795F ($1,249 MSRP) projectors will be sold through authorized Epson resellers.

20190214             ) For wireless functionality, including via the Epson iProjection App, the projector must be configured on a network, either through the Ethernet port on the projector (check model specifications for availability) or via a wireless connection.

20190214             Check your owner's manual to determine if a wireless LAN module must be purchased separately to enable a wireless connection. Not all Epson projectors are able to be networked

20190214             The Epson iProjection App does not support all files and formats. See
www.epson.com for details.

20190214             https://www.youtube.com/embed/X9LPebIAX34?autoplay=1&rel=0

20190214             YW-40

20190214             Miracast

20190214             https://mkchromecast.com/

20190214             sudo ufw allow 5000

20190214             Google Cast and Sonos Devices

20190214             that supports "Miracast"

20190214             https://youtu.be/fCbH-qNaekI
airtime

20190106             TOUMEI Mini Beamer, Android 7.1 C800S Projektor DLP LED Wireless Portable 1080P WiF...
20190106             33
20190106             EUR 228,98

https://www.amazon.de/dp/B07H5G1DQC/?smid=A1Z8SOXUW1AUSZ&tag=preisvergleich-idealode02-21&linkCode=asn&creative=6742&camp=1638&creativeASIN=B07H5G1DQC&ascsubtag=E6Po6og9GYfeUKFMFXkftA#productDetails

20190106             Mini Projektor Beamer, Android7.1 Videoprojektor TOUMEI C800S LED Portable Heimkino Beamer WiFi Bluetooth Quad-Core HDMI / TF / USB Pocket Video Beamer Multi-Bildschirm für Smartphone PC Laptop
20190106             —VON, TOUMEI
20190106             3.8 von 5 Sternen 5 Kundenrezensionen
20190106             Preis: 	EUR 209,99 Kostenlose Lieferung. Details
20190106             Alle Preisangaben inkl. deutscher USt. Weitere Informationen.

20190105             Xgimi H2

20190105             Mlison Projector

20190105             wowoto t8e and toumei v3,
soneed
20190105             MXQ PROJECT
20190105             —VOR, 5—MONATEn
20190105             The Xgimi aurora is more for portability, the z6 would be more for a home environment?

20190105             Xgimi H1 review.?

Notepad++: Mehrere Zeilen tauschen
Es ist leider nicht so ohne weiteres Möglich 1.unsortierte Liste zu invertieren. Um die Zeilen durch zu tauschen, so dass die 1. Zeile —AM—ENDE steht, die 2. Zeile an zweitletzter Stelle, etc., kann man im Notepad++-Editor das Plugin TextFX nutzen.
Zeilen markieren
Zeilennummern hinzufügen
TextFX > TextFX Tools > Insert Line Numbers
Zeilen absteigend sortieren
TextFX > TextFX Tools > +Sort ascending deaktivieren
TextFX > TextFX Tools > Sort lines case sensitive (at column)
Zeilennummern entfernen
TextFX > TextFX Tools  > Delete Line Numbers or 1. Word
Mit Hilfe des Plugins Python Script können die einzelnen Schritte als Script gespeichert werden und per Schaltfläche oder Menü abgerufen werden. Es muss nur noch der betreffenden Text markiert werden und sichergestellt werden, dass Sort ascending deaktiviert ist.
notepad.runMenuCommand('TextFX Tools', 'Insert Line Numbers')
notepad.runMenuCommand('TextFX Tools', 'Sort lines case sensitive (at column)')
notepad.runMenuCommand('TextFX Tools', 'Delete Line Numbers or 1. Word')

Mit der Tastenkombination Strg+Shift+L wird die aktuelle Zeile in Notepad++ gelöscht.

Um bei Notepad++ Text im Block zu markieren, einfach zusätzlich die ALT-Taste drücken.
Durch 1 Klick auf den Dokumentenrand lassen sich Lesezeichen setzen, die mit F2 angesprungen werden können.

STRG + D Zeile duplizieren
STRG + G Gehe zu Zeile
STRG + L Zeile ausschneiden
STRG + B Suche zugehörige Klammer
STRG + M Alle gleichen Wörter markieren
STRG + Nach oben Nach oben scrollen
STRG + BACKSPACE Text vor Cursor löschen (aktives Wort)
STRG + Nach unten Nach unten scrollen
STRG + Entf Text nach Cursor löschen (aktives Wort)
STRG + ALT + I Inkrementelle Suche
STRG + SHIFT + Nach oben Zeile nach oben schieben
STRG + SHIFT + Nach unten Zeile nach unten schieben
STRG + SHIFT + M Alle Markierungen entfernen
Wer die übrigen Shortcuts des Programms studieren will, sollte 1 Blick in die primären Funktionen von Notepad++ werfen, die über den Menüpunkt "Einstellungen -> Tastatur…" und anschließend unter der Registerkarte "Scintilla commands" zu finden sind.

Direkte Autovervollständigung in Notepad++
Notepad++ bietet die Funktion "Autovervollständigung" an, welche durch den Tastaturbefehl STRG + SPACE ein Menü mit den entsprechenden Funktionsvorschlägen einblendet. Seit Version 5 ist es jedoch auch möglich, das Menü ohne Tastaturbefehl direkt bei 1 Texteingabe erscheinen zu lassen. Die Option ist in den Standardeinstellungen des Editors deaktiviert, so dass sie für den 1 oder anderen vielleicht unbemerkt blieb.
Wer die Autovervollständigung (sowohl Funktionen als auch Wörter lassen sich vervollständigen) einschalten möchte, muss lediglich den Eintrag "Aktiviere Autovervollständigung" in den Programmeinstellungen anklicken. Die Option ist über das Menü "Einstellungen -> Optionen…" erreichbar und anschließend über "SICHERHEITS—kopie/Autovervollständigung" zu finden.
Notepad++ Einstellungen
In den Einstellungen kann der Benutzer dann zwischen Funktions- und Wortvervollständigung wählen. Auch der Code-Editor von Dreamweaver bietet die direkte Autovervollständigung (ohne zusätzlichen Tastaturbefehl), welche den Schreibaufwand erheblich verringert.

gibt es 1.Möglichkeit, nur Zeilen, die ein bestimmtes Wortenthalten, oder mit einem bestimmten Begriff beginnen, zu behalten, und den Rest automatiusch zu löschen? Oder derartige Zeilen automatisch zu kopieren?
Ich habe 1.Textdatei, die aus immer wiederkehrenden, gleich aufgebauten Blöcken besteht, von denen ich jeweils nur 1.Zeile behalten will. Wie vorgehen?
Jan Schreiber
Jan Schreiber - 2011-12-09
Das ist zum Glück ganz einfach: Der Suchen-Dialog hat 1 Reiter (Tab) namens "Vorkommnisse markieren". Dort das Kontrollkästchen "Lesezeichen setzen" aktivieren und nach dem fraglichen Wort suchen. Anschließend im Menü "Suchen -> Lesezeichen" den Menüpunkt "Zeilen ohne Lesezeichen löschen" wählen. Auch das Kopieren der gewünschten Zeilen funktioniert mit fast denselben Schritten.
================
multiple lines, words changing
ad charakter at every line
first line
shift, alt, down
type charakter
revrse =, right button, delete

multiple words changing by songle word
settings
multiple editing settt.
enable (ctrl+mouse click/selection)
ctrl
select (left mouse)
type word  ________________  TEXTFX

7.5.7 32 bit
20181117             7.5.7 32 bit

---------------------------------------------
20181115             msg='apparmor="DENIED" operation="dbus_signal"  bus

20181115             usb 2-1.3: dvb_usb_v2: 'Dexatek DK DVB-T Dongle' successfully initialized and connected

20181115             "/usr/bin/dbus-daemon" sauid=105 hostname=? addr=? terminal=?'
-----

apt-get install kdelibs5-dev libvlc-dev libxss-dev vlc \
libkf5coreaddons-dev libkf5i18n-dev libqt5x11extras5-dev \
libkf5windowsystem-dev \
libkf5solid-dev libkf5widgetsaddons-dev kio-dev \
qt5-default libdvbv5-dev \
cmake extra-cmake-modules make g++ gettext

------
https://www.ubuntupit.com/mesa-3d-graphics-library-available-to-install-in-ubuntu-linux/
--------------------
me@Me-Me:~$ glxinfo -B
name of display: :0
display: :0  screen: 0
direct rendering: Yes
Extended renderer info (GLX_MESA_query_renderer):
    Vendor: Intel Open Source Technology Center (0x8086)
    Device: Mesa DRI Intel(R) HD Graphics 5500 (BROADWELL GT2)  (0x16160000             )
    Version: 18.0.5
    Accelerated: yes
    Video memory: 3072MB
    Unified memory: yes
    Preferred profile: core (0x1)
    Max core profile version: 4.5
    Max compat profile version: 3.0
    Max GLES1 profile version: 1.1
    Max GLES[23] profile version: 3.1
OpenGL vendor string: Intel Open Source Technology Center
OpenGL renderer string: Mesa DRI Intel(R) HD Graphics 5500 (BROADWELL GT2) 
OpenGL core profile version string: 4.5 (Core Profile) Mesa 18.0.5
OpenGL core profile shading language version string: 4.50
OpenGL core profile context flags: (none)
OpenGL core profile profile mask: core profile

OpenGL version string: 3.0 Mesa 18.0.5
OpenGL shading language version string: 1.30
OpenGL context flags: (none)

OpenGL ES profile version string: OpenGL ES 3.1 Mesa 18.0.5
OpenGL ES profile shading language version string: OpenGL ES GLSL ES 3.10

me@Me-Me:~$ sudo apt-get install ppa-purge && sudo ppa-purge ppa:ubuntu-x-swat/updates
[sudo] Passwort für me: 
Paketlisten werden gelesen... Fertig
Abhängigkeitsbaum wird aufgebaut.       
Statusinformationen werden eingelesen.... Fertig
Die folgenden Pakete wurden automatisch installiert und werden nicht mehr benötigt:
  linux-image-4.13.0-46-generic linux-image-extra-4.13.0-46-generic
  linux-signed-image-4.13.0-46-generic
Verwenden Sie »sudo apt autoremove«, um sie zu entfernen.
Vorgeschlagene Pakete:
  aptitude
Die folgenden NEUEN Pakete werden installiert:
  ppa-purge
0 aktualisiert, 1 neu installiert, 0 zu entfernen und 0 nicht aktualisiert.
Es müssen 6.312 B an Archiven heruntergeladen werden.
Nach dieser Operation werden 24,6 kB Plattenplatz zusätzlich benutzt.
Holen:1 http://archive.ubuntumirror.dei.uc.pt/ubuntu bionic/universe amd64 ppa-purge all 0.2.8+bzr63 [6.312 B]
Es wurden 6.312 B in 2 s geholt (3.420 B/s).
Vormals nicht ausgewähltes Paket ppa-purge wird gewählt.
(Lese DATEN—BANK ... 271705 Dateien und Verzeichnisse sind —DERZEIT, installiert.)
Vorbereitung zum Entpacken von .../ppa-purge_0.2.8+bzr63_all.deb ...
Entpacken von ppa-purge (0.2.8+bzr63) ...
ppa-purge (0.2.8+bzr63) wird eingerichtet ...
Trigger für man-db (2.8.3-2ubuntu0.1) werden verarbeitet ...
Updating packages lists
PPA to be removed: ubuntu-x-swat updates
Warning:  Could not find package list for PPA: ubuntu-x-swat updates
me@Me-Me:~$ sudo add-apt-repository ppa:ubuntu-x-swat/updates
[sudo] Passwort für me: 
 Updated versions of X.org drivers, libraries, etc. for Ubuntu.

This PPA is for stable upstream releases of X.org components. If you're looking for something even more bleeding-edge, please see the xorg-edgers PPA.

While Ubuntu does not "officially/formally" support these packages, if you discover problems when installing these debs please feel free to report bugs to launchpad. However, please make sure to clearly state that you are running packages from this PPA so we know the fixes need to come here.

If you are upgrading from one release to another with this PPA activated, please install the ppa-purge package and use it to downgrade everything in here beforehand. sudo ppa-purge ppa:ubuntu-x-swat/updates will do it.

[Directions for packaging drivers can be seen at https://wiki.ubuntu.com/X/DriverBuilding]
 Mehr Informationen: https://launchpad.net/~ubuntu-x-swat/+archive/ubuntu/updates
[ENTER] drücken zum Weitermachen oder Strg-c, um das Hinzufügen abzubrechen.

OK:1 http://archive.ubuntumirror.dei.uc.pt/ubuntu bionic InRelease
Holen:2 http://ppa.launchpad.net/ubuntu-x-swat/updates/ubuntu bionic InRelease [20,7 kB]            
OK:3 http://archive.canonical.com/ubuntu bionic InRelease             
Holen:4 http://archive.ubuntumirror.dei.uc.pt/ubuntu bionic-updates InRelease [88,7 kB]
Holen:5 http://ppa.launchpad.net/ubuntu-x-swat/updates/ubuntu bionic/main amd64 Packages [12,4 kB]
Holen:6 http://archive.ubuntumirror.dei.uc.pt/ubuntu bionic-backports InRelease [74,6 kB]          
Holen:7 http://ppa.launchpad.net/ubuntu-x-swat/updates/ubuntu bionic/main i386 Packages [12,4 kB]           
Holen:8 http://archive.ubuntumirror.dei.uc.pt/ubuntu bionic-security InRelease [83,2 kB]             
Holen:9 http://ppa.launchpad.net/ubuntu-x-swat/updates/ubuntu bionic/main Translation-en [8.664 B]
Es wurden 301 kB in 4 s geholt (75,0 kB/s).             
Paketlisten werden gelesen... Fertig
me@Me-Me:~$ glxinfo | grep "OpenGL version"
OpenGL version string: 3.0 Mesa 18.0.5
me@Me-Me:~$ 

--------------------------
me@Me-Me:~$ glxinfo -B
name of display: :0
display: :0  screen: 0
direct rendering: Yes
Extended renderer info (GLX_MESA_query_renderer):
    Vendor: Intel Open Source Technology Center (0x8086)
    Device: Mesa DRI Intel(R) HD Graphics 5500 (BROADWELL GT2)  (0x16160000             )
    Version: 18.0.5
    Accelerated: yes
    Video memory: 3072MB
    Unified memory: yes
    Preferred profile: core (0x1)
    Max core profile version: 4.5
    Max compat profile version: 3.0
    Max GLES1 profile version: 1.1
    Max GLES[23] profile version: 3.1
OpenGL vendor string: Intel Open Source Technology Center
OpenGL renderer string: Mesa DRI Intel(R) HD Graphics 5500 (BROADWELL GT2) 
OpenGL core profile version string: 4.5 (Core Profile) Mesa 18.0.5
OpenGL core profile shading language version string: 4.50
OpenGL core profile context flags: (none)
OpenGL core profile profile mask: core profile

OpenGL version string: 3.0 Mesa 18.0.5
OpenGL shading language version string: 1.30
OpenGL context flags: (none)

OpenGL ES profile version string: OpenGL ES 3.1 Mesa 18.0.5
OpenGL ES profile shading language version string: OpenGL ES GLSL ES 3.10

me@Me-Me:~$ sudo apt-get install ppa-purge && sudo ppa-purge ppa:ubuntu-x-swat/updates
[sudo] Passwort für me: 
Paketlisten werden gelesen... Fertig
Abhängigkeitsbaum wird aufgebaut.       
Statusinformationen werden eingelesen.... Fertig
Die folgenden Pakete wurden automatisch installiert und werden nicht mehr benötigt:
  linux-image-4.13.0-46-generic linux-image-extra-4.13.0-46-generic
  linux-signed-image-4.13.0-46-generic
Verwenden Sie »sudo apt autoremove«, um sie zu entfernen.
Vorgeschlagene Pakete:
  aptitude
Die folgenden NEUEN Pakete werden installiert:
  ppa-purge
0 aktualisiert, 1 neu installiert, 0 zu entfernen und 0 nicht aktualisiert.
Es müssen 6.312 B an Archiven heruntergeladen werden.
Nach dieser Operation werden 24,6 kB Plattenplatz zusätzlich benutzt.
Holen:1 http://archive.ubuntumirror.dei.uc.pt/ubuntu bionic/universe amd64 ppa-purge all 0.2.8+bzr63 [6.312 B]
Es wurden 6.312 B in 2 s geholt (3.420 B/s).
Vormals nicht ausgewähltes Paket ppa-purge wird gewählt.
(Lese DATEN—BANK ... 271705 Dateien und Verzeichnisse sind —DERZEIT, installiert.)
Vorbereitung zum Entpacken von .../ppa-purge_0.2.8+bzr63_all.deb ...
Entpacken von ppa-purge (0.2.8+bzr63) ...
ppa-purge (0.2.8+bzr63) wird eingerichtet ...
Trigger für man-db (2.8.3-2ubuntu0.1) werden verarbeitet ...
Updating packages lists
PPA to be removed: ubuntu-x-swat updates
Warning:  Could not find package list for PPA: ubuntu-x-swat updates

---------------------------------
sudo apt-get install ppa-purge && sudo ppa-purge ppa:ubuntu-x-swat/updates
-----------------------
https://www.google.com/search?client=ubuntu&channel=fs&q=Mesa+18.0.5&ie=utf-8&oe=utf-8
---------------------

Posted byu/grandmastermoth
5 months ago
Upgrade from 16.04 to 18.04 can potentially disable hardware acceleration on Mesa drivers

Upgrading form 16.04 to 18.04 disabled hardware acceleration for me, 
as the 18.04 was using the llvmpipe software renderer. 
I noticed the problem when video playback turned out to be very choppy and slow.

I confirmed it by running the following command:

glxinfo -B

The solution is to delete or comment out the following file:

/etc/X11/Xsession.d/50_check_unity_support

This may affect other people....apologies if this has ALREADY been posted.
-----------------
Bei mir :
---------------
me@Me-Me:~$ glxinfo -B
name of display: :0
display: :0  screen: 0
direct rendering: Yes
Extended renderer info (GLX_MESA_query_renderer):
    Vendor: Intel Open Source Technology Center (0x8086)
    Device: Mesa DRI Intel(R) HD Graphics 5500 (BROADWELL GT2)  (0x16160000             )
    Version: 18.0.5
    Accelerated: yes
    Video memory: 3072MB
    Unified memory: yes
    Preferred profile: core (0x1)
    Max core profile version: 4.5
    Max compat profile version: 3.0
    Max GLES1 profile version: 1.1
    Max GLES[23] profile version: 3.1
OpenGL vendor string: Intel Open Source Technology Center
OpenGL renderer string: Mesa DRI Intel(R) HD Graphics 5500 (BROADWELL GT2) 
OpenGL core profile version string: 4.5 (Core Profile) Mesa 18.0.5
OpenGL core profile shading language version string: 4.50
OpenGL core profile context flags: (none)
OpenGL core profile profile mask: core profile

OpenGL version string: 3.0 Mesa 18.0.5
OpenGL shading language version string: 1.30
OpenGL context flags: (none)

OpenGL ES profile version string: OpenGL ES 3.1 Mesa 18.0.5
OpenGL ES profile shading language version string: OpenGL ES GLSL ES 3.10

-----------------------------------------------
https://www.youtube.com/watch?v=L55OnlsSQvQ
----------------------------------------------------------
sudo add-apt-repository ppa:ubuntugis/ubuntugis-unstable
sudo apt-get update
me@Me-Me:~$ sudo add-apt-repository ppa:ubuntugis/ubuntugis-unstable
[sudo] Passwort für me:
Unstable releases of Ubuntu GIS packages. 
These releases are more bleeding edge and while generally they should work well,
they dont receive the same amount of quality assurance as our stable releases do.
Mehr Informationen: https://launchpad.net/~ubuntugis/+archive/ubuntu/ubuntugis-unstable
[ENTER] drücken zum Weitermachen oder Strg-c, um das Hinzufügen abzubrechen.
gpg: Die "Keybox" `/tmp/tmp1wsuj_6x/pubring.gpg' wurde erstellt
gpg: /tmp/tmp1wsuj_6x/trustdb.gpg: trust-db erzeugt
gpg: Schlüssel 089EBE08314DF160: Öffentlicher Schlüssel "Launchpad ubuntugis-stable" importiert
gpg: Anzahl insgesamt bearbeiteter Schlüssel: 1
gpg:             importiert: 1
OK
me@Me-Me:~$ sudo apt-get update
OK:1 http://archive.canonical.com/ubuntu artful InRelease
OK:2 http://archive.ubuntumirror.dei.uc.pt/ubuntu artful InRelease
Ign:3 http://ppa.launchpad.net/michael-lamothe/ubuntu gutsy InRelease
OK:4 http://archive.ubuntumirror.dei.uc.pt/ubuntu artful-updates InRelease
OK:5 http://archive.ubuntumirror.dei.uc.pt/ubuntu artful-backports InRelease
OK:6 https://dl.winehq.org/wine-builds/ubuntu artful InRelease
Ign:7 http://ppa.launchpad.net/crass/v-mobile-broadband/ubuntu artful InRelease
OK:8 http://archive.ubuntumirror.dei.uc.pt/ubuntu artful-security InRelease
Holen:9 http://archive.ubuntumirror.dei.uc.pt/ubuntu artful/main Translation-en_CA [5.448 B]
Holen:10 http://archive.ubuntumirror.dei.uc.pt/ubuntu artful/universe Translation-en_CA [1.124 B]
Holen:11 http://ppa.launchpad.net/forkotov02/ppa/ubuntu artful InRelease [15,4 kB]
Ign:12 http://ppa.launchpad.net/gnome-dvb-daemon/ppa/ubuntu artful InRelease
Ign:13 http://ppa.launchpad.net/gnome3-team/gnome3/ubuntu artful InRelease
OK:14 http://ppa.launchpad.net/mamarley/tvheadend-git-stable/ubuntu artful InRelease
OK:15 http://ppa.launchpad.net/rvm/smplayer/ubuntu artful InRelease
Ign:16 http://ppa.launchpad.net/shutter/ppa/ubuntu artful InRelease
OK:17 http://ppa.launchpad.net/team-xbmc/ppa/ubuntu artful InRelease
OK:18 http://ppa.launchpad.net/teejee2008/ppa/ubuntu artful InRelease
Ign:19 http://ppa.launchpad.net/ubuntugis/ubuntugis-unstable/ubuntu artful InRelease
Holen:20 http://ppa.launchpad.net/michael-lamothe/ubuntu gutsy Release [27,6 kB]
Fehl:21 http://ppa.launchpad.net/crass/v-mobile-broadband/ubuntu artful Release
404  Not Found
Fehl:22 http://ppa.launchpad.net/gnome-dvb-daemon/ppa/ubuntu artful Release
404  Not Found
Fehl:23 http://ppa.launchpad.net/gnome3-team/gnome3/ubuntu artful Release
404  Not Found
Fehl:24 http://ppa.launchpad.net/shutter/ppa/ubuntu artful Release
404  Not Found
Fehl:25 http://ppa.launchpad.net/ubuntugis/ubuntugis-unstable/ubuntu artful Release
404  Not Found
Ign:26 http://ppa.launchpad.net/michael-lamothe/ubuntu gutsy Release.gpg
Paketlisten werden gelesen... Fertig
E: The repository 'http://ppa.launchpad.net/crass/v-mobile-broadband/ubuntu artful Release' does not have a Release file.
N: Updating from such a repository can't be done securely, and is therefore disabled by default.
N: See apt-secure(8) manpage for repository creation and user configuration details.
E: The repository 'http://ppa.launchpad.net/gnome-dvb-daemon/ppa/ubuntu artful Release' does not have a Release file.
N: Updating from such a repository can't be done securely, and is therefore disabled by default.
N: See apt-secure(8) manpage for repository creation and user configuration details.
E: The repository 'http://ppa.launchpad.net/gnome3-team/gnome3/ubuntu artful Release' does not have a Release file.
N: Updating from such a repository can't be done securely, and is therefore disabled by default.
N: See apt-secure(8) manpage for repository creation and user configuration details.
E: The repository 'http://ppa.launchpad.net/shutter/ppa/ubuntu artful Release' does not have a Release file.
N: Updating from such a repository can't be done securely, and is therefore disabled by default.
N: See apt-secure(8) manpage for repository creation and user configuration details.
E: The repository 'http://ppa.launchpad.net/ubuntugis/ubuntugis-unstable/ubuntu artful Release' does not have a Release file.
N: Updating from such a repository can't be done securely, and is therefore disabled by default.
N: See apt-secure(8) manpage for repository creation and user configuration details.
E: The repository 'http://ppa.launchpad.net/michael-lamothe/ubuntu gutsy Release' is not signed.
N: Updating from such a repository can't be done securely, and is therefore disabled by default.
N: See apt-secure(8) manpage for repository creation and user configuration details.
me@Me-Me:~$
------------------------------
C:\users\me\Application Data\Notepad++\backup\
------------
20180511             0131_radio_news
20180511             _radio_news_mono
20180511             0131_radio
Dexatek DK DVB-T Dongle (Logilink VG0002A) :: 00000991
20180511             Realtek RTL2832U DVB-T on Ubuntu
20180511             demodulate
20180511             CubicSDR
20180511             Dexatek DK DVB-T Dongle on ubuntu 17.1
20180511             kaffeine
20180511             Anyways, pull the TV dongle out, plug it in and immediately open a terminal and type:
20180511             Code:
20180511             dmesg
20180511             Mine looks like this:
20180511             Code:
20180511             [94625.342295] usb 2-1.1: Product: RTL2838UHIDIR
20180511             [94625.342298] usb 2-1.1: Manufacturer: Realtek
20180511             [94625.348056] usb 2-1.1: dvb_usb_v2: found a 'Realtek RTL2832U reference design' in warm state
20180511             [94625.411072] usb 2-1.1: dvb_usb_v2: will pass the complete MPEG2 transport stream to THE—SOFTWARE demuxer
20180511             [94625.411101] DVB: registering new adapter (Realtek RTL2832U reference design)
20180511             [94625.414604] usb 2-1.1: DVB: registering adapter 0 frontend 0 (Realtek RTL2832 (DVB-T))...
20180511             [94625.423970] i2c i2c-0: e4000: Elonics E4000 successfully identified
20180511             [94625.435564] Registered IR keymap rc-empty
20180511             [94625.435739] input: Realtek RTL2832U reference design as /devices/pci0000:00/0000:00:1d.0/usb2/2-1/2-1.1/rc/rc3/input20
20180511             [94625.435878] rc3: Realtek RTL2832U reference design as /devices/pci0000:00/0000:00:1d.0/usb2/2-1/2-1.1/rc/rc3
20180511             [94625.436261] input: MCE IR Keyboard/Mouse (dvb_usb_rtl28xxu) as /devices/virtual/input/input21
20180511             [94625.436559] rc rc3: lirc_dev: driver ir-lirc-codec (dvb_usb_rtl28xxu) registered at minor = 0
20180511             [94625.436571] usb 2-1.1: dvb_usb_v2: schedule remote query interval to 400 msecs
20180511             [94625.448640] usb 2-1.1: dvb_usb_v2: 'Realtek RTL2832U reference design' successfully initialized and connected
20180511             Try MeTV and see if you get the same response. It's in the repositories.
20180511             I'm also trying TVHeadend, that is what I'm really interested in, and here also doesn't work.
20180511             TVHeadend
20180511             I'm going to try MeTV, althought I want TVHEadend to work and it doesn't
20180511             If you try MeTV and it picks up the dongle, that has an autoscan for channels.
20180511             Ich habe von Kaffeine 4 Versionen unter 4 Betriebssystemen auf 2 Laptops. 
3 davon laufen (und deinterlacen) einwandfrei, nur bei dieser Version  hier verdoppelt Deinterlacing die CPU-Last von kaffeine-xbu/Xorg. 
Für mich unbrauchbar.
2018051https://www.youtube.com/watch?v=y8vm9es6FL0
20180511             w_scan
2018051https://www.youtube.com/results?search_query=tvheadend+dvb-tV+ubuntu
20180511             Learn how to install a Hauppauge TV tuner under Ubuntu. For step by step instructions, please see:
www.hauppauge.com/linuxtv
2018051https://www.youtube.com/watch?v=mouZj92Z9bk
20180511             sudo add-apt-repository ppa:team-xbmc/ppa
20180511             sudo apt-get update
20180511             sudo apt-get install
2018051https://www.ubuntuupdates.org/package/xbmc/artful/main/base/kodi-pvr-dvbviewer
--------------------------
20180510             Als Ultrakurzwellen (UKW) bezeichnet man elektromagnetische Wellen in 1 Frequenzbereich von 30 MHz bis 300 MHz, entsprechend Wellenlängen zwischen zehn Meter und 1—METER. Sie liegen somit zwischen den Kurzwellen (die länger sind als Ultrakurzwellen) und den Dezimeterwellen (die kürzer sind).
20180510             Im englischen Sprachraum wird für Ultrakurzwelle der Begriff VHF (very high frequency – sehr hohe Frequenz) verwendet.
20180510             Der Begriff frequency modulation (Frequenzmodulation) wird im Rundfunkbereich fälschlicherweise als Synonym eingesetzt und es wird die Abkürzung FM verwendet.
             Im allgemeinen Sprachgebrauch wird der Begriff UKW häufig für UKW-Rundfunk im Bereich 87,5 bis 108 MHz des VHF-Bandes II verwendet
20180510             Zu den Ultrakurzwellen gehören jedoch auch die für Fernsehsender verwendeten Frequenzen der Rundfunkbänder I und III sowie die unteren und oberen Sonderkanäle des Kabelfernsehens.
20180510             Das Hyperband (Erweiterter Sonderkanalbereich) und die Rundfunkbänder IV und V gehören dagegen zu den Dezimeterwellen.
20180510             Weiterhin ist der Begriff UKW auch im Bereich des Sprechfunks gebräuchlich. Es handelt sich dabei vor allem um das 4-m-Band (also die Frequenzen unterhalb des UKW-Rundfunks), die Bereiche des Flugfunks mit Frequenzen oberhalb 108 MHz sowie das 2-m-BAND—Im Bereich von 140 bis 174 MHz, wo sich viele verschiedene professionelle Funkdienste sowie ein Amateurfunkband befinden.
20180510             Der Begriff Langwellenrundfunk bezeichnet den Rund- bzw. Hörfunk i—METER—LANGwellenband. Hierfür ist der Frequenzbereich zwischen 148,5 kHz und 283,5 kHz vorgesehen. Er dient heute überwiegend zur terrestrischen Ausstrahlung von nationalen Hörfunkprogrammen über die Landesgrenzen hinaus, daneben auch wie der Kurzwellenrundfunk zur Verbreitung fremdsprachiger Programme für Hörer in anderen Ländern
2018051https://de.wikipedia.org/wiki/Ultrakurzwelle
20180510             Ausserdem gibt es 1.Live-Distro (Bootbar ab DVD) mit allen wichtigen Programmen rund um SDR. Informationen dazu auch im GNURadio-Wiki: https://gnuradio.org/redmine/projects/gnuradio/wiki/GNURadioLiveDVD.
20180510             professionelleren RTL-SDR-Stick von Jani Electronics (ca. 120.–sFr.)
20180510             gqrx
20180510             Mit Hilfe der SOFTWARE „gqrx“, die auf gnuradio basiert, kann nun das Frequenzspektrum visualisiert, und bekannte Signale (AM/FM/SSB) demoduliert werden. Der Frequenzbereich und die Bandbreite wird hier von der verwendeten Hardware begrenzt. Zum Testen wählt man am besten 1.bekannte Radio-Frequenz und wählt als Demodulator „FM Stereo“. Im Screenshot läuft Radio SRF1 (Schweizer Radio) auf 88.2 MHz.
20180510             Für den Einstieg in DIE—WELT des SDR eignet sich gqrx sehr gut, da es nicht all zu viele Funktionen bietet und für die meisten Linux-Distributionen als Installations-Paket zur Verfügung steht. Im SOFTWARE—MANAGER der Distribution einfach nach „gqrx“ suchen.
20180510             gqrx-radio_srf1
20180510             1 weiteres Tool für gqrx ist gqrx-scan, dass diverse Scan-Möglichkeiten zur Verfügung stellt: https://github.com/khaytsus/gqrx-scan. Dazu gehört übrigens auch das automatische Aufzeichnen bei Aktivität.
20180510             CubicSDR
20180510             1 sehr interessantes SOFTWARE—PROJEKT ist CubicSDR. Momentan (Mitte 2015) noch in der Preview-Phase, soll es bald viele Möglichkeiten im Zusammenhang mit SDR bieten (z.B. auch das demodulieren mehrerer Signale gleichzeitig).
2018051https://github.com/cjcliffe/CubicSDR
2018051http://www.markus-gerber.ch/2014/11/sdr-unter-linux-mit-einem-realtek-rtl2832u-usb-stick/
2018051https://de.wikipedia.org/wiki/GNU_Radio
------------------------------------------
https://help.ubuntu.com/community/AptGet/Howto?ACTION=show&redirect=AptGetHowto
AptGet/Howto
Redirected from page "AptGetHowto"
Contents
    Package management with APT
       —INTRODUCTIOn
        Commands
            Installation commands
             auto-apt
            Maintenance commands
            Removal commands
            Search commands
        Typical usage example
        Setting up apt-get to use a http-proxy
            TEMPORAry proxy session
            APT configuration file method
            BASH rc method
            How to login a proxy user
        Useful additional packages
        Additional links
        Troubleshooting
(i) This article applies to all supported versions of Ubuntu
Package management with APT
Package management via apt-get runs hand-in-hand with the /etc/apt/sources.list file.
 For information on editing or updating your sources list see SourcesList.
Introduction
This page describes how to handle the packages on your —SYSTEM using apt-get and related commands. For example, you can install a new package, remove an installed package, or update all installed packages to the latest versions.
Commands
All these commands except the search commands must be run as root or with superuser privileges, see sudo for more information.
    IconsPage/example.png Example:
    sudo apt-get install ubuntu-desktop 
Installation commands
    apt-get install <package_name> 
    This command installs a new package.
    apt-get build-dep <package_name> 
    This command searches the repositories and installs the build dependencies for <package_name>. If the package is not in the repositories it will return an error.
    aptitude install <package_name>
    Aptitude is an Ncurses viewer of packages installed or available. 
	Aptitude can be used from the command line in a similar way to apt-get.
	Enter man aptitude for more information.
    APT and aptitude will accept multiple package names as a space delimited list. For example:
    apt-get install <package1_name> <package2_name> <package3_name>
Use the -s flag to simulate an ACTION. For example: "apt-get -s install <package_name>"will simulate installing the package, showing you what packages will be installed and configured.
auto-apt
    auto-apt run <command_string>
    This command runs <command_string> under the control of auto-apt. 
	If a program tries to access a file known to belong in an uninstalled package, auto-apt will install that package using apt-get. 
	This feature requires apt and sudo to work.
    Auto-apt keeps databases which need to be kept up-to-date in order for it to be effective. 
	This is achieved by calling the commands auto-apt update, auto-apt updatedb and auto-apt update-local.
    Usage example
You're compiling a program and, all of a sudden, there's an error because it needs a file you don't have. 
The program auto-apt asks you to install packages if they're needed, stopping the relevant process and continuing once the package is installed.
             # auto-apt run ./configure
        It will then ask to install the needed packages and call apt-get automatically. 
		If you're running X, a graphical interface will replace the default text interface.
Maintenance commands
    apt-get update
    Run this command after changing /etc/apt/sources.list or /etc/apt/preferences . 
	For information regarding /etc/apt/preferences, see PinningHowto. 
	Run this command periodically to make sure your source list is up-to-date. 
	This is the equivalent of "Reload"in Synaptic or "Fetch updates"in Adept.
    apt-get upgrade
    This command upgrades all installed packages. 
	This is the equivalent of "MARK all upgrades"in Synaptic.
    apt-get dist-upgrade
    The same as the above, except add the "smart upgrade"checkbox. 
	It tells APT to use "smart"KONFLIKT resolution system, and
	it will attempt to upgrade the most important packages at the expense of less important ones if necessary.
"apt-get dist-upgrade"does not upgrade from a previous version of Ubuntu. 
For more information of upgrading from a previous version of Ubuntu see 
http://www.ubuntu.com/getubuntu/upgrading
    apt-get check
    This command is a diagnostic tool. It does an update of the package lists and checks for broken dependencies.
    apt-get -f install
    This command does the same thing as Edit->Fix Broken Packages in Synaptic. 
	Do this if you get complaints about packages with "unmet dependencies".
    apt-get autoclean
    This command removes .deb files for packages that are no longer installed on your system. 
	Depending on your installation habits, removing these files from /var/cache/apt/archives may regain a significant amount of diskspace.
    apt-get clean
    The same as above, except it removes all packages from the package cache.
	This may not be desirable if you have a slow INTERNET connection, since
	it will cause you to redownload any packages you need to install a program.
        The package cache is in /var/cache/apt/archives . 
		
		The command
        du -sh /var/cache/apt/archives
        will tell you how much space cached packages are consuming.
    dpkg-reconfigure <package_name>
    Reconfigure the named package. 
	With many packages, you’ll be prompted with some configuration questions you may not have known were there.
For example:
        dpkg-reconfigure fontconfig-config
        will present you with a "wizard"on configuring fonts in Ubuntu.
    echo "<package_name> hold"| dpkg --set-selections
    This command places the desired package on hold.
This command may have the unintended side effect of preventing upgrades to packages that depend on updated versions of the pinned package. 
apt-get dist-upgrade will override this, but will warn you first.
 If you want to use this command with sudo, you need to use echo "<package_name> hold"| sudo dpkg --set-selections not sudo echo "<package_name> hold"| dpkg --set-selections.
    echo "<package_name> install"| dpkg --set-selections
    This command removes the "hold"or "locked package"state set by the above command. The note above about sudo usage applies to this command.
Removal commands
    apt-get remove <package_name>
    This command removes an installed package, leaving configuration files intact.
    apt-get purge <package_name>
    This command completely removes a package and the associated configuration files. 
	Configuration files residing in ~ are not usually affected by this command.
        † operator
If you want to remove package1 and install package2 in one step:
            apt-get remove <package1> <package2>+
            .
    apt-get autoremove
    This command removes packages that were installed by other packages and are no longer needed.
        apt-get autoremove <package_name>
        This command removes an installed package and dependencies.
    While there is no built in way to remove all of your configuration information from your removed packages 
	you can remove all configuration data from every removed package with the following command.
    dpkg -l | grep '^rc' | awk '{print $2}' | xargs dpkg --purge
Search commands
    apt-cache search <search_term>
    Each package has a name and a description. 
	This command lists packages whose name or description contains <search_term>.
    dpkg -l *<search_term>*
    This will find packages whose names contain <search_term>. 
	Similar to apt-cache search, but also 
	shows whether a package is installed on your —SYSTEM by marking it with ii (installed) and un (not installed).
    apt-cache show <package_name>
    This command shows the description of package <package_name> and other relevant information including version, size, dependencies and KONFLIKTs.
    dpkg --print-avail <package_name>
    This command is similar to "apt-cache show".
    dpkg -L <package_name>
    This command will list files in package <package_name>.
    dpkg -c foo.deb
    This command lists files in the package "foo.deb". 
	Note that foo.deb is a pathname. 
	Use this command on .deb packages that you have manually downloaded.
    dlocate <package_name>
    This command determines which installed package owns <package_name>. 
	It shows files from installed packages that match <package_name>, with the name of the package they came from. 
	Consider this to be a "reverse lookup"utility.
In order to use this command, the package dlocate must be installed on your system.
    dpkg -S <filename_search_pattern>
    This command does the same as dlocate, but does not require the installation of any additional packages. 
	It is slower than dlocate but has the advantage of being installed by default on all Debian and Ubuntu systems.
    apt-file search <filename_search_pattern>
    This command acts like dlocate and dpkg -S, but searches all available packages. 
	It answers the question, "what package provides this file?".
        apt-file needs to be updated regularly like apt-get. 
		
		Use the command:
        apt-file update
In order to use this command, the package apt-file must be installed on your system.
    apt-cache pkgnames
    This command provides a listing of every package —IN—THE—system
    A general note on searching: 
	If searching generates a list that is too long, you can filter your results by piping them through the command grep. Examples:
        apt-cache search <filename> | grep -w <filename>
        will show only the files that contain <filename> as a whole word
        dpkg -L package | grep /usr/bin 
        will list files located in THE—DIRECTORy /usr/bin, useful if you're looking for a particular executable.
For more information on apt-get, apt-cache and dpkg consult their manual pages by using the man command. 
These manuals will provide a wider scope of information in addition to all of the options that you can use with each program.
Example:
    man apt-get
    .
Typical usage example
I want to feel the wind in my hair, I want the adrenaline of speed. So let's install a racing game. But 
what racing games are available?
apt-cache search racing game
It gives me a lot of answers. I see a game named "torcs".  
Let's get some more information on this game.
apt-cache show torcs
Hmmm... it seems interesting. But is this game not ALREADY installed on my computer? 
And what is the available version? Which repository is it from (Universe or Main)?
apt-cache policy torcs
Ok, so now, let's install it!
apt-get install torcs
What is the command I must type in the console to launch this game? 
In this example, it's straightforward ("torcs"), but that's not always the case. 
One way of finding the name of the binary is to look at what files the package has installed in "/usr/bin". 
For games, the binary will be in "/usr/games". For administrative programs, it's in "/usr/sbin".
dpkg -L torcs | grep /usr/games/
The 1. part of the command display all files installed by the package "torcs"(try it). 
With the second part, we ask to only display lines containing "/usr/games/".
Hmmm, that game is cool. Maybe there are some extra tracks?
apt-cache search torcs
But I'm running out of space. I will delete the apt cache!
apt-get clean
Oh no, my mother asked me to remove all games from this computer. 
But I want to keep the configuration files so I can simply re-install it later.
apt-get remove torcs
If I want to also remove config files :
apt-get purge torcs
Setting up apt-get to use a http-proxy
These are 3 methods of using apt-get with a http-proxy.
TEMPORAry proxy session
This is a temporary method that you can manually use each time you want to use apt-get through a http-proxy. This method is useful if you only want to temporarily use a http-proxy.
Enter this line in the terminal prior to using apt-get (substitute your details for yourproxyaddress and proxyport).
export http_proxy=http://yourproxyaddress:proxyport
If you normally use sudo to run apt-get you will need to login as root 1. for this to work unless you also add some explicit environment settings to /etc/sudoers, e.g.
Defaults env_keep = "http_proxy https_proxy ftp_proxy"
APT configuration file method
This method uses the apt.conf file which is found in your /etc/apt/ directory. This method is useful if you only want apt-get (and not other applications) to use a http-proxy permanently.
IconsPage/info.png On some installations there will be no apt-conf file set up. This procedure will either edit an existing apt-conf file or create a new apt-conf file.
gksudo gedit /etc/apt/apt.conf
Add this line to your /etc/apt/apt.conf file (substitute your details for yourproxyaddress and proxyport).
Acquire::http::Proxy "http://yourproxyaddress:proxyport";
Save the apt.conf file.
BASH rc method
This method adds a two lines to your .bashrc file in your $HOME directory. This method is useful if you would like apt-get and other applications for instance wget, to use a http-proxy.
gedit ~/.bashrc
Add these lines to the bottom of your ~/.bashrc file (substitute your details for yourproxyaddress and proxyport)
http_proxy=http://yourproxyaddress:proxyport
export http_proxy
Save the file. Close your terminal window and then open another terminal window or source the ~/.bashrc file:
source ~/.bashrc
Test your proxy with sudo apt-get update and whatever networking tool you desire. 
You can use firestarter or conky to see active connections.
If you make a mistake and go back to edit the file AGAIN, you can close the terminal and reopen it or you can source ~/.bashrc as shown above.
source ~/.bashrc
How to login a proxy user
If you need to login to the Proxy server this can be achieved in most cases by using the following layout in specifying the proxy address in http-proxy. (substitute your details for username, password, yourproxyaddress and proxyport)
http_proxy=http://username:password@yourproxyaddress:proxyport
Useful additional packages
    Deborphan
    Debfoster 
Additional links
    Repositories/CommandLine
    PinningHowto
    AutoDeb
    Synaptic Package Manager
    Ubuntu Community Forums: Installations and Upgrades
    How to speed up package updates using apt-fast 
Troubleshooting
    https://help.ubuntu.com/community/PackageManagerTroubleshootingProcedure 
CategoryPackageManagement CategoryCommandLine
AptGet/Howto (last edited 2016-06-30 11:33:13 by clissold345)
THE—MATERIAL on this wiki is available under a free license, see Copyright / License for details
You can contribute to this wiki, see Wiki Guide for details
---------------------------------
20180506             How to Upgrade to Ubuntu 18.04 LTS
20180506             You can upgrade Ubuntu 16.04 LTS to Ubuntu 18.04 LTS, or 17.10 to 18.04, 
using the command line or THE—SOFTWARE Updater app.
-------------------------------------
20180503             https://askubuntu.com/questions/285493/how-to-show-full-date-and-time-in-nautilus-files-3-6-list-view
-----------------------------------------------------------------------
20180503             Advanced format settings
20180503             The Language Support method for setting regional formats assumes that one language-country combination (locale) is sufficient to set all the format aspects in accordance with your preferences. 
Even if that is often the case, —SITUATIONs when you want more fine tuned format settings may occur. 
For such a case, below are some variables that you may want to assign locale names individually. 
You can do so by editing the .profile configuration file in your home folder.
20180503             LC_NUMERIC
20180503             How you format your numbers. For example, in many countries a point is used as a decimal separator, while others use a comma.
20180503             LC_TIME
20180503             How your time and date are formatted.
20180503             LC_MONETARY
20180503             What currency you use, its name, and its symbol.
20180503             Click here for more LC_* variables with explanations.
20180503             An example
20180503             Take a user IN—THE—US who choose \u201cEnglish (UNITED—STATES)\u201d in the drop-down list on the Regional Formats tab. 
If s/he prefers that dates and times are displayed more like what ISO 8601 prescribes than what's typically the case IN—THE—US, the below line may be added to the .profile file:
20180503             export LC_TIME="en_DK.UTF-8"
20180503             https://help.ubuntu.com/community/Locale
20180503             LC_TIME
20180503             How your time and date are formatted.
Use for example "en_DK.UTF-8"to get a 24-hour-clock in some programs. 
20180503             https://forum.ubuntuusers.de/topic/datumsformat-einstellen/
20180503             https://forum.ubuntuusers.de/topic/gnome-einstellungen-DATUM-waehrung-.../?highlight=datumsformat#post-267730
20180503             die Formate DATUM, Währung etc. sind abhängig von der eingestellten Sprache. 
20180503             Wenn du am Loginbildschirm deutsch wählst, dann solltest du das DATUM auch im Format tag.monat.jahr sehen.
20180503             Willst du eines der Formate unabhängig von der Sprache einstellen, dann ist mir kein grafisches Tool für Gnome bekannt. 
20180503             Du kannst dies aber mit 1 Texteditor ändern, indem du die Datei .gnomerc in deinem Home-Verzeichnis erstellst bzw. editierst und folgendes einträgst:
20180503             export LC_TIME="de_DE"
20180503             Damit stellst du das deutsche Datumsformat für diesen 1 Nutzer ein. 
Du kannst natürlich auch 1.andere Sprache nehmen, z.B. C für englisch.
20180503             Es gibt noch einige andere Formate, die du auf diese Weise umstellen kannst. 
Wirf dazu bitte 1 Blick in man locale.
20180503             Beitrag 20060707 11:45
20180503             Ich habe wie oben beschrieben die Datei .gnomerc angepasst, allerdings ohne Erfolg. 
Das Datumsformat ist weiterhin englisch. 
Wenn ich die Sprache komplett auf deutsch ändere stimmt das DATUM. 
Leider möchte ich aber 1 englischen Desktop mit deutschem Datumsformat...
20180503             Ändere die Zeile mal leicht ab.
20180503             export LC_TIME="de_DE.UTF-8"
20180503             Beiträge: 28
20180503             Zitieren
20180503             Beitrag 20060708 19:14
20180503             Das war die Lösung (export LC_TIME="de_DE.UTF-8"). Vielen Dank für den Tipp!
20180503             Würde das DATUM jedoch gerne nach JJJJ-MM-TT einstellen können:
20180503             export LC_TIME="en_DK.UTF-8"in .gnomerc
20180503             gconf-editor
----------------------------------------
sudo apt-get update
-------------------------
201805https://launchpad.net/~gnome-dvb-daemon/+archive/ppa
201805https://launchpad.net/~gnome-dvb-daemon/+archive/ubuntu/ppa
20180501             You can update your —SYSTEM with unsupported packages from this untrusted PPA by adding ppa:gnome-dvb-daemon/ppa to your system's SOFTWARE Sources. (Read about installing)
20180501             sudo add-apt-repository ppa:gnome-dvb-daemon/ppa
20180501             sudo apt-get update
20180501             sudo add-apt-repository ppa:gnome-dvb-daemon/ppa
20180501             sudo apt-get update
----------------
http://knowledge.seagate.com/articles/en_US/FAQ/005929en
How to Diskpart Erase/Clean a Drive Through the Command Prompt
20180426            SIM card slot
20180426             ExpressCard slot
20180426            Some networks require that a valid SIM card be properly inserted in Personal Computer or Handheld Computer incorporating wireless WAN modem.
20180426            N : SIM Card slot
20180426            <Only for model with Wireless WAN>
20180426            \uf0e8
20180426            Reference Manual \u201cWireless WAN\u201d
20180426            O : 2nd LAN Port *4 / Modem Port *5 / IEEE 1394 Interface C
20180426            https://www.google.com/search?q=Wireless+WAN+laptop+sim+slot&client=ubuntu&tbm=isch&tbs=rimg:CY1WhshhptsHIjiaoz1mkUlJ-5DWGFdCIg4Lzl96I4PjUaLZeMMrjjUi0t191SjEGmisz4SNVERgut0fdsSaSav51CoSCZqjPWaRSUn7ERdncLxOv3BeKhIJkNYYV0IiDgsRG8j_1or1o1DEqEgnOX3ojg-NRohE_1cnb0-Hj2DioSCdl4wyuONSLSER2p2eFH9J3GKhIJ3X3VKMQaaKwRIl-YgOq082QqEgnPhI1URGC63RHENezTZCFDJCoSCR92xJpJq_1nUEYGCiIN3h6O-&tbo=u&sa=X&ved=2ahUKEwi1—MPu3dfaAhVJkRQKHekrCDAQ9C96BAgAEBg&biw=1552&bih=863&dpr=1
-----------------
20180417             Kindprozess »/snap/bin/network-manager.networkmanager« konnte nicht ausgeführt werden (Datei oder Verzeichnis nicht gefunden)
-------------------------------------------------------------------
20180417             Ziel	Zugang	Netzmaske	Schnittstelle
20180417             0.0.0.0	0.0.0.0	0.0.0.0	ppp0
20180417             169.254.0.0	0.0.0.0	255.255.0.0	ppp0
20180417             ::1	::	128	lo
20180417             ::	::	0	lo
20180417             ::1	::	128	lo
20180417             ::	::	0	lo
20180417             #
20180417             # ARIN WHOIS data and services are subject to the Terms of Use
20180417             # available at: https://www.arin.net/whois_tou.html
20180417             #
20180417             —If you see inaccuracies in the results, please report at
20180417             # https://www.arin.net/public/whoisinaccuracy/index.xhtml
20180417             #
20180417             # The following results may also be obtained via:
20180417             # https://whois.arin.net/rest/nets;q=169.254.0.0?showDetails=true&showARIN=false&showNonArinTopLevelNet=false&ext=netref2
20180417             #
20180417             NetRange:       169.254.0.0 - 169.254.255.255
20180417             CIDR:           169.254.0.0/16
20180417             NetName:        LINKLOCAL-RFC3927-IANA-RESERVED
20180417             NetHandle:      NET—169-254-0-0-1
20180417             Parent:         NET169 (NET—169-0-0-0-0)
20180417             NetType:        IANA Special Use
20180417             OriginAS:
20180417             ORGANIZATION:   INTERNET Assigned Numbers Authority (IANA)
20180417             RegDate:        1998-01-27
20180417             Updated:        2014-01-09
20180417             Comment:        Computers use addresses starting with "169.254."when they do not have a manually configured address or when they are not told which address to use by a service on the network.  They are commonly called the "link local"addresses.
20180417             Comment:
20180417             Comment:        Routers are not allowed to forward packets sent from an IPv4 "link local"address, so they are always used by a directly connected device.
20180417             Comment:
20180417             Comment:        These addresses were assigned by the IETF, the ORGANIZATION that develops INTERNET protocols, —IN—THE——STANDARDS Track document, RFC3927, which can be found at:
20180417             Comment:        http://datatracker.ietf.org/doc/rfc3927
20180417             Ref:            https://whois.arin.net/rest/net/NET—169-254-0-0-1
20180417             OrgName:        INTERNET Assigned Numbers Authority
20180417             OrgId:          IANA
20180417             Address:        12025 Waterfront Drive
20180417             Address:        Suite 300
20180417             City:           LOS—ANGELES
20180417             StateProv:      CA
20180417             —POSTalCode:     90292
20180417             Country:        US
20180417             RegDate:
20180417             Updated:        2012-08-31
20180417             Ref:            https://whois.arin.net/rest/org/IANA
20180417             OrgTechHandle: IANA-IP-ARIN
20180417             OrgTechName:   ICANN
20180417             OrgTechPhone:  +1-310-301-5820
20180417             OrgTechEmail:  abuse@iana.org
20180417             OrgTechRef:    https://whois.arin.net/rest/poc/IANA-IP-ARIN
20180417             OrgAbuseHandle: IANA-IP-ARIN
20180417             OrgAbuseName:   ICANN
20180417             OrgAbusePhone:  +1-310-301-5820
20180417             OrgAbuseEmail:  abuse@iana.org
20180417             OrgAbuseRef:    https://whois.arin.net/rest/poc/IANA-IP-ARIN
20180417             #
20180417             # ARIN WHOIS data and services are subject to the Terms of Use
20180417             # available at: https://www.arin.net/whois_tou.html
20180417             #
20180417             —If you see inaccuracies in the results, please report at
20180417             # https://www.arin.net/public/whoisinaccuracy/index.xhtml
20180417             #
RenameMaster
Batch renamer tool for
To install PyRenamer in Ubuntu/Linux Mint use this command:
Terminal Commands:
sudo apt-get install pyrenamer
To install Metamorphose2 in Ubuntu 17.10 Artful/17.04 Zesty/16.04 Xenial/Linux Mint 18 use these commands:
Terminal Commands:
wget -O metamorphose2.deb https://goo.gl/eSSDMz
sudo dpkg -i metamorphose2.deb
sudo apt-get -f install
To install RNM Utility in Ubuntu/Linux Mint use these commands:
sudo add-apt-repository -y ppa:neurobin/ppa
sudo apt-get update
sudo apt-get install rnm
E: Paket rnm kann nicht gefunden werden.
Bildschirmfoto von »
exit
Bildschirmfoto von »
—FOTO—VOM, 2018-03—15 01-37-52
{year}{month}{day}
wget -O metamorphose2.deb https://goo.gl/eSSDMz
sudo dpkg -i metamorphose2.deb
sudo apt-get -f install
-------------------------------------------------------------------------
20180322            notepadqq
\home\eppenich\Dokumente\_A_O_\_CHRONOLOGIE_IN_ARBEIT
/media/eppenich/FREECOM HDD/z/mozilla-thunderbird—17-0-es-en-br-fr-de-it-cn-jp-ar-ru-nl-pl-cz-dk-f1—gr-in-kr-no-se-tr-ubu.deb
Thunderbird ist ein voll ausgestatteter E-Mail-, RSS— , Newsgroup- Client, welcher DIE—VERWALTUNG—VON—NEAPELE-Mails sicherer, schneller und einfacher als jemals zuvor gestaltet. Es unterstützt verschiedene Kontotypen (POP, IMAP, Gmail), enthält 1 einfach Kontoeinrichtungsassistenten, ein simples Adressbuch, 1.mit Reitern konfigurierbare Oberfläche, 1 integrierten lernenden Spamfilter, erweiterte Such— , Markierungsfunktionen sowie leichte Verwaltung der E-Mails dank Markierens und virtuellen Ordnern. Es unterstützt zusätzlich unübertroffene Erweiterbarkeit.
copy
file:///media/eppenich/FREECOM%20HDD/z/_A_O_Whois
AVerTV Volar Hybrid Q (H837)
H837
Conceptronic USB2.0 DVB-T CTVDIGRCU V3.0
https://linuxtv.org/wiki/index.php/AVerMedia
AVerMedia AVerTV DVB-T USB 2.0 A800
AVerMedia AVerTV AverTV Volar HD & HD PRO (A835)
AVerMedia AVerTV AverTV Volar HD & HD PRO (A835B)
AVerMedia AverTV Volar HD PRO A835B(1835)
AVerMedia AVerTV Volar Black HD (A850)
AVerMedia AVerTV Volar GPS 805 (A805)
Conceptronic USB2.0 DVB-T CTVDIGRCU V3.0 	? Yes, in kernel since 2.6.31
USB DVB-T TV fm Stick
AverTV Volar HD2
/home/eppenich/Bilder/Bildschirm—FOTO—VOM, 2018-03-20 12-39-22.png
/home/eppenich/Bilder/Bildschirm—FOTO—VOM, 2018-03-20 12-42-09.png
Freecom
Freecom rev 4 DVB-T USB 2.0 tuner
Pinnacle
Pinnacle 230100031 PCTV USB DVB-T Stick Freeview Digital TV Tuner
https://youtu.be/hxcZ5NwdEzs
Pinnacle 230100031 PCTV
kdiff3 und kompare
https://wiki.ubuntuusers.de/OCRFeeder/
9
https://wiki.ubuntuusers.de/PC-Direktverbindung_per_NETZ—WERK-Kabel/
https://wiki.ubuntuusers.de/PC-Direktverbindung_per_WLAN/
20180404             https://wiki.ubuntuusers.de/Bluetooth/Einrichtung/
20180404             eazykeyboard
20180404             https://wiki.ubuntuusers.de/PC-Direktverbindung_per_WLAN/
20180404             network-manager
20180404             https://wiki.ubuntuusers.de/NetworkManager/
20180404             https://wiki.ubuntuusers.de/PC-Direktverbindung_per_WLAN/
https://wiki.ubuntuusers.de/PCMan_File_Manager/Benutzerdefinierte_Aktionen/
https://wiki.ubuntuusers.de/Zeitgeist/
WÄHREND find und locate sich auf die Suche nach Dateien beschränken, kann grep die Inhalte von Textdateien auswerten.
https://wiki.ubuntuusers.de/grep/
https://wiki.ubuntuusers.de/Desktopsuchmaschinen/
Métamorphose2
Set date and time manually or get from system.
https://sourceforge.net/p/file-folder-ren/feature-requests/search/?q=%21status%3Awont-fix+%26%26+%21status%3Aclosed-invalid+%26%26+%21status%3Aclosed-rejected+%26%26+%21status%3Aclosed-out-of-date+%26%26+%21status%3Aclosed-accepted+%26%26+%21status%3Aclosed-works-for-me+%26%26+%21status%3Aclosed+%26%26+%21status%3Aclosed-duplicate+%26%26+%21status%3Aclosed-fixed
/home/eppenich/dwhelper
/home/eppenich/Dokumente/VIDEO_DOWNLOADHELPER
sudo add-apt-repository ppa:notepadqq-team/notepadqq
sudo apt-get update
sudo apt-get install ocrfeeder 
eppenich@LAP-Eppenich:~$ sudo apt-get install ocrfeeder 
Paketlisten werden gelesen... Fertig
Abhängigkeitsbaum wird aufgebaut.       
Statusinformationen werden eingelesen.... Fertig
Die folgenden Pakete wurden automatisch installiert und werden nicht mehr benötigt:
  libieee1284-3:i386 libpango1.0-0:i386 libpangox-1.0-0:i386 libpangoxft-1.0-0:i386 libwine libwine:i386 libxft2:i386
  linux-headers-4.13.0-21 linux-headers-4.13.0-21-generic linux-image-4.13.0-21-generic
  linux-image-extra-4.13.0-21-generic thunderbird-globalmenu:i386 wine32:i386 wine64
Verwenden Sie »sudo apt autoremove«, um sie zu entfernen.
Dash
https://wiki.ubuntuusers.de/OCRFeeder/#source-2
AVerTV Volar Hybrid Q (H837)
H837
Conceptronic USB2.0 DVB-T CTVDIGRCU V3.0
https://linuxtv.org/wiki/index.php/AVerMedia
AVerMedia AVerTV DVB-T USB 2.0 A800
AVerMedia AVerTV AverTV Volar HD & HD PRO (A835)
AVerMedia AVerTV AverTV Volar HD & HD PRO (A835B)
AVerMedia AverTV Volar HD PRO A835B(1835)
AVerMedia AVerTV Volar Black HD (A850)
AVerMedia AVerTV Volar GPS 805 (A805)
Conceptronic USB2.0 DVB-T CTVDIGRCU V3.0 	? Yes, in kernel since 2.6.31
USB DVB-T TV fm Stick
AverTV Volar HD2
/home/eppenich/Bilder/Bildschirm—FOTO—VOM, 2018-03-20 12-39-22.png
/home/eppenich/Bilder/Bildschirm—FOTO—VOM, 2018-03-20 12-42-09.png
Freecom
Freecom rev 4 DVB-T USB 2.0 tuner
Pinnacle
Pinnacle 230100031 PCTV USB DVB-T Stick Freeview Digital TV Tuner
https://youtu.be/hxcZ5NwdEzs
Pinnacle 230100031 PCTV
kdiff3 und kompare
https://wiki.ubuntuusers.de/OCRFeeder/
https://wiki.ubuntuusers.de/PC-Direktverbindung_per_NETZ—WERK-Kabel/
https://wiki.ubuntuusers.de/PC-Direktverbindung_per_WLAN/
https://wiki.ubuntuusers.de/PCMan_File_Manager/Benutzerdefinierte_Aktionen/
https://wiki.ubuntuusers.de/Zeitgeist/
WÄHREND find und locate sich auf die Suche nach Dateien beschränken, kann grep die Inhalte von Textdateien auswerten.
https://wiki.ubuntuusers.de/grep/
https://wiki.ubuntuusers.de/Desktopsuchmaschinen/
sudo apt-get install wine-stable
https://de.wikihow.com/Wine-unter-Ubuntu-installieren
20180310             ? https://help.ubuntu.com/community/Wine
20180310             ? http://wiki.winehq.org/FAQ
eazykeyboardSollte euch der Editor nicht zusagen, könnt ihr ihn mit wenigen Befehlen wieder deinstallieren. via
eazykeyboardsudo apt-get remove notepadqq
eazykeyboardsudo add-apt-repository --remove ppa:notepadqq-team/notepadqq
eazykeyboardUbuntu
eazykeyboardInstall via PPA
eazykeyboardPPA address: https://launchpad.net/~notepadqq-team/+archive/notepadqq
eazykeyboardTo install Notepadqq from Ubuntu, simply run the following commands in a terminal:
eazykeyboardsudo add-apt-repository ppa:notepadqq-team/notepadqq
eazykeyboardsudo apt-get update
eazykeyboardsudo apt-get install notepadqq
eazykeyboardhttps://notepadqq.com/wp/download/
20180315             digital linux
http://www.ntech.pt/
20180315             .ntech
20180315             Chipset Realtek RTL2832
https://www.linuxtv.org/wiki/index.php/RealTek_RTL2832U
20180315             RealTek RTL2832U
20180315             GENERAL Description
20180315             (from the specifications page at RealTek [1]) The RTL2832U is a high-performance DVB-T COFDM demodulator that supports a USB 2.0 interface. The RTL2832U complies with NorDig Unified 1.0.3, D-Book 5.0, and EN300 744 (ETSI Specification). It supports 2K or 8K mode with 6, 7, and 8MHz bandwidth. Modulation parameters, e.g., code rate, and guard interval, are automatically detected. It is sometimes identified as RTL2838.
20180315             Drivers
20180315             In Ubuntu 13.10 the 3.11 kernel is available with the dvb-usb-rtl28xxu driver out of the box. Another user has tested the stick with Ubuntu and OpenELEC distributions with kernel 3.14 and the device works out of the box ok.
20180315             Directions for installation are here: http://git.linuxtv.org/media_build.git
20180315             RealTek RTL2832U
https://linuxtv.org/wiki/index.php/DVB-T_USB_Devices
https://linuxtv.org/repo/
https://ubuntuforums.org/showthread.php?t=2239884
20180315             RTL2832U Drivers Download for
https://www.google.pt/url?sa=t&rct=j&q=&esrc=s&source=web&cd=10&cad=rja&uact=8&ved=0ahUKEwih2fW6wu_ZAhVGVBQKHQU_AKYQFgiKATAJ&url=https%3A%2F%2Fwww.scoop.it%2Ft%2Frealtek-rtl2832u-dvb-t-linux-driver-3%2Fp%2F4090696521%2F2017%2F12%2F13%2Frealtek-rtl2832u-dvb-t-linux-driver&usg=AOvVaw2Wrse_6tNBLvgOz6-eEhRV
20180315             PLACA TV DIGITAL NTECH LV5THD DONGLE HD E RÁDIO USB
20180315             Conversor TDT DVB-T LV5THD
20180315             Permite fazer visualização de TV em formato Digital no computador
20180315             Permite ouvir rádio no computador
20180315             IC compatível com SDR
20180315             Chipset Realtek RTL2832
http://exsite.pt/PLACA-TV-DIGITAL-NTECH-LV5THD-DONGLE-HD-RADIO-USB
http://www.openbricks.org/src/1.2.4/
https://ubuntuforums.org/showthread.php?t=1678094
https://www.scoop.it/t/realtek-rtl2832u-dvb-t-linux-driver-3/p/4090696521/2017/12/13/realtek-rtl2832u-dvb-t-linux-driver
http://relaws.ru/21?keyword=realtek-rtl2832u-dvb-t-linux-driver&charset=utf-8&source=scoop
https://www.google.pt/search?q=lv5thd&ie=utf-8&oe=utf-8&client=firefox-b&gfe_rd=cr&dcr=0&ei=m_2qWteHEfOs8weIwrqIDA
https://www.google.pt/search?q=lv5thd&client=firefox-b&dcr=0&ei=3P-qWpLGFcqsUc_MmagD&start=10&sa=N&biw=1146&bih=784
20180316            Supported Scanners - Search Engine
20180316            http://www.sane-project.org/cg1—bin/driver.pl
20180316            SANE - Scanner Access Now Easy
20180316            http://www.sane-project.org/
20180316            https://wiki.ubuntuusers.de/DVB-Karten/
20180316            DVB-Karten
20180316            https://wiki.ubuntuusers.de/DVB-Karten/
20180316            https://wiki.ubuntuusers.de/TV/
20180316            VDR
20180316            ./vdr.jpg Der VDR (Video Disc Recorder) von Klaus Schmidinger ist 1.SOFTWARE—FÜR—1 digitalen Videorekorder auf Linux-Basis. Neben der einfachen Aufzeichnung oder Wiedergabe von TV-Signalen enthält VDR auch DVB-Unterstützung.
20180316            DVB-T-Aufnahmen aus dem TV-Browser starten - Zeitge—STEUERt oder zum "automatischen"Einschalten von Sendungen
20180316            https://wiki.ubuntuusers.de/Skripte/DVB-T-Aufnahmen_aus_dem_TV-Browser_starten/
20180316            https://wiki.ubuntuusers.de/TV/
20180316            https://wiki.ubuntuusers.de/VLC/
20180311             kprobe FDC 
http://free-data-capture.software.informer.com/download/
20180311             A-Z Technology
20180311             A-Z Finder Private 1.08.120
http://www.freeware-archiv.de/download.php
20180311             eazykeyboard
https://code.google.com/archive/p/eazykeyboard/downloads
20180311             OnScreen Keyboard
https://launchpad.net/screenlets
20180311             If you are interested in individual screenlets not the framework itself, please refer to https://launchpad.net/indiv-screenlets.
20180311             sudo add-apt-repository ppa:noobslab/apps
20180311             sudo apt-get update
20180311             sudo apt-get install gis-weather
20180311             sudo add-apt-repository ppa:atareao/atareao
20180311             sudo apt-get update
20180311             sudo apt-get install my-weather-indicator
20180311             
ubuntu Clock Applet
20180322            /home/eppenich/Downloads/RADIX_KARL
20180322            printer_name=DeskJet_3630
20180322            https://duckduckgo.com/?q=ubuntu+printer_name%3DDeskJet_3632&t=canonical&atb=v107-7&ia=web
20180311             As long as you didn't tell the panel to "delete"the clock applet, you should be able to get it back with a simple restart of the gnome-panel itself. 
Just hit Alt-F2, then run :
killall gnome-panel
20180311             That will restart the panel and reload your clock.
20180311             If you've deleted the clock applet, you'll have to re-apply it. Right click on an empty area of your panel, right click and choose "Add to panel". Then find and choose the "Clock"applet, then hit the add button at the bottom.
20180311             If killall gnome-panel didn't work for you, that's because you're using a newer version of Ubuntu, running Unity. The command then should be
20180311             killall unity-panel-service
20180311             How do I reload the clock applet
https://wiki.ubuntuusers.de/Cairo-Clock/
20180311             Der eingeschränkte Funktionsumfang mag manchen verleiten, auf Ubuntu SOFTWARE zu verzichten und stattdessen das SOFTWARE-Center nachzuinstallieren. Da dieses aber nicht mehr weiterentwickelt wird, ist das keine gute Idee.
20180311             Eine einsteigerfreundliche Empfehlung fällt —DERZEIT, schwer (Stand: Mai 2016). Fortgeschrittene und Profis schwören —SCHON—SEIT längerer Zeit auf Synaptic oder verwenden gleich die Kommandozeile
(SIEHE Advanced Packaging Tool).
https://wiki.ubuntuusers.de/Synaptic/
20180311             Personal Package Archive - PPAs freischalten
https://wiki.ubuntuusers.de/Paketverwaltung/
20180311             apturl - Erweiterung für den Browser, mit der sich Programme via Browser bzw.  
Link installieren lassen
20180311             APT
20180311             Als grafischer Ersatz zur Installation von Fremdpaketen kann generell gdebi dienen.
20180311             Sie stellen ein Piconet dar (Personal Area Network), bei dem 1.Punkt-zu- Punkt-Verbindung besteht.
20180311             Untereinander identifizieren sich die Geräte per AMA (Active Member Address).
20180311             In der Regel lassen sich bis zu 8 Geräte aktiv miteinander verbinden. Dann spricht man von 1 Punkt-zu-Mehrpunkt-Verbindung.
20180311             Hier fungiert ein Gerät als Master, jedes andere als Slave. Außerdem können die Geräte im Piconet auch im passiven Modus verweilen. Hier sind sie zwar angemeldet, aber als Standby oder Parked im Bluetooth—NETZ gekennzeichnet. Deshalb erhalten sie die Adresse PMA (Passive Member Address). Da es sich um 1.8-Bit-Adresse handelt, können theoretisch bis zu 256 Geräte (2 hoch 8) im Standby-Modus verweilen. Sind mehrere Piconetze zusammengefasst, spricht man von Scatternetz. Hier muss mindestens ein Bluetooth-Gerät gemeinsam enthalten sein.
20180311             Um 2 Geräte per Bluetooth zu verbinden, müssen Sie die Funktion bei allen Geräten aktivieren. Der Pairingvorgang geht immer von 1 Gerät aus: am Smartphone wählen Sie das Gerät aus der Liste, die unter Einstellungen > Bluetooth erscheint. Vor dem eigentlichen Verbinden tauschen die Geräte 1 SICHERHEITS—codeaus, den Sie entweder nur bestätigen oder an 1 Gerät eingeben. Erst danach startet der Pairingprozess.
20180311             Bluetooth nutzt das ISM-Band (Industrial, Scientific and Medical Band)
20180311             Löschen Sie alte Koppelungseinträge aus der Bluetooth-Liste.
20180311             Allerdings ist das Einschalten von Bluetooth nur die halbe Miete, denn bevor 2 Geräte  über Bluetooth senden und empfangen können, müssen Sie die beiden miteinander koppeln (Pairing). Dazu müssen Sie Bluetooth auch am anderen Gerät einschalten. Aktivieren Sie dann den Menüeintrag zur Umgebungssuche, etwa Geräte suchen, Umgebungssuche, sichtbar oder detectable, damit das Gerät auf Bluetooth-Suchanfragen reagiert. Nun sucht Windows nach allen empfangsbereiten Bluetooth-Geräten, die sich in der Nähe befinden. Wurde keines gefunden, bringen Sie die beiden Geräte näher zusammen und wiederholen den Suchvorgang.
20180311             Markieren Sie das gefundene Gerät und geben Sie gegebenenfalls den auf dem Bildschirm des anderen Geräts angezeigten PIN-Code ein. Nach 1 kurzen Wartezeit meldet Windows, dass das neue Gerät verbunden wurde.
20180311             Möchten Sie unterwegs mit dem NoteBOOK—Ins INTERNET und ist kein WLAN-Hotspot verfügbar, ist Ihr Smartphone mit Bluetooth die willkommene Alternative. Dazu muss das Mobiltelefon die Funktion Tethering  also die Freigabe der INTERNET—VERBINDUNG  unterstützen. Und außerdem muss Tethering je nach Provider im Mobilfunkvertrag enthalten sein.
20180311             Hinter solchen Verbindungsproblemen steckt meistens 1.fehlende Authentifizierung. Damit 2 Bluetooth-Geräte  austauschen, muss immer ein 1. Kennenlernen stattfinden  das Pairing (Kopplung).
20180311             Dabei übermitteln beide Geräte die für die Bluetooth-Verschlüsselung zuständigen Anmeldedaten. Erst nach dem Pairing können beide miteinander kommunizieren, sofern mindestens ein korrespondierendes Bluetooth-Profil als Protokoll vorhanden ist. Durch die Unterstützung eines bestimmten Bluetooth-Profils zeigt ein Gerät seine Fähigkeiten bezüglich 1 bestimmten Aufgabenstellung, etwa Audioübermittlung, Drucken, Headset-Sprachverarbeitung oder abgleich. Es gibt mehrere Dutzend solcher Profile. Bluetooth-Geräte informieren sich beim Aufbau 1 Verbindung gegenseitig über die jeweils unterstützten Profile. Erst wenn sich beide auf ein bestimmtes Profil geeinigt haben, klappt DIE—ZUSAMMEN—ARBEIT. Gut: Für das Senden und Empfangen von Dateien wählt Windows automatisch DAS—RICHTIGE Profil aus.
20180311             Machen Sie zuerst das Gerät sichtbar, mit dem Sie sich verbinden wollen. Dann suchen Sie in der Umgebung nach verfügbaren Bluetooth-Geräten und wählen das Gewünschte aus. Auf beiden Geräten wird 1.PIN angezeigt, die Sie eintippen oder bestätigen müssen. DAS—PRINZIP ist unter allen Betriebssystemen gleich und erlaubt Verbindungen über alle Plattformen hinweg. Sie können auf die gleiche Weise  mit PCs unter Mac-OS X, Linux oder Windows und Smartphones mit Android oder Windows Phone (nicht jedoch iOS) austauschen.
20180311             Für mehr Komfort sorgt NFC (Near Field Communication). Sie halten dabei einfach Ihr Smartphone an die Lautsprecherbox, und die Verbindung wird automatisch hergestellt. NFC muss dazu auf dem Smartphone aktiviert sein.
20180311             Was per Bluetooth möglich ist, wird über Profile festgelegt. Es gibt knapp 50 Profildefinitionen, dazu kommen noch 6 ÜbertragungS—PROTOKOLLE. Wenn sich Geräte miteinander verbinden, tauschen sie Informationen über die jeweils vorhandene Profile aus. Abhängig davon stehen unterschiedliche Funktionen zur Verfügung. Für die Musikübertragung ist beispielsweise das Advanced Audio Distribution Profile (AD2P) zuständig, für Kopfhörer HSP (Headset Profile) und bei Druckern kommt HCRP (Hardcopy Cable Replacement Profile) zum Einsatz. Damit überhaupt 1.Verbindung möglich ist, sind GAP (Generic Access Profile) und SDAP (Service Discovery Application Profile) nötig.
20180311             Jedes Bluetooth-Gerät bietet abhängig von den jeweils vorhanden Profilen unterschiedliche Dienste an. Bei 1 Maus ist beispielsweise nur das Human Interface Device Profile (HID) erforderlich. Windows-PCs bieten mit Standard-Treibern meist nur den Dateitransfer an.
20180311             Es kann dann helfen, das Pairing bei beiden Geräten aufzuheben und erneut durchzuführen.
20180311             4. Treiber und Bluetooth unter Windows einrichten
20180311             Windows 7 und 8 erkennen viele Bluetooth-Adapter automatisch und richten den passenden Treiber ein. Dieser bietet jedoch meist nur Grundfunktionen für den Verbindungsaufbau und den transfer. Damit sich alle Funktionen nutzen lassen, installieren Sie das Treiberpaket des Adapter-oder PC—HERSTELLERs. In sehr vielen Geräten stecken Chips von Broadcom. Der Hersteller bietet ein Installationspaket für Windows XP, Vista, 7 und 8 an . Das Setup—PROGRAMM prüft zuerst, ob ein Broadcom-Chip vorhanden ist, lädt dann die passende SOFTWARE herunter und installiert sie. Danach müssen Sie Windows neu starten.
20180311             Treiber und Bluetooth-SOFTWARE gibt es außerdem von Intel, allerdings nur für eigene Geräte, etwa Intel NUC. Treiber für Notebooks mit Intel-Chipsatz erhalten Sie im Download-Bereich des Notebook—HERSTELLERs.
20180311             7. Zugriff auf NETZ—WERK-freigaben über Bluetooth
20180311             Es ist möglich, über Bluetooth direkt auf freigegebene Ordner eines anderen Windows-PCs zuzugreifen. Koppeln Sie die Geräte zuerst, wie unter Punkt 2 beschrieben. Beim PC, der über Bluetooth Zugang zu den Freigaben haben soll, trennen Sie die NETZ—WERKverbindungen über WLAN oder Ethernetkabel. Öffnen Sie in der SYSTEM—STEUERung Geräte und Drucker. Wählen Sie den PC aus, mit dem Sie sich verbinden möchten, und gehen Sie im Kontextmenü auf Verbindung herstellen über: > Direkte Verbindung. Ist die Verbindung aufgebaut, öffnen Sie den Windows-Explorer und gehen auf NETZ—WERK. Im oberen Bereich des Fensters erscheint DIE—MELDUNG NETZ—WERKerkennung ist deaktiviert. NETZ—WERKcomputer und -geräte sind nicht sichtbar. Klicken Sie hier, um dies zu ändern. Nach 1 Klick auf DIE—MELDUNG wählen Sie NETZ—WERKkennung und Dateifreigabe aktivieren. Es erscheint ein Fenster, in dem Sie auf Nein, das NETZ—WERK, zu dem die Verbindung besteht, zu 1 privaten NETZ—WERK machen klicken. Der andere PC und seine NETZ—WERKfreigaben sind jetzt im Windows-Explorer unterhalb von NETZ—WERK zu sehen.
pin 723983
20180311             bluetooth geräte verbinden
20180311             Treiber
20180311             Gelegentlich fehlt auch der geeignete Treiber, siehe dazu Linux-backports-modules. Möglicherweise fehlt aber auch nur die Firmware.
20180311             Konfiguration
20180311             Nach der Installation muss der Bluetooth-Dienst evtl. neu gestartet werden. Dies geschieht im Terminal [3] mit dem Befehl
20180311             sudo service bluetooth restart
20180311             bzw. mit
20180311             sudo /etc/init.d/bluetooth restart
20180311             Sind die benötigten Pakete installiert, wird beim Einstecken des Bluetooth-Dongles normalerweise automatisch das hcid (Host Controller Interface Device) gestartet. Dieses dient als Schnittstelle zum Bluetooth-Gerät. Informationen über das Bluetooth-Gerät erhält man mit dem Befehl:
20180311             hciconfig --all
20180311             Die Option --all sorgt dabei für 1.erweiterte Informationsausgabe. Zum Beispiel sieht die Ausgabe so aus:
https://wiki.ubuntuusers.de/Bluetooth/Einrichtung/
20180311             Verbindung mit dem Mobiltelefon
20180311             Beim Mobiltelefon muss man nun die Bluetooth-Menüpunkte durchgehen - diese sind bei jedem Gerät woanders untergebracht. Besonders wichtig ist, dass es auf "Sichtbar"eingestellt wird.
20180311             Wenn das Pairing von 1 Rechner unter Unity eingeleitet wird, muss im Mobiltelefon in der Einstellung Bluetooth der Unter-Menüpunkt "sichtbar"aktiv sein.
20180311             Im rechten Teil des Unity-Panel ist das Bluetooth-Symbol zu sehen. Nach dem Anklicken öffnet sich ein Fenster. In der untersten Zeile dieses Fenster muss das Feld "Bluetooth-Einstellungen..."aktiviert werden.
20180311             1 weiteres Fenster namens "Bluetooth"wird geöffnet. Im unteren rechten Teil befindet sich der Button + . Wird dieser Button betätigt, geht das Fenster "Suchen nach Geräten"auf, Im Feld Geräte erscheint das gefundene Mobiltelefon. Diese Zeile muss angeklickt werden und der Button "weiter"ist aktiviert. In der Standard-Einstellung wird 1.PIN automatisch generiert. Mit Betätigen des Buttons "weiter"wird diese sowohl auf dem Rechner als auch im Mobiltelefon angezeigt und muss auf beiden Geräten bestätigt werden.
https://wiki.ubuntuusers.de/Bluetooth/Einrichtung/
uart
bcsp
https://wiki.ubuntuusers.de/OCRFeeder/#source-2
New Plugin gets 'This ANSI plugin is not compatible with your Unicode Notepad++'
I’ve created a sample Plugin derived from NppPluginTemplate. Its compiled with Embarcadero’s C++ Builder as a 32 Bit application and with UNICODE. The function isUnicode() is build and exported from the DLL. But if i start Npp i get the messagebox:
This ANSI plugin is not compatible with your Unicode Notepad++
NppPluginDemo.dll is not compatible with the current version of Notepad++
Npp Debug Info is:
Notepad++ v7.5.4 (32-bit)
Build time : Jan 1 2018 - 01:47:45
Path : C:\Program Files (x86)\Notepad++\notepad++.exe
Admin mode : OFF
Local Conf mode : OFF
OS : Windows 10 (64-bit)
Plugins : ComparePlugin.dll DSpellCheck.dll mimeTools.dll NppConverter.dll NppExec.dll NppExport.dll NppFTP.dll NPPJSONViewer.dll NppTextFX.dll PluginManager.dll PyNPP.dll PythonScript.dll SourceCookifier.dll
https://notepad-plus-plus.org/community/search/ANSI?in=titlesposts&sortBy=timestamp&sortDirection=desc&showAs=posts
How can I use a function like "Encoding - Convert to ANSI"in my code?
I want to convert a UTF8 string to current —SYSTEM encoding, and “Encoding - Convert to ANSI” works perfect.
I’m trying to find how this function is implemented, but couldn’t find the file.
Is it in a part of github:src/WinControls/AnsiCharPanel? Or, reading which part of code may helps?
- SPIEGEL—ONLINE - Netzwelt
Druckversion -
20180326            Notepad++ v7.5.6   (32-bit)
20180326            Build time : Mar 19 2018 - 00:26:59
20180326            Path : C:\Program Files (x86)\Notepad++\notepad++.exe
20180326            Admin mode : ON
20180326            Local Conf mode : OFF
20180326            OS : Windows 7 (64-bit)
20180326            Plugins : DSpellCheck.dll mimeTools.dll NppConverter.dll NppExport.dll
Notepad++ 32-bit x86 ersetzen durch Notepad++ 64-bit x64
20180326            ANSI ist die Abkürzung für American National Standards Institute. Die Zeichencodes (ASCII, ANSI, Unicode) wurden eingeführt, als Computeranwender über DAS—INTERNET bzw. über verschiedene NETZ—WERKe kommunizieren konnten bzw. wollten.
20180326            kommunizieren konnten bzw. wollten.
20180326            bzw. MUSSTEN
20180326            Change file—SYSTEM encoding to ANSI in Ubuntu
Notepad++
Notepad++ 32-bit x86 ersetzen durch Notepad++ 64-bit x64
Once you have located your donwload:
- Click in your Download file!
- Follow the installer instructions.
file:///home/eppenich/Bilder/201601011231        /CdRsYZDUsAAHyh-.jpg%20orig.jpg
C:\Program Files\Notepad++
/home/eppenich/Downloads/plugins
/home/eppenich/Downloads/PluginManager_v1.4.9_x64.zip
Since Notepad++ Version 6 you can use this regex —IN—THE—search and replace dialogue:
^(.*?)$\s+?^(?=.*^\1$)
and replace with nothing.
 This leaves from all duplicate rows the last occurrence in the file.
No sorting is needed for that and the duplicate rows can be anywhere in the file!
You need to check the options "Regular expression"and ". matches newline":
^ matches the start of the line.
(.*?) matches any characters 0 or more times, but as few as possible 
(It matches exactly on row, this is needed because of the ". matches newline"option). 
The matched row is stored, because of the brackets around and accessible using \1$ matches the end of the line.
\s+?^ this part matches all whitespace characters (newlines!) till the start of the next row 
==> This removes the newlines after the matchd row, so that no empty row is there after the replacement.
(?=.*^\1$) this is a positive lookahead assertion. 
This is the important part in this regex, a row is only matched (and removed), when there is exactly the same row following somewhere else in the file.
https://stackoverflow.com/questions/3958350/removing-duplicate-rows-in-notepad
Notepad++
-> Replace window
Ensure that in Search Mode
you have selected Regular expression radio button
Find what:
^(.*)(\r?\n\1)+$
Replace with:
$1
before:
and we think there
single line
Is it possible to
after:
and we think there
single line
Is it possible to
^(.*)(\r?\n\1)+$
$1
Plugin Manager
tjis ansi plugin is not compatible with the current version of notepad++
libcurl.dll
feuerzeug
In the google search box you can type “plugin manager site:notepad-plus-plus.org” and that will get you started.
Once you get the plugin manager going, you can find the “compare” plugin and install it.
How to install?
Usually, the only installation procedure plugins require is to
place the dll in the plugins subfolder of the Notepad++ install folder;
place any configuration file it COMES with in plugin\config
preferrably, place all documentation files in plugin\doc, or in some subfolder of it
NppShell_06.dll
%APPDATA%\Notepad++\plugins
ANSI
----------------------------------------
TV Stick
Eletty USB2.0 DAB FM DVB-T RTL2832U Digital Tv Tuner RTL-SDR E4000 Upgrade Verion Dongle Tv Stick
Price: 	$12.22 + $1.49 shipping
In Stock.
This item does not ship to PORTUGAL. Please check other sellers who may ship internationally.
Ships from and sold by PSFS.
??Chip?R820T + RTL2832U chip.
??Supports ?SDR,DAB,FM,DVB-T, and Windows 2000 / XP / Vista / WIN7, both MPEG-2, MPEG-4 H.264 encoding.
??Functions?watch and record digital terrestrial TV on PC or Laptop, record and play digital TV as DVD quality, ?And also remote control.
??MHz?full DVB-T bandwidth reception (6/7/8 MHz).
??Remark?1. Confirm your local or local DVB-T signal. 2. UNITED—STATES and CANADA can not use the DVB-T function local without DVB-T signal, but the other functions could be used.
› See more product details
New (1) from $12.22 + $1.49 shipping
https://www.amazon.com/Ecloud-ShopUS-Flash-Drive-Player/dp/B00J5C6CR4/ref=sr_1_fkmr3_3?s=electronics&ie=UTF8&qid=1522746015&sr=1-3-fkmr3&keywords=usb+DTV-T%2C+fm%2C+Stick
AGPTEK U3 USB Stick Mp3 Player, 8GB Music Player Supports Replaceable Battery, Recording, FM Radio, Expandable Up to 64GB, Black
3.9 out of 5 stars 328 customer reviews
| 166 answered questions
Price: 	$24.99
10% off item with purchase of 1 items 9 Applicable Promotion(s)
In Stock.
This item ships to PORTUGAL. Want it Thursday,;;04;;5? Order within and choose AmazonGlobal Priority Shipping at checkout.  
Learn more
Sold by Linking Port and Fulfilled by Amazon. Gift-wrap available.
Color: U3 8GB
REPLACEABLE BATTERY: Never worried about no power, Replacing at any time with 1 AAA Battery(Not included).
USB DESIGN: No Cable needed, you can directly connect with PC to transfer files.USB 2.0 providing high speed transfer,Could be used as a flash drive
BIG Memory: 8 GB Memory capacity Stores up to 2000 songs; Supports up to 64 GB Micro SD Card (not included).
SIMPLE OPREATION: Support Music format: MP3/WMA, Playing modes: normal, shuffle (random), repeat .Support 7 equalizer and variable speed playback
MULTI-FUNCTION: With MP3, Recording and FM function. Easy and convenient.
New (1) from $24.99 & FREE shipping on orders over $25.00. Details
https://www.amazon.com/AGPTEK-Supports-Replaceable-Recording-Expandable/dp/B01NAJ3KQB/ref=pd_bxgy_147_2?_encoding=UTF8&pd_rd_i=B01NAJ3KQB&pd_rd_r=S1P7MJB1A9V2K2P1G7X0&pd_rd_w=vzSQ6&pd_rd_wg=LwJyz&psc=1&refRID=S1P7MJB1A9V2K2P1G7X0
Adafruit (PID 1497) SOFTWARE Defined Radio Receiver USB Stick - RTL2832 w/R820T
---------------------------------------------------
Plugin Config path is:
C:\users\eppenich\Application Data\Notepad++\plugins\Config
Plug-ins in user's AppData directory are disabled 
- to enable in Notepad++ version 5.9.7 onwards
 place an empty file called 
allowAppDataPlugins.xml
 in the Notepad++ directory.
-------------------------------
Plugin Config path is:
C:\users\eppenich\Application Data\Notepad++\plugins\Config
Plugins in user's AppData directory are enabled. 
Remove the allowAppDataPlugins.xml file from the Notepad++ directory to disable.
------------------------------------
lte/4g modul qualcomm em7305
ubuntu
Linux SDK
Setting up a
Configure Cellular Connections
Check whether a modem was properly detected via:
https://docs.ubuntu.com/core/en/stacks/network/network-manager/docs/configure-cellular-connections
Exploring Network Status
This section shows how to use the nmcli command-line tool to examine the status of NetworkManager?s connections and devices.
Show the status of devices known to NetworkManager:
$ nmcli d
Show more information for this option:
$ nmcli d --help
Show the current status of each of NetworkManager?s connections:
$ nmcli c
Command ?c? is for connections but is a abbreviated form of the real command "connections". As for the devices command, ?--help? shows more information for this option. Finally, we can see THE—STATE—OF—radio interfaces, including WiFi and WWAN (cellular) with:
$ nmcli r
WIFI-HW  WIFI     WWAN-HW  WWAN
enabled  enabled  enabled  enabled
It is important to make sure that WiFi/WWAN radios are enabled so the respective connection types can establish a connection (we will specify how to this in following sections). As with the other commands, ?--help? shows usage information.
Observe NetworkManage activity (changes in connectivity state, devices or connection properties):
$ nmcli monitor
See nmcli connection monitor and nmcli device monito
https://docs.ubuntu.com/core/en/stacks/network/network-manager/docs/explore-network-status
Setting up a Huawei E3276—150 4G/LTE USB modem on Ubuntu Server/Desktop
https://trick77.com/setting-up-huawe1—e3276—150-4g-lte-usb-modem-ubuntu-server-desktop/
Or from the command line:
nmcli connection show
Find your broadband entry on the list,
 let's say it's "My Broadband", then delete it with this:
nmcli connection delete "My Broadband"
1
down vote
accepted
You can launch another GUI connection manager by running the following command in Terminal
nm-connection-editor
Once the window appears, select the connection you want to remove and delete it by clicking on the "-"(minus) symbol.
https://open-cells.com/index.php/blog/
All in one OpenAirInterface, ;;08;; 22nd
https://open-cells.com/index.php/blog/
This document explains how to install and configure OAI EPC+eNB on one single Ubuntu 17.04 64 bits machine connected with a regular UE, routing the UE traffic to internet.
https://forum.ubuntuusers.de/topic/sierra-wireless-em7305-zum-laufen-bringen/
Nur fürs Protokoll und evtl. andere, der Thread hat mir geholfen..
selbiges EM7305 mit Mint 18.2 (= 16.04 LTS) in 1 Fujitsu E736: ging garnichts, erst nach FIRMWARE-Update des LTE-Modems (musste ich nativ unter Win10 machen) ging es auf Anhieb
Code:
usb-devices
The drivers have loaded for the device,
need to see if device will list by-id
from the teminal
Code:
ls -al /dev/serial/by-id
cinnamon desktop
20180408            https://www.google.pt/search?client=firefox-b&dcr=0&q=ubuntu+network+manager+restart&sa=X&ved=0ahUKEwjDhsjLo6vaAhWEWBQKHbErA2oQ1QIIdCgG&biw=829&bih=733
lte/4g modul qualcomm em7305
20180407            SIM-Card
20180407            https://askubuntu.com/questions/747959/sierra-e7455-mobile-broadband-modem
20180407            https://forums.lenovo.com/t5/Linux-Discussion/ThinkPad-X1-Yoga-LTE-Sierra-EM7455-on-Linux-Ubuntu—16-04/td-p/3344299/highlight/true
20180407            1
20180407            down vote
20180407            After doing what @zanna describes, 
you still need to do the following for network manager to get an IP address.
20180407            in terminal sudo rfkill unblock wwan
20180407             Enable broadBAND—In network manager 
(you need to do this because it sends the magic packet to bring the EM7455 out of low-power state)
20180407            watch syslog - after a few seconds it will fail.
20180407            in terminal sudo mbim-network /dev/cdc-wdm1 start
20180407            watch syslog, it will succeed, but you won't have an IP address.
20180407            in terminal sudo mbim-network /dev/cdc-wdm1 stop
20180407             Enable broadBAND—In network manager
20180407            and it works!
20180407            note your modem might be /dev/cdc-wdm0 or some other integer
20180407            Long-term evolution (LTE), also known as 4G,
20180407            Sierra Wireless EM7305
20180407            Article Number: 10217
20180407            Supplier number: 1102572
20180407            The Sierra Wireless EM7305 Embedded Module is an M.2 modem that provides LTE, DC-HSPA+, HSPA+, HSDPA, HSUPA, WCDMA, GSM, GPRS, EDGE, and GNSS connectivity for notebook, ultrabook, and tablet computers over several radio frequency bands. 
The device also supports 2G / 3G roaming.
20180407            https://techship.com/products/sierra-wireless-em7305/
20180407            AirPrime Module 	Region (Carrier) 	Bands 	Fallback
20180407             EM7305 	EMEA/Australia (Orange, Telefonica, Telstra, Vodafone) 	LTE: B1, B3, B7, B8, B20 	2G, 3G 	Technical Specs
20180407            https://www.sierrawireless.com/products-and-solutions/embedded-solutions/networking-modules/
20180407            
https://forum.ubuntuusers.de/topic/mobils-breitband-unter-ubuntu—16-04-lts-sierra/
cinnamon desktop
nm-applet
Verbindungs—MANAGER
sudo apt-get install usb-modeswitch usb-modeswitch-data
20180408            nmcli device
20180408            lspci
20180408            lsusb
20180408            sudo apt-get install network-manager
20180408            Kindprozess »/snap/bin/network-manager.networkmanager« konnte nicht ausgeführt werden (Datei oder Verzeichnis nicht gefunden)
20180408            https://www.computersnyou.com/4981/how-to-reinstall-ubuntu-without-losing-data/
wget -q -O - https://dl.google.com/linux/linux_signing_key.pub | sudo apt-key add -
sudo sh -c 'echo "deb http://dl.google.com/linux/earth/deb/ stable main">> /etc/apt/sources.list.d/google-earth.list'
20180411             Synaptic Package Manager
20180411             google-earth
20180411             wget -q -O - https://dl.google.com/linux/linux_signing_key.pub | sudo apt-key add -
20180411             sudo sh -c 'echo "deb http://dl.google.com/linux/earth/deb/ stable main">> /etc/apt/sources.list.d/google-earth.list'
20180411             Synaptic Package Manager
20180411             pkexec synaptic
20180411             sudo apt-get install synaptic
20180411             1.5 If there is any contradiction between what the Additional Terms say and what the Universal Terms say, then the Additional Terms shall take precedence in relation to that Service.
20180411             3.2 If there is any contradiction between what THE—ENGLISH language version of the Terms says and what a translation says, then THE—ENGLISH language version shall take precedence.
20180411             You acknowledge and agree that the form and nature of the Services which Google provides may change from time to time without prior notice to you.
20180411             4.4 You acknowledge and agree that if Google disables access to your account, you may be prevented from accessing the Services, your account details or any files or other content which is contained in your account.
20180411             5.3 Unless you have been specifically permitted to do so in a separate agreement with Google, you agree that you will not reproduce, duplicate, copy, sell, trade or resell the Services for any purpose.
20180411             6.2 You agree to THE—USE—OF—your data in accordance with Google’s privacy policies.
20180411             You may not modify, rent, lease, loan, sell, distribute or create derivative works based on this Content (either in whole or in part) unless you have been specifically told that you may do so by Google or by THE—OWNERS—OF—that Content, in a separate agreement.
20180411             19.5 If any COURT—OF—law, having the jurisdiction to decide on this matter, rules that any provision of these Terms is invalid, then that provision will be removed from the Terms without affecting the rest of the Terms. The remaining provisions of the Terms will continue to be valid and enforceable.
20121113             Connect to mobile broadband
You can set up a connection to a cellular (3G) network with your computer’s built-in 3G modem, 
your mobile phone, or an INTERNET stick.
           IF YOU DO NOT HAVE A BUILT-IN 3G MODEM, connect your phone or INTERNET stick to a USB port on your computer.
20121113             Open THE—SYSTEM menu from the right side of the top bar.
20121113             Select Mobile Broadband Off. The Mobile Broadband section of the menu will expand.
20121113             If Mobile Broadband does not appear IN—THE—SYSTEM status menu, ensure that your device is not set to connect as Mass Storage.
https://itsfoss.com/share-folders-local-network-ubuntu-windows/
https://appuals.com/ubuntu—16-04-to—17—10-wif1—and-ethernet—Problem/
20121113             If you’re on a fresh install of Ubuntu, like if you just upgraded from 16.04 to 17.10, you may very well likely be affected by the ‘random MAC address’ bug that has been reported by many users (and the Ubuntu developers are certainly aware of it). Alternatively, you may be effected by a driver issue (very common, and certain Realtek-based wifi adapters are notoriously more difficult than others).
20121113             press CTRL + ALT + T to open the terminal.
20121113             sudogedit /etc/NetworkManager/NetworkManager.conf
20121113             TETHERING
20121113             Tethering, or phone-as-modem, is the sharing of a mobile device's internet connection with other connected computers. 
Connection of a mobile device with other devices can be done over wireless LAN, over Bluetooth or by physical connection using a cable, for example through USB.
20121113             Tethering - Wikipedia
20121113             Tethering, or phone-as-modem (PAM), is the sharing of a mobile device's internet connection with other connected computers. 
Connection of a mobile device with other devices can be done over wireless LAN (), over Bluetooth or by physical connection using a cable, for example through USB.
20121113             [Search domain en.wikipedia.org] https://en.wikipedia.org/wiki/Tethering
https://en.wikipedia.org/wiki/Tethering
20121113             service network-manager restart
20121113             So I kept googling for stuff like ‘network manager shows as disconnected but browser has internet access’ and a lot of variations of the same thing. It was only until about 20 mins that it occurred to me to look for the ‘device not managed’ error.
https://www.blackmoreops.com/2013/11/25/how-to-fix-wired-network-interface-device-not-managed-error/
20121113             ‘device not managed’ error.
20121113             I get permission denied on /etc/NetworkManager/NetworkManager.conf and /etc/network/interfaces.
https://www.blackmoreops.com/2013/11/25/how-to-fix-wired-network-interface-device-not-managed-error/
20121113             So let’s start with the basics .. what is a PCI device…
20121113             What is Peripheral Component Interconnect or PCI?
https://www.blackmoreops.com/2014/08/20/identify-pc1—usb-wired-wireless-driver-linux-identify-pc1—driver/
20121113             Typical PCI cards used in PCs include: network cards, sound cards, modems, extra ports such as USB or serial, TV tuner cards and disk controllers.
20121113             PCI video cards replaced ISA and VESA cards until growing bandwidth requirements outgrew the capabilities of PCI. The preferred interface for video cards then became AGP, itself a superset of CONVENTIONal PCI, before giving way to PCI Express.
20121113             An internal connector for laptop cards, called Mini PCI, was introduced in version 2.2 of the PCI specification. The PCI bus was also adopted for an external laptop connector standard—the CardBus. The 1. PCI specification was developed by Intel, but subsequent development of the —STANDARD became the responsibility of the PCI Special Interest Group (PCI-SIG).
20121113             Many kinds of devices previously available on PCI expansion cards are now commonly integrated onto motherboards or available in universal serial bus and PCI Express versions. Source: Wikipedia
http://en.wikipedia.org/wiki/Peripheral_Component_Interconnect
20121113             Question: How do I identify PCI driver for anything in Linux?
20121113             Identify PCI Driver Chipset Information in Linux
20121113             lspci which is a —STANDARD command in all Linux distribution will show you the PCI devices on your system.
20121113             LS = List
20121113             PCI = Peripheral Component Interconnect devices
20121113             Step 1: List all PCI devices – Identify PCI driver
https://www.blackmoreops.com/2014/08/20/identify-pc1—usb-wired-wireless-driver-linux-identify-pc1—driver/
20180412             —ON, screen keyboard
20180412             virtual keyboard
20180412             ACPI Hot Plug PCI Controller Driver
20180412             PCIeHotplug PME AER PCIeCapability
20180412             ubuntu 17.1 internes 3-G modem aktivieren
20180412             https://www.vodafone.de/downloadarea/VMB_Anleitung.pdf
20180412             lte/4g modul
20180412             Laptop mit 1 integrierten LTE-Modem
20180412             Abhängig von dem Gerät, das Sie mit Vodafone Mobile Connect verwenden möchten, benötigen Sie außerdem:
20180412             \u2022 1 Computer mit integrierter Datenkarte
20180412             2. Installation
20180412             Auf den nachfolgenden Seiten finden Sie die Anleitungen zur Installation der Vodafone Mobile Broadband-Soft-
20180412             ware für Embedded Notebooks, Vodafone Mobile Connect Card und Vodafone Mobile Connect USB Stick.
20180412             2.1 Embedded Notebooks
20180412             1)
20180412             SIM Karte in Ihr Notebook einlegen
20180412             \u2022 Schließen Sie alle Anwendungen und fahren Sie Ihren Rechner runter.
20180412             \u2022 Lösen Sie alle Kabel von Ihrem Rechner.
20180412             \u2022 Schließen Sie das Display Ihres Rechners, drehen Sie Ihren Rechner um
20180412             und öffnen Sie das Batteriefach. Entnehmen Sie den Akku.
20180412             \u2022 Entnehmen Sie der Dokumentation Ihres Notebooks, wo sich der
20180412             Schacht für die SIM-Karte genau befindet, und legen die die SIM-Karte ein.
20180412             2)
20180412             Integrierte Datenkarte aktivieren
20180412             Notebooks mit integriertem UMTS Broadband haben oft 1 separaten Schalter, über den die Dat
20180412             2)
20180412             Integrierte Datenkarte aktivieren
20180412             Notebooks mit integriertem UMTS Broadband haben oft 1 separaten Schalter,
 über den DIE—DATENkarte aktiviert oder deaktiviert werden kann. 
 Stellen Sie sicher, dass die interne Datenkarte aktiviert ist.
20180412             3)
20180412             SOFTWARE installieren
20180412             \u2022 Legen Sie die CD in Ihren Rechner ein. Der Set-up-Assistent wird automatisch gestartet. Folgen Sie den
20180412             Schritten des Assistenten.
20180412             \u2022 Die Installation kann einige Minuten dauern. Nach der erfolgreichen Installation starten Sie den Rechner bitte
20180412             neu.
20180412             \u2022 Die Installation ist erfolgreich abgeschlossen. Jetzt können Sie Ihr mobiles INTERNET nutzen.
20180412             Hinweis: Notebooks mit bereits installierter Verbindungssoftware
20180412             Sofern auf Ihrem Notebook bereits 1.Verbindungssoftware installiert wurde, vergewissern Sie sich, dass der
20180412             richtige Zugangspunkt (APN = Access Point Name) hinterlegt wurde.
 Für die Nutzung von Vodafone WebSessions lautet dieser APN: \u201eevent.vodafone.de\u201c.
 Für die Nutzung mit 1 Vodafone—DATENvertrag lautet der APN: \u201eweb.
20180412             vodafone.de\u201d
20180412             Diese Einstellung findet man oft unter der Rubrik \u201eEinstellungen\u201c oder \u201eExtras\u201c der Verbindungs-
20180412             software.
20180412             ttyUSB2
20180412            notebook lte/4g modul
 integriert sim einlegen
20180414             Smart Cards (auch Chipkarte oder Integrated Circuit Card genannt),
20180414             lsusb
20180414             pcsc_scan
20180416             vodafone-mobile-connect-card-driver-for-linux
20180416             uname -sr
20180416             groups
20180416             addgroup
20180416    XXXXXXXXXXXXXXXXXXXXXXXXXXXXXXX         vodafone-mobile-connect-card-driver-for-linux
20180416             Notebooks mit UMTS Broadband
20180416             BUILT-IN 3G MOBILE BROADBAND FROM VODAFONE PRODUCT 
–  THE—DATA service, provided by Vodafone to enable the Customer to do any or all of the following,
 using one or more of the Bearer Services: 
 communicate between devices and/or people; 
 acquire and/or exchange information; 
 provide and/or receive entertainment; analyse data;
20180416             
https://www.vodafone.co.uk/terms-and-conditions/consumer/mobile/mobile-broadband/laptops-with-builtin-3g/
20180416             3. USE OF THE BUILT-IN 3G MOBILE BROADBAND FROM VODAFONE PRODUCT
20180416             Broadband Wireless notebook
20180416             Broadband Wireless
20180416             integrated wireless WAN capabilities
https://www.youtube.com/embed/tFFNiMV27VY?version=3&rel=1&fs=1&autohide=2&showsearch=0&showinfo=1&iv_load_policy=1&wmode=transparent
20180206             LGA 1151 	Intel H110
20180206             Rufus 2.18
https://rufus.akeo.ie/
20180206             Erstelle bootbare USB-Laufwerke auf einfache Art und Weise
20180206             Der Sockel 1151 ist ein Prozessorsockel für Desktop—PROZESSoren mit Skylake-, Kaby-Lake— , Coffee-Lake-Mikroarchitektur. 
Wikipedia
20180206             Prozessoren: Skylake, Kaby-Lake, Coffee-Lake
20180206             Einführung: August 2015
terra mobile industry 1582 motherboards
20180206             If having a spare USB drive, use an utility (ex: Rufus) for making it bootable, and 
see if the computer does boot from it.
20180206             I have no problem accessing the BIOS. 
I am using F2 and it works fine. 
I can even access the BIOS through the new Windows 8 process (more complex than necessary).
20180206             The problem is: 
the computer will not recognize the bootable USB or the bootable CD. 
I have changed the option in the BIOS to boot from THE—USB port, but 
it doesn't.
 There is no option to allow me to boot from the CD. 
I have no idea why not. 
Not sure if this is an ASUS hardware problem or a BIOS problem. 
As I mentioned, 
THE—USB thumb drive and the CD worked on another computer. 
Just not this ASUS: MB Ver Q500A-BHI7T05; Check #8147.
20180206             You have to Enable the "Launch CSM"option in Boot section of Bios. 
CSM means the Compatibility Support Module. 
Without this you can boot only UEFI mode. 
Windows 8 in UEFI mode receive serial key from BIOS. 
Windows 7 in UEFI mode can not boot in my case.
20180206             Conclusion
20180206             If you want to install any new OS to your PC or Laptop with UEFI Bios just turn off Security Boot and turn on Launch CSM option.
 Try these options if your OS installer does not boot.
 This method also works with Windows XP CD and Linux CD/USB Flash.
20180206             —See more at: http://bitprison.net/UEFI-BIOS-Windows-7-install#commen...
http://bitprison.net/UEFI-BIOS-Windows-7-install#comment-53519
20180206             "Launch CSM"is greyed-out, it seems by default.
20180206             The only way I could get it enabled was to 1. Disable Secure Boot Control.
20180206             Therefore, the correct order is:
20180206             1. Enter the BIOS setup menu by pressing and holding the F2 key, when powering on.
20180206             2. Switch to “Security” and set “Secure Boot Control” to Disabled.
20180206             3. Switch to “Boot” and set “Launch CSM” to Enabled.
20180206             4. Press F10 to save and exit.
20180206             5. Press and hold ESC key to launch boot menu when the Unit restarts.
20180206             To boot from the DVD, press and hold the ESC key and the boot menu will appear.
http://www.tomsguide.com/answers/id—1973164/change-asus-boot-order.html
20180206             Leagcy CSM schaltet Secure Boot ab und sorgt für Abwärtskompatibilität.
20180206             5. Hybrid image confirmation
20180206             Leave all other parameters with their default values and click Start to initiate the write process.
20180206             You will then be alerted that Rufus has detected that the Ubuntu ISO is an ISOHybrid image. 
This means the same image file can be used as THE—SOURCE for both a DVD and a USB stick without requiring conversion.
20180206             Keep Write in ISO Image mode selected and click on OK to continue.
20180206             The —STANDARD Ubuntu Cd can be used as a LiveCd as well as an installer.  
Live mode is the default option when booting from CD.
https://help.ubuntu.com/community/LiveCD?ACTION=show&redirect=LiveCd
20180206             What s PCI LAN: IBA GE SLOT 0008 v1336?
20180206             ?10-08—2010 02:30 AM
20180206             Hello,
20180206             In BIOS boot priority I can see this device as selectable, but I don't know what it is physically.
20180206             Maybe is Express card slot?!
20180206             That's the Ethernet port. 
It appear—IN—THE—S Boot priority order for booting over your network.
20180206             Re: What s PCI LAN: IBA GE SLOT 0008 v1336?
20180206             For an optimized installation (and especially for those wishing to run more than ~3 GiB of RAM) however, a 64-bit installation CD is available.
20180207             Secure Boot
20180207             Secure Boot ist 1.(U)EFI—FUNKTION ab Version 2.3.1 und nun schon auf vielen Mainboards anzutreffen.
20180207             Secure Boot soll per Definition den Start von Schadsoftware verhindern, 
blockiert aber auch das Booten vieler USB-Sticks oder optischer Medien und somit
 auch die Installation anderer Betriebssysteme.
20180207             Microsoft schreibt zwar vor, dass man die Option secure-boot auf normalen x86-PCs und -Notebooks abschalten kann, aber 
dazu ist je nach Hersteller - sowohl Hardware als auch Firmware - ein Ausflug ins BIOS - beziehungsweise UEFI-Setup unabdingbar.
20180207             "Secure Boot Mode"
20180207             Die Option "Standard"stellt in der Regel nur den vom Microsoft dem Board—HERSTELLER zur Verfügung gestellte Signatur bereit.
20180207             Die Option "Custom"lässt bei der AMI-EFI-Firmware die Benutzung von nicht in der Firmware hinterlegten Signaturen zu.
20180207             Abfrage unter Windows
20180207             Ob das secure-boot aktiviert ist oder nicht, kann man auch im Windows abfragen.
 Der Schlüssel in der
20180207             "Registry"--> "HKLM\SYSTEM\CurrentControlSet\Control\SecureBoot\State"
20180207             Wert 1: Aktiviert
20180207             Wert 0: Abgeschaltet
20180207             informiert über den momentanen Zustand.
20180207             Wenn Secure Boot aktivert wurde, 
ist der Modus "Compatibility Support Module"kurz CSM (frei übersetzt = BIOS-Kompatibilitäts-Modus) in der Regel nicht verfügbar.
https://wiki.ubuntuusers.de/EFI_GRUND—LAGEn/
20180207             Im CSM-Modus verhält sich DAS—SYSTEM - was Start und Installation anbelangt - dann so, 
wie man es von 1 reinen BIOS-SYSTEM gewohnt ist.
20180207             Die Aktivierung des CSM-Modus zwingt den Anwender aber auch dazu, 
sich beim Start eines Start-trägers für 1 der 2 Modi (UEFI oder Legacy) im EFI Menü zu entscheiden.
20180207             Installations-Medien
20180207             Unabdingbar ist das Vorhandensein eines ISO mit 64-Bit—ARCHITEKTUR ab der Version Precise Pangolin (12.04.2 LTS).
20180207             1 herunter geladenes ISO brennt man wegen seiner Größe (in der Regel > 800 MB) auf 1.DVD und benutzt diese DVD zum Installieren.
HKLM\SYSTEM\CurrentControlSet\Control\SecureBoot\State
bug: unable to handle kernel paging request
Ob DAS—SYSTEM im BIOS oder im EFI/UEFI gestartet wurde,
 kann man sich im LIVESYSTEM im Terminal anzeigen lassen mit:
[ -d /sys/firmware/efi ] && echo UEFI || echo BIOS
https://wiki.ubuntuusers.de/EFI_GRUND—LAGEn/#EFI-Bootverzeichnis
https://wiki.ubuntuusers.de/EFI_USB-Stick/
Terminal
IF UBUNTU IS THE ONLY OPERATING SYSTEM ON YOUR COMPUTER, THEN
 IT DOES NOT MATTER WHETHER YOU INSTALL UBUNTU IN UEFI MODE OR NOT.
https://help.ubuntu.com/community/UEFI
https://help.ubuntu.com/community/UEFI#Identifying_if_the_computer_boots_the_HDD_in_EFI_mode
Set up the firmware in UEFI or BIOS/CSM/Legacy mode
Some recent computers (>2011)
 allow you to set up the computer to boot either in UEFI mode or in BIOS/CSM/Legacy (not-EFI) mode. 
The way to adjust this setting depends on the computers, but 
generally this setting is located in the "Boot order"tab of the BIOS
 (to access the BIOS screens, it is generally necessary to press a key during the PC startup). 
It can also often be set on a per-boot basis by
 hitting a function key (F8 and F10 are common choices) soon after you power on the computer.
NOTE: 
SOME UEFIs (e.g. AMERICAN MEGATRENDS' "APTIO", 
found on the Asus vivobook series) 
CALL LEGACY MODE "COMPATIBILITY SUPPORT MODULE"OR SIMPLY 
"CSM".
Performing the Installation
Once you've taken care of the preliminaries,
 you can install Ubuntu normally.
 Aside from the ESP, 
Ubuntu installed in UEFI mode 
has no special partition requirements, and
 you need not adjust other installation options. 
Note that in a UEFI-mode installation,
 Ubuntu will not ask you where to install the boot loader. 
If it does, or 
if it complains about the lack of a BIOS Boot Partition, 
you've probably accidentally booted in BIOS/CSM/legacy mode.
https://help.ubuntu.com/community/UEFI#Identifying_if_the_computer_boots_the_HDD_in_EFI_mode
Installing Ubuntu for Single Boot with a Random Boot Mode
IF YOU AREN'T MULTI-BOOTING WITH ANOTHER OS AND 
YOU DON'T CARE ABOUT YOUR BOOT MODE, 
YOU CAN FOREGO SOME OF THE PICKY DETAILS OF THE PRECEDING PROCEDURE AND
 INSTALL UBUNTU IN WHATEVER BOOT MODE YOUR COMPUTER HAPPENS TO PICK
If the PC does not load Ubuntu, 
boot your PC using the Live CD/DVD or Live USB and 
choose "Try Ubuntu"once AGAIN. 
When the live session has loaded,
 run Boot-Repair (see link for details). 
When Boot-Repair loads, 
click on the "Recommended repair"button, and
 write on a paper the URL (paste.ubuntu.com/XXXXXX/) that will appear. 
Then reboot the computer. 
DO NOT RUN BOOT-REPAIR UNLESS YOU HAVE PROBLEMS BOOTING THE COMPUTER; the expression "if it ain't broke, don't fix it"applies to this tool.
https://help.ubuntu.com/community/Boot-Repair
Boot-Repair lets you fix these issues with a simple click, which (generally reinstalls GRUB and) restores access to the operating systems you had installed before the issue.
instaler failed 
Fehlerhafte Implementationen von UEFI haben bei mehreren Herstellern zu irreparablen Schäden an SYSTEMen geführt.
20130600             —IM, wurden Notebooks von Samsung beim Bootvorgang mit Linux eingefroren, SOBALD DAS BETRIEBSSYSTEM SCHREIBEND AUF DIE UEFI-FIRMWARE ZUGRIFF. 
20130600             —IM, Das Mainboard wurde dadurch unlösbar blockiert.[27] 
ANFANG 2014 trat das gleiche Problem bei Geräten von Lenovo auf und
ENDE 2015 bei Geräten von Asus.[28][29]
https://de.wikipedia.org/wiki/Unified_Extensible_Firmware_Interface
20180211             LIVESYSTEM
20180211             Terminal
20180211             Boot-Repair
https://sourceforge.net/u/yannubuntu/profile/
https://sourceforge.net/p/os-uninstaller/
https://sourceforge.net/p/boot-info/
https://sourceforge.net/p/boot-repair/
https://sourceforge.net/p/boot-repair-cd/
20180211             When the bootloader (GRUB) is broken, I cannot access neither Ubuntu nor Windows.
20180211             I heard that an easy solution to fix this is to use the Boot-Repair tool from an Ubuntu liveCD (or liveUSB).
20180211             What are the steps to do this?
https://askubuntu.com/questions/226061/how-to-install-the-boot-repair-tool-in-an-ubuntu-live-disc
20180211             Connect to THE—INTERNET, then open a terminal with Ctrl+Alt+t, paste the following commands and run them by pressing Enter:
20180211             sudo apt install software-properties-common; \
20180211             sudo add-apt-repository -y ppa:yannubuntu/boot-repair; \
20180211             sudo apt-get update; \
20180211             sudo apt-get install -y boot-repair && boot-repair
20180211             Note: You copy and run them all at once. If you want to run them individually just remove the trailing "; \".
20180211             That's it, the Boot-Repair window will appear!
20180211             accepted
20180211             What is it:
20180211             The terminal is an interface in which you can type and execute text based commands.
20180211             Alternative names for the terminal:
20180211             Console
20180211             SHELL
20180211             Command Line
20180211             Command Prompt
20180211             You can open it via the utilities part of the apllications menu, or press Alt+F2 and type gnome-terminal.
20180211             You can start the terminal from Applications -> Accessories -> Terminal.
https://help.ubuntu.com/community/UsingTheTerminal
20180211             The traditional Unix environment is a CLI (command line interface), 
where you type commands to tell the computer what to do. 
That is faster and more powerful, but requires finding out what the commands are."
20180211             The easiest way to open the terminal is to use the 'search' function on the dash.
20180211             Or you can click on the 'More Apps' button, click on the 'See more results' by the installed section, and find it in that list of applications.
20180211             A third way, available after you click on the 'More Apps' button, is to go to the search bar, and see that the far right end of it says 'All Applications'.
20180211             You then click on that, and you'll see the full list.
20180211             —THEN, you can go to Accessories -> Terminal after that. So, the methods in Unity are:
20180211             Dash -> Search for Terminal
20180211             Dash -> More Apps -> 'See More Results' -> Terminal
20180211             Dash -> More Apps -> Accessories -> Terminal
20180211             Keyboard Shortcut: Ctrl + Alt + T
20180211             sudo: Executing Commands with Administrative Privileges
20180211             The sudo command executes a command with administrative privileges (root-user administrative level), 
which is necessary, for example, when working with directories or files not owned by your user account.
When using sudo you will be prompted for your password.
 Only users with administrative privileges are allowed to use sudo.
20180211             Be careful when executing commands with administrative privileges 
- you might damage your system! 
You should never use normal sudo to start graphical applications with administrative privileges.
 Please see RootSudo for more information on using sudo correctly.
https://help.ubuntu.com/community/RootSudo
20180211             ctrl+shift+V pastes into a GNOME terminal; 
you can also do middle button click on your mouse (both buttons simultaneously on a two-button mouse) 
or right click and select Paste from the menu. 
However, if you want to avoid the mouse and yet paste it, use "Shift + Insert", to paste the command.
 If you have to copy it from another terminal / webpage, you can use "Ctrl + Insert"to copy.
20180211             Pasting in commands
20180211             Change the text
20180211             The mouse won't work. Use the left/right arrow keys to move around the line.
20180211             When the cursor is where you want it in the line, typing inserts text - ie it doesn't overtype what's ALREADY there.
20180211             Ctrl + A or Home
20180211             Moves the cursor to the start of a line.
20180211             Ctrl+ E or End
20180211             Moves the cursor to the end of a line.
20180211             Esc + B
20180211             Moves to—THE—BEGINNING—OF the previous or current word.
20180211             Ctrl + K
20180211             Deletes from the current cursor position to the end of the line.
20180211             Ctrl + U
20180211             Deletes from the start of the line to the current cursor position.
20180211             Ctrl + W
20180211             Deletes the word before the cursor.
20180211             Alt + B
20180211             Goes back one word at a time.
20180211             Alt + F
20180211             Moves forward one word at a time.
20180211             Alt + C
20180211             Capitalizes letter where cursor is and moves to end of word.
https://askubuntu.com/questions/824880/how-to-remove-a-partition-on-a-hard-disk
https://help.ubuntu.com/community/UsingTheTerminal
https://help.ubuntu.com/community/UEFI#Identifying_if_the_computer_boots_the_Ubuntu_DVD_in_EFI_mode
20180211             Creating an UEFI partition"paragraph below).
https://help.ubuntu.com/community/UEFI#Creating_an_UEFI_partition
20180211             Disable the RAID, for me it was using the Intel rapid management thingy and telling it to disable the acceleration or THE—USE—OF—the SSD. If you have a different system, just disable the RAID —SYSTEM then install Ubuntu. Once installed you can then re-enable it.
https://ubuntuforums.org/showthread.php?t=2105418&s=69796ad2ae444e001ec71131495481f0&p=12460938#post12460938
20180211             Grub können Sie unter Ubuntu mit 1 Tool namens "Boot-Repair"reparieren. Hierfür brauchen Sie das Installationsmedium, mit dem Sie Ubuntu installiert haben.
https://praxistipps.chip.de/ubuntu-grub-reparieren-so-gehts_44077
http://www.chip.de/artikel/ISO-NRG-BIN-IMG-CUE-Image-Date1—brennen_30152845.html
https://www.youtube.com/watch?v=cgmdiuRySVc
20180211             Kernel panic no sync - fatal exception. What the key should I use for resolving it??
20180212             PCIe-Moduls
20180212             LTE/4G-PCIe-Modul
20180212             GitHub - tpm2-software/tpm2-tools: THE—SOURCE repository for the TPM ...
https://github.com/tpm2-software/tpm2-tools
20180212             Diese Seite übersetzen
20180212             tpm2-tools - THE—SOURCE repository for the TPM (Trusted Platform Module) 2 tools.
https://www.google.pt/url?sa=t&rct=j&q=&esrc=s&source=web&cd=1&cad=rja&uact=8&ved=0ahUKEwiWoqrf6KfZAhVIJcAKHYYdB90QFgguMAA&url=https%3A%2F%2Fwww.computerbase.de%2Fforum%2Fshowthread.php%3Ft%3D1551420&usg=AOvVaw2JeuM5FN_am_VBsjE6UcCP
https://www.disk-partition.com/de/ssd-management/samsung-850-evo-nicht-erkannt.html
20180215             Samsung SSD 850 EVO wird im BIOS
20180215             "Warning: Continue booting with this drive being locked might cause —SYSTEM hang with some OS".
https://www.computerbase.de/forum/showthread.php?t=1505142
20180215             Asus
20180215             AES Schlüssel der SSD verloren
20180215             Nutzt man stattdessen 1.Verschlüsselungssoftware wie Microsofts Bitlocker, liegt der Schlüssel zusätzlich als Backup im Active Directory des Unternehmens oder auf 1 USB-Stick im Tresor. Besonders praktisch ist Bitlocker, wenn man 1.SSD mit erweiterten SICHERHEITS—funktionen einsetzt: Bitlocker kümmert sich im Hintergrund um DIE—SICHERHEIT, überlässt aber DIE—ARBEIT der Verschlüsselung der SSD. Dazu muss diese die OPAL-2.0-Spezifikation der Trusted Computing Group und den Standard IEEE 1667 zur Passwortübergabe unterstützen.
https://www.heise.de/ct/ausgabe/2015-2-Test-SSDs-mit-Selbstverschluesselung-und-langer-Laufzeit-2500560.html
20180215             der ATA-Befehl Secure Erase. Durch Wahl eines neuen Geheimnisses sind in Sekundenbruchteilen sämtliche  quasi gelöscht, nämlich nach DERZEITigem Stand der Technik nicht mehr rekonstruierbar.
20180215             Per ATA Secure Erase lassen sich nicht mehr benötigte  auf SEDs schnell entsorgen, ohne das Medium schreddern zu müssen; das nutzen Firmen, um DATEN—SCHUTZDIE—RICHTLINIEn umzusetzen.
20180215             Anders als bei SOFTWARE-Verschlüsselung mit offenem und geprüftem Quellcode muss man bei 1 SED darauf vertrauen, dass die Firmware keine Bugs oder Hintertüren enthält. Einige SEDs sind nach dem US—Standard FIPS 140-2 zertifiziert.
http://www.notebookinfo.de/artikel/ausprobiert-msata-ssd-nachruesten-und-windows-8-von-der—FESTplatte-umziehen-lassen/3932/
20180215             EFI Boot-Eintrag
20180215             den Bootmodus im BIOS auf Legacy stellen.
20180215             Einige DER—NEUErungen von Windows 8 haben weitreichende Folgen. Dazu gehört die Ablösung des veralteten Basic Input/Output SYSTEM, kurz BIOS. Der Nachfolger hört auf die Abkürzung UEFI für Unified Extensible Firmware Interface und bringt theoretisch Vorteile.  
Leider gibt es aber Stolperfallen und FIRMWARE-Bugs, die 1 den Spaß an UEFI verleiden können.
20180215             Dass trotzdem so viele Windows-8-SYSTEMe im UEFI-Modus booten, hat 1 simplen Grund: Microsoft schreibt es ausdrücklich vor, wenn der Rechner ein Windows-Logo tragen soll.
https://www.heise.de/ct/ausgabe/2013—15-Loesungen-fuer-haeufige-UEFI—PANNEn-2319431.html
20180215             Microsoft verlangt dann außerdem, dass die UEFI—FUNKTION Secure Boot [1] eingeschaltet ist: Im AUSLIEFERUNGS—zustand starten folglich ausschließlich Betriebssysteme, deren Bootloader Microsoft digital signiert hat. Das soll Trojaner und Schädlinge daran hindern, sich schon vor dem Windows-Start im SYSTEM einzunisten. Secure Boot verhindert jedoch auch den Start von älteren bootfähigen DVDs oder USB-Sticks. Wer also etwa ein Live-Linux booten möchte oder 1 selbst präparierten Stick mit Windows PE, schaut nicht selten in die Röhre. Auch ältere Windows-Versionen lassen sich nicht installieren, weil den jeweiligen Setup-Medien die nötige MICROSOFT—Signatur fehlt.
20180215             Secure Boot lässt sich fast immer abschalten – bloß in welchem Menü, ist oft unklar
20180215             Der Ausschalter steckt im BIOS-Setup, pardon, im UEFI-FIRMWARE-Setup des jeweiligen SYSTEMs
20180215             Der Haken an der Sache: Man muss sich zwischen BIOS- oder UEFI-Startmodus entscheiden
20180215             Im BIOS-Modus startet ein im UEFI-Modus installiertes Windows nicht mehr. Dafür gibt es keinen technischen Grund, wie Linux beweist, sondern es ist Willkür von Microsoft: 1 im BIOS-Modus installiertes Windows verlangt unbedingt 1 Master Boot Record (MBR) auf dem träger mit der SYSTEMpartition.
20180215             Im UEFI-Modus von Windows muss die Bootpartition hingegen zwingend auf 1 Festplatte oder 1 SSD liegen, die 1.GUID-Partitionstabelle (GPT) besitzt.
20180215             Geht es bloß darum, mal eben schnell ein Live-Linux vom Stick zu starten, dann kann man aber auch zeitweise den BIOS-Modus per Setup einschalten.
20180215             Tücken bergen die Setup-DVDs der 64-Bit-Versionen von Windows 7 und Windows 8, die sowohl im BIOS- als auch im UEFI-Modus starten können
20180215             So booten manche SYSTEMe etwa nicht von USB-3.0-Anschlüssen, sondern nur an USB-2.0-Ports.
20180215             Bei Mainboards für Desktop-Rechner, die einzeln als Komponenten verkauft werden, sind wir seltener auf schwerwiegende UEFI-Bugs gestoßen – aber durchaus auf Ungereimtheiten. So erlaubt es die Firmware mancher Asrock-Mainboards, sowohl Secure Boot als auch gleichzeitig den Start im BIOS-Modus via CMS zu aktivieren. Das ist von der UEFI-Spezifikation ausdrücklich verboten, weil es den Secure-Boot-Schutz aushebelt – aber es ist 1.praktische Lösung, die DIE—ZAHL—DER—Support-Anfragen bei Asrock reduzieren dürfte …
20180215             UEFI
20180215             Hardware-Verschlüsselung für SSD
20180215             AW: Mainboard: SSD 'entsperren' oder Status 'frozen' aufheben
20180215             Auf der Samsung Service-Hotline für SSDs wurde mir heute gesagt, dass ein secure erase mit GParted wohl auch nicht möglich ist, weil GParted die SSD mit Nullen überschreibt, der 'Gelöscht'-Zustand der Samsung-SSDs aber als "mit Einsen überschrieben"definiert ist. Würde ich GParted verwenden, wäre die SSD also anschließend komplett voll geschrieben ...
http://extreme.pcgameshardware.de/mainboards-und-arbeitsspeicher/301493-mainboard-ssd-entsperren-oder-status-frozen-aufheben.html
20180215             Hardware-Verschlüsselung
20180215             Es handelt sich um 840 Pro Laufwerke. In den Dokus steht nichts.  
Lt. Testberichte muss man die HW-Verschlüsselung deaktiveren können. Nur wo und wie?
20180215             AW: Samsung - Hardwareverschlüsselung deaktivieren
20180215             Die 840 pro nutzt wie viele andere SSDs intern 1 AES encryption algorithmus, um die  zufällig über die Speicherzellen zu verteilen (wear levelling). Das kann man weder aktivieren noch deaktivieren. Es ist teil der Basisfunktionalität. Die Verschlüsselung erfolgt eben nicht seperat über das OS oder SOFTWARE sondern direkt in der SSD.
20180215             Mit 1 geeigneten BIOS, das ATA security unterstützt, kann man 1 eigenes Passwort verwenden, das man dann vor dem boot eingeben muss. Erst dann kann auf die  auf der Festplatte zugegriffen werden. Verwendet man aber keinen eigenes Passwort bzw hat kein geeignetes BIOS, sind die  zwar trotzdem verschlüsselt auf den Speicherchips abgelegt, aber es kann jeder einfach über den Controller darauf zugreifen. Dann sind die  also defakto nicht veschlüsselt (zumindest nicht in dem Sinn, dass niemand darauf zugreifen kann).
20180215             Du musst in jedem Fall nichts deaktivieren. Willst du deine  sicher speichern, brauchst du aber ein entsprechendes BIOS. Manche Notebooks können das, viele Desktop Mainboards leider nicht. Und es ist fast unmöglich herauszufinden, welches das kann.
20180215             lg
20180215             Lion
20180215             Geändert von StuffedLion (20121117             um 14:39 Uhr)
https://www.computerbase.de/forum/showthread.php?t=1136742
20180215             ein PW kann jeder im Mainboard Bios setzen. Die SSD eigene AES Verschlüsselung, was nur wenige können, ist was anderes.
20180215             SSD eigene AES Verschlüsselung
20180215             Um die sensiblen  auf SSDs zu schützen wird heute meist AES-Verschlüsselung eingesetzt. Der "Advanced Encryption Standard"wurde von dem NATIONAL—INSTITUTE—OF—Standards and Technology (NIST) zum Schutz elektronischer  ins Leben gerufen und ist weltweit verbreitet.
20180215             Bei Samsung besitzen die 840, 840 EVO und 840 PRO Laufwerke 1.AES Hardware-Verschlüsselung auf Basis von 256-Bit-Schlüsseln.
20180215             Auf den SSD 840-Laufwerken ist die AES-Verschlüsselung grundsätzlich aktiv.
20180215             Um jedoch auch den gewünschten SICHERHEITS—effekt zu erreichen, muss das ATA Passwort im SYSTEM gesetzt sein - nur dann ist die "Tür"auch abgeschlossen und die  gesichert
20180215             Um ein ATA-Passwort zu setzen, müssen Sie den passenden Menüpunkt im SYSTEM—BIOS oder der UEFI-Oberfläche aufsuchen.
20180215             Dieser heißt meist "Security". Dort setzen Sie beim Punkt "Password on boot"ein HDD-Passwort.
20180215             Administratoren haben zudem die Option, ein "Master Password"zu setzen, mit dessen Hilfe das HDD-Passwort zurückgesetzt werden kann, oder mit welchem das Laufwerk entsperrt beziehugsweise komplett gelöscht werden kann
20180215             Eine Löschung zerstört alle, macht das Laufwerk dabei aber für 1.neue Verwendung bereit. Diese Vorgänge unterscheiden sich von SYSTEM zu SYSTEM und je nach BIOS oder UEFI-Variante. DAS—SYSTEMhandbuch gibt im Zweifelsfall Aufschluss.
https://www.computerwoche.de/a/gut-geschuetzt,2555417
20180215             Für die Gewährleistung der Sicherheit ist die 850 EVO mit 1 AES-256-Bit—HARDWAREverschlüsselung ausgestattet, die keinen negativen Einfluss auf die PC-Performance hat und konform mit hochentwickelten SICHERHEITS—verwaltungslösungen wie IEEE® 1667 und TCG™ Opal. Zusätzlich schützt der Dynamic Thermal Guard vor Überhitzung.
20180215             AES-Verschlüsselung
20180215             850 EVO SATA III 2.5zoll SSD
20180215             ie AES Verschlüsslung immer aktiv ist, obwohl das ja Rechenzeit kostet und es solange kein anderes PW als der Masterkey gesetzt ist gar nichts bringt
20180215             Und wenn der TE nicht mal weiß, wo man die encryption "aktiviert"und die PW verwaltet, wird er sie auch nicht aktiviert haben.
http://www.canadatechblog.com/2011/01/27/sandforce-ssd-encryption-demystified
20180215             How is the access to the drive secured to allow only the Authorized user to access it? Is there a boot- up password that is entered via a BIOS dialog?
20180215             When the BIOS requests the Master Boot Record from the drive, the drive instead returns the pre-boot record to THE—USer. This pre-boot record is a complete, though quite restricted OS, usually something simple like MS-DOS or LINUX. The pre-boot image requests the Authentication Credentials from THE—USer, which are passed to and checked directly by the drive logic. If accepted, then the drive returns the MBR and the OS is loaded. Important point: This pre-boot authentication is the 1. thing that happens and is controlled by the drive directly. This has the added advantages of not modifying the MBR, which many software encryption products do, and allowing the MBR to be encrypted like all other user accessible data.
20180215             The encryption key is generated during manufacturing, presumably at an Asian subcontractor. Why should I trust a contractor with a key that lasts the lifetime of the SED?
20180215             The encryption key is generated on board the drive and NEVER LEAVES THE DRIVE. The manufacturer does NOT retain or even have access to the key. Moreover, you do not have to trust it. When putting an SED into service it is considered good practice to start by directing the SED to regenerate its encryption key. Doing this before loading any software on the drive eliminates the possibility of the drive manufacturer ,or anyone else who might have had a chance to access the drive before the current owner, acquiring any secret, like the encryption key, that could be later used to break into THE—USer data.
https://arstechnica.com/civis/viewtopic.php?f=11&t=1243475
20180215             The BIOS is required to handle a "SECURITY—set"drive, but not required to be able to set it.
20180215             To set an ATA password, simply access the BIOS, navigate to the “Security” menu, enable “Password on boot” and set an “HDD Password.”
20180215             Oh, and that whitepaper also mentions the evil backdoor ATA Master password:
20180215             Quote:
20180215             Administrators also have the option of setting a “Master Password,” which can allow a lost user password (“HDD Password) to be recovered.
https://arstechnica.com/civis/viewtopic.php?f=11&t=1243475
20180215             For example, if the ATA password was used to secure the drive's crypto key, then there may be a backdoor Master ATA password that will at least allow access to the drive. From this thread, I quote this response from labtech:
20180215             Quote:
20180215             Check here too (http://www.samsung.com/us/pdf/memory-st ... I_Spec.pdf)
20180215             5.2.4 Lost Password
20180215             If THE—USer password is lost and High level security is set, the drive does not allow THE—USer to access any data.
20180215             However, the drive can be unlocked using the master password.
20180215             If THE—USer password is lost and Maximum security level is set, it is impossible to access data.
20180215             However, the drive can be unlocked using the ERASE UNIT command with the master password. The drive will erase all user data and unlock the drive.
20180215             The only way to securely wipe a SSD is with the manufacturers secure erase tool.
20180215             As it has been said before, the controller might turn all of that into nothing depending on what was written. You also might miss some data due to re-allocated blocks.
20180215             I bought a Samsung 840 Pro and I still can't conclusively determine if an SSD that is FDE with a BIOS "HDD Password"is bricked if the laptop it was originally FDEed in dies.
20180215             Does anyone know if a 840 Pro can be reused in such a —SITUATION? Assume I don't care about THE—DATA.
20180215             firmware error schreibschutz aufheben festplatte
20180215             samsung ssd verschlüsselung deaktivieren
20180215             DAS—PRINZIP ist simpel:
20180215             Alle, die auf dem Sata-Anschluß zur Platte reingehen, werden
20180215             verschlüsselt im Flash abgelegt. Als "Schlüssel"dient ein Hash des
20180215             HDD-Passworts, das an den bekannten Stellen in Klartext im
20180215             Flashbereich für die Firmwareparameter abgelegt wird.
20180215             Beim Auslesen der FLashsteine Richtung Sata-Anschluß des Mainboards
20180215             werden die  wieder entschlüsselt. Also völlig transparent.
20180215             Lediglich das HDD-Passwort, das früher die Platte lediglich "Erreichbar
20180215             —AM, IDE/Sata-Bus machte", hat 1.weitere Funktion bekommen. Ohne PW
20180215             keine . Das HDD-Passwort wird der SSD beim PC-Start über das BIOS
20180215             mitgeteilt, alternativ kann es der Mount-Befehl übergeben.
20180215             Diese Art der Verschlüsselung dient dazu, die Passwortsperre der HDD
20180215             wirksam gegen jene durchzusetzen, die die Flashchips nach dem Auslöten
20180215             direkt auslesen wollen. Alternativ kann durch Überschreiben des
20180215             Passworts der gesamten Inhalt "gelöscht"werden - Vorausgesetzt die
20180215             Firmware speichert die Firmwareparameter nicht ebenso wie die anderen
20180215             im Flash ab: an anderer(!) Stelle neu schreiben.
20180215             retter haben in der Regel _keine_Probleme, die  bei
20180215             vergessenen Pw wieder herzustellen.
https://www.mikrocontroller.net/topic/313034
20180215             samsung ssd verschlüsselung deaktivieren
20180215             Automatische Verschlüsselung auf der SSD mit fatalen Folgen
20180215             Eine sehr negative Entwicklung ist Die—INZWISCHEN weit verbreitete selbstständige Verschlüsselung der ROH—DATEN auf der SSD. Diese vom Controller durchgeführte Verschlüsselung erfolgt oft ohne das Wissen und die Eingabe eines Passwortes seitens des Anwenders. Gerade diese Form der Verschlüsselung stößt nicht nur in der rettungsbranche auf blankes Unverständnis. Dabei ist nicht die Verschlüsselung an sich, sondern der Mehrwert fraglich. Ist keine Passworteingabe notwendig, dann kann jeder User, der diese SSD funktionsfähig in die Hände bekommt, die  des Besitzers einsehen. Der Schutz durch Verschlüsselung greift hier also nicht. Sollte kein Zugriff mehr möglich sein, sei es durch Beschädigung des Controllers oder auch durch Firmwarefehler, so hat man keine Möglichkeit mehr, an die  zu gelangen. In einigen Fällen können nicht einmal professionelle retter helfen. Hier arbeitet die Kryptographie an 1 Stelle, wo sie es nicht soll. Weshalb Storage—HERSTELLER verstärkt auf diese Form der Verschlüsselung zurückgreifen bleibt —BISHER, deren Geheimnis – ein Mehrwert für den Kunden ist zumindest vordergründig nicht zu erkennen.
https://www.computerwoche.de/a/die-geheimen-schwaechen-der-ssd,2501912,5
20180215             Hardware-Verschlüsselung abschalten
20180215             Zum anderen bieten zumindest einige SSD-Modelle 1.Variante, bei der Bitlocker und Hardware-Verschlüsselung zusammenwirken. Diese Variante wird auch TCG OPAL genannt: Die Spezifikation Opal wird von der Trusted Computing Group definiert, 1 Zusammenschluss diverser Hardware—HERSTELLER, und erlaubt es etwa mit Bitlocker zu arbeiten, die eigentliche Verschlüsselungs—ARBEIT aber der Hardware zu überlassen.
https://www.netzwelt.de/download/18703-samsung-magician.html
20180215             Die Samsung SSD SOFTWARE erkennt die Evo nun auch, wenn ich den Windowsboot geduldig abwarte.
20180215             Sie wird mit Status "SSD ist gesperrt"angezeigt und dem Hinweis, die Sperre im Bios freizuschalten.
https://www.computerbase.de/forum/showthread.php?t=1505142
20180215             AW: SSD Samsung 850 EVO gesperrt nach BIOS Flash AsRock Z68 Extreme3 Gen3 2.30g
20180215             Nein, die SSD muss nicht ins Repair Center. Klar sagt dir das der Samsung-Support - entweder die wissen es selbst nicht besser, haben keine Lust auf langwierige Erklärungen, oder wollen einfach daran verdienen.
20180215             Mit Parted Magic kannst du die SSD per (Enhanced) Secure Erase wieder gangbar machen; hab ich selbst schon durch und ging problemlos mit 1 Samsung-SSD, die verschlüsselt aus 1 Notebook ausgebaut und dann nicht mehr vom PC erkannt wurde.
20180215             Falls der Rechner nicht mit der SSD bootet, schließ sie einfach nach dem BIOS-POST und vor dem Starten von Parted Magic an.
20180215             Das Secure Erase-Tool erkennt die gesperrte SSD und verlangt, den Rechner kurz in den Standbymodus zu schicken und wieder aufzuwecken, wodurch das Masterpasswort umgangen wird. Nach dem folgenden Secure Erase sind alle  weg und die SSD ist wieder normal verwendbar.
http://www.chip.de/downloads/Parted-Magic_32391033.html
https://www.computerbase.de/downloads/systemtools/festplatten/parted-magic/
20180215             —NUN ist die gute SSD zum Reset unterwegs. Kosten sind —BISHER, keine genannt oder erwähnt worden.
20180215             Der Schutz wird aktiviert, indem man mit dem ATA—KOMMANDO Security Set Password ein User-Passwort setzt (das Setzen des Master-Passworts aktiviert ihn nicht).
20180215             Das Kommando Security Unlock, zusammen mit dem korrekten Passwort, entsperrt die Platte vorübergehend und man kann dann normal damit arbeiten. DIE—SICHERHEITS—funktion bleibt jedoch aktiviert: Nach dem nächsten Kaltstart ist die Platte automatisch wieder verriegelt. Erst das Kommando Security Disable, zusammen mit dem korrekten Passwort, schaltet die Sperre dauerhaft ab. Die Platte akzeptiert es nur im entsperrten Zustand.
20180215             AOMEI Partition Assistant ist ein rundum und zuverlässig Dienst—PROGRAMM für Samsung SSD. 
Zum Beispiel können Sie das Betriebs—SYSTEM auf 1.neue Samsung SSD verschieben, ohne Windows neu zu installieren, indem Sie diese SOFTWARE verwenden.
https://www.disk-partition.com/de/ssd-management/samsung-850-evo-nicht-erkannt.html
20180215             UEFI samsung ssd evo blockiert freischalten
20181124             Und PGP an mich bitte immer nur an:
20181124             $ gpg --recv-key FC32CEECA534A9C6
20181124             $ gpg --list-keys --fingerprint FC32CEECA534A9C6
20181124             pub   rsa4096 2013-10-03 [SC]
20181124             2DEC 3301 51BB 9F7D AD8B  0BDC FC32 CEEC A534 A9C6
20181124             uid           [ unknown] Input für Fefes Blog <felix-bloginput@fefe.de>
20181124             uid           [ unknown] Felix von Leitner <felix@fefe.de>
20181124             sub   rsa4096 2013-10-03 [E] 
20170414             Insgesamt kann so ein Archiv 200 bis 300 Fotos plus private Videofilme und Audiomitschnitte umfassen. Hinzu kommen etwa Dokumente wie das Abschlusszeugnis der Schule, das Hochschuldiplom, wichtige Briefe oder DIE—ERGEBNISSE genealogischer Forschungen zum Familienstammbaum.
20170414             Je älter DAS—ARCHIV, desto interessanter ist es für die Nachfahren.
20170414—20060000    —SEIT, hat PNG das ältere GIF praktisch abgelöst.  
Letzteres Format ist nur noch in Nischen relevant.
20170414—19920000    —SEIT, Für JPEG gibt es 1 Norm (ISO/IEC 10918-1) und seit dem Siegeszug des World Wide Webs besteht kein Zweifel, dass es das Foto-Austauschformat Nummer eins ist.
20170414             Was seit 25—JAHREn als Standard gilt, wird wahrscheinlich auch in 25—JAHREn noch verbreitet und lesbar sein.
20170414             TIF. Die neueste Spezifikation stammt ebenfalls aus dem Jahr 1992 und ist öffentlich zugänglich.
20170414             Für ZUKUNFTssicherheit sollte man keine Kompression verwenden, auf mehrseitige TIFs verzichten und bei 8 Bit Farbtiefe pro Kanal bleiben.
20170414             Metadaten wie Ortsnamen, Zeitstempel und Namen der abgebildeten Personen sollte man im ISO-Standard XMP einbetten
20170414             Das Kommandozeilen—PROGRAMM ExifTool setzt ein beliebiges Aufnahmedatum.
https://www.heise.de/download/product/exiftool-35845
20170414             Sicher gehen Sie mit aussagekräftigen Dateinamen nach dem Muster "1995-05—16_Abiturentlassung-Andre-Kramer.JPG".
20170414             aussagekräftigen Dateinamen
20170414             Folgender Befehl setzt mit dem ExifTool alle verfügbaren Datumsangaben 1 Datei auf den 19640601             um 12 Uhr: exiftool -alldates="1964:06:01 12:00:00"
20170414             Der QUASI—Standard für Office—DOKUMENTe sind die Formate von Microsoft Office - in 20 oder 50—JAHREn kann das aber anders aussehen.
20170414             Wer zum Beispiel seine Diplom—ARBEIT in den Achtzigerjahren mit Word für DOS geschrieben hat, kann diese —HEUTE—SCHON in neueren Versionen nicht mehr öffnen.
20170414             Bestenfalls kann man versuchen, solche Dateien in LibreOffice Writer zu importieren, das immerhin 1 Import-Filter für dieses Format mitbringt.
20170414             DAS—PROBLEM könnte in ZUKUNFT auch die seit Office 2007 veralteten Binärformate betreffen, die durch ein Dateiformat auf XML-Basis ersetzt wurden.
20170414             Dieses "Office Open XML"(OOXML) ist von der ISO als Standardformat anerkannt und speichert alle Bestandteile eines Dokuments wie Text, Grafiken und Bilder in 1 Container-Datei im ZIP-Format.
20170414             Notfalls lässt sich der Text aus dem ZIP-Archiv extrahieren und mit 1 einfachen Texteditor öffnen.
20170414             Dazu muss man die Dateien in Word im DOCX-Format und in Excel als XLSX-Datei speichern.
20170414             —SCHON vor Microsofts OOXML hat die ISO das in Open— , LibreOffice verwendete OpenDocument Format (ODF) als offenen Standard zertifiziert.
20170414             Auch ODF speichert alle Bestandteile des Dokuments innerhalb eines ZIP-Archivs.
20170414             Spezialfälle wie den Stammbaum aus der Genealogie-SOFTWARE wird zukünftig kaum jemand im herstellereigenen Format lesen können.
20170414             Solche Dokumente archiviert man am besten im Portable Document Format (PDF).
20170414             Erstens lässt sich so ziemlich alles von Office- über Layout- bis hin zu CAD-Dateien ins PDF konvertieren,
20170414             zweitens pflegt die ISO mit PDF/A 1 Standard für die Langzeitarchivierung.
20170414             PDF ist ein Container-Format, das Text, Grafik, Bilder und anderes enthalten kann.
20170414             PDF/A schränkt DIE—FREIHEITen drastisch ein.
20170414             Der Standard verbietet Videos und Skripte, zwingt zum Einbetten von Schriften und erlaubt nur zukunftssichere, nicht patentbehaftete Bildkompressionsverfahren.
20170414             Die 1. Teile des Standards PDF/A-1 und PDF/A-2 sind sehr restriktiv und frieren das Dokument in seinem Ist-Zustand ein, WÄHREND
20170414             PDF/A-3 auch Anhänge erlaubt.
20170414             Die Archivtauglichkeit dieser Anhänge wiederum wird vom Standard nicht geregelt.
20170414             Für die Langzeitarchivierung wählen Sie also bevorzugt PDF/A-1 oder A-2.
20170414             Microsoft Office, OpenOffice und PDF Creator exportieren Inhalte als PDF/A.
20170414             OpenOffice und Microsoft Office erzeugen die ursprüngliche Variante PDF/A-1a (a steht für "accessible").
20170414             In OpenOffice rufen Sie dazu "Datei/Als PDF exportieren"auf
20170414             Wer prüfen möchte, ob ein PDF den Anforderungen genügt, kann den Open-Source-PDF/A-Validierer veraPDF nutzen.
http://www.verapdf.org/
20170414             auf Java-Basis für Linux, Windows und macOS veröffentlicht.
20170414             An Tonbändern und Musikkassetten nagt der Zahn der Zeit.
20170414             Um private Aufnahmen zu retten, kann man 1 Kassettenrecorder mit USB-Anschluss anschaffen
20170414             Bessere Qualität liefert ein altes Tape-Deck eines Markenherstellers, das man mit den Ausgängen an ein billiges Audio-Interface anschließt (zum Beispiel Behringer UMC202HD für 66—EURO).
20170414             Zur Archivierung sollte man ein Format wählen, das die Aufnahmen verlustfrei speichert, weit verbreitet und wenn möglich Open Source ist - Finger weg von exotischen oder DRM-geschützten Formaten. Dateien im Wav-Format lassen sich unabhängig vom Betriebs—SYSTEM überall abspielen
20170414             Für digitalisierte Analogaufnahmen genügt 1.Wortbreite von 16 Bit bei 1 Abtastrate von 44,1 kHz, da Schallplatten und Musikkassetten 1 geringen Dynamikumfang haben. 24 Bit Wortbreite und 96 kHz Abtastrate sind nur für professionelle Aufnahmen nötig.
20170414             16 Bit bei 1 Abtastrate von 44,1 kHz,
20170414             Das Wav-Format benötigt vergleichsweise viel Speicherplatz und speichert keine Meta-Tags, die Aufschluss über den Titel, Künstler und Komponisten geben.
20170414             Dateien im Format FLAC hingegen sind nur etwa halb so groß.
20170414             Es speichert ebenfalls verlustfrei, lässt sich mit Meta-Tags beschriften und ist Open Source.
20170414             Allerdings werden FLAC-Dateien nicht von jedem Abspielgerät ohne Weiteres wiedergegeben.
20170414             Um die Wiedergabe zu vereinfachen, bietet sich 1.zusätzliche Kopie als MP3 an.
20170414             MP3 kann von nahezu jedem Gerät wiedergegeben werden und benötigt wenig Platz
20170414             Für professionelle Aufnahmen ist es allerdings ungeeignet, da speziell die Höhen unter der verlustbehafteten Kompression leiden.
20170414             Um DIE—EINBUßEN zu verringern, sollte man 1.Bitrate von 256 kBit/s nicht unterschreiten.
20170414             Das Open-Source—PROGRAMM Audacity exportiert WAV-Dateien.
20170414             Mit dem freien MP3-Codec Lame lassen sich auch MP3-Dateien ausgeben.
20170414             FLAC-Tools finden sich auf Xiph.org
20170414             Der auf Video dokumentierte Bühnenauftritt und der selbst gedrehte Urlaubsfilm sind oft auf VHS-Kassetten, SUPER—8-Filmen oder digital erhalten
20170414             im 1. Anlauf sollte man differenzieren zwischen analogen Video-Kassetten und Bewegtbildern auf DVD, Blu-ray-Disc, als Datei oder auf DV-Kassette.
20170414             Analoge Aufnahmen sollten Sie zunächst digitalisieren - entweder selbst oder durch Auftrag an 1 Dienstleister, der in der Regel 1.Video-DVD zurückliefert.
20170414             Hier reicht die Auflösung von 720 x 576 Pixeln und als Format ein MPEG-2-strom.
20170414             Das Resultat entspricht der "Standard Definition"(SD) genannten Auflösung, in der auch MPEG-2-kodierte Filme auf DVD gespeichert sind.
20170414             Auf Grund der weiten Verbreitung von Video-DVDs lassen sich solche Filme auch in ZUKUNFT noch wiedergeben.
20170414             Um aus 1 DVD nur 1 Teil herauszuschneiden, empfiehlt sich 1.preisgünstige, aber kommerzielle SOFTWARE: Das erspart Schwierigkeiten mit Codecs, da viele Verfahren patentrechtlich geschützt sind.
20170414             In Frage kommen etwa Video deluxe von Magix, PowerDirector von CyberLink oDER—PREMIERe Elements von Adobe.
20170414             Mit diesen Programmen lässt sich das gewünschte Material importieren, schneiden und als MPEG-2-Datei exportieren.
20170414             Aufnahmen von 1 ACTION-Cam in 1280 x 720 (HD, 720p) oder 1920 x 1080 Pixel (1080p, Full HD) liegen in der Regel im Videoformat MPEG-4 H.264 AVC vor, auch AVC-HD genannt.
20170414             In diesem sind die meisten Filme auf Blu-ray kodiert. Dieses Format werden handelsübliche Blu-ray-Player sicher noch länger als MPEG-2 wiedergeben können.
20170414             Das letzte Backup